// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "qca956x.dtsi"

/ {
	model = "NEC Aterm WG800HP";
	compatible = "nec,wg800hp", "qca,qca9563";

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;
		led-upgrade = &power_green;
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&jtag_disable_pins>;

		wlan2g_red {
			label = "wg800hp:red:wlan2g";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};

		active_red {
			label = "wg800hp:red:active";
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
		};

		active_green {
			label = "wg800hp:green:active";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};

		power_red: power_red {
			label = "wg800hp:red:power";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		power_green: power_green {
			label = "wg800hp:green:power";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wlan5g_red {
			label = "wg800hp:red:wlan5g";
			gpios = <&gpio 16 GPIO_ACTIVE_HIGH>;
		};

		wlan5g_green {
			label = "wg800hp:green:wlan5g";
			gpios = <&gpio 17 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy0tpt";
		};

		wlan2g_green {
			label = "wg800hp:green:wlan2g";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	keys {
		compatible = "gpio-keys";

		br {
			label = "br";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
		};
	};
};

&spi {
	status = "okay";
	num-cs = <1>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x050000 0x6f0000>;
			};

			partition@740000 {
				label = "user_data";
				reg = <0x740000 0x0a0000>;
				read-only;
			};

			partition@7e0000 {
				label = "board_data";
				reg = <0x7e0000 0x010000>;
				read-only;
			};

			art: partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x010000>;
				read-only;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;

		qca,ar8327-initvals = <
			0x04 0x00000080 /* PORT0 PAD MODE CTRL */
			0x50 0xcc35cc35 /* LED_CTRL0 */
			0x54 0xca35ca35 /* LED_CTRL1 */
			0x58 0xc935c935 /* LED_CTRL2 */
			0x5c 0x03ffff00 /* LED_CTRL3 */
			0x7c 0x0000007e /* PORT0_STATUS */
		>;
	};
};

&eth0 {
	status = "okay";

	phy-mode = "sgmii";
	phy-handle = <&phy0>;
};

&pcie {
	status = "okay";
};

&uart {
	status = "okay";
};

&wmac {
	status = "okay";
	qca,no-eeprom;
};
