// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "ar7100.dtsi"

/ {
	compatible = "aruba,ap-105", "qca,ar7161";
	model = "Aruba AP-105";

	chosen {
		bootargs = "console=ttyS0,9600";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;
		led-upgrade = &power_green;
	};

	extosc: ref {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-output-names = "ref";
		clock-frequency = <40000000>;
	};

	leds {
		compatible = "gpio-leds";

		power_green: power_green {
			label = "ap-105:green:power";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		power_red: power_red {
			label = "ap-105:red:power";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			panic-indicator;
		};

		wifi_2g_red: wifi_2g_red {
			label = "ap-105:red:wlan2g";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};

		wifi_5g_red: wifi_5g_red {
			label = "ap-105:red:wlan5g";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};
	};

	ath9k-leds {
		compatible = "gpio-leds";

		wifi_2g_green {
			label = "ap-105:green:wlan2g";
			gpios = <&ath9k0 5 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wifi_5g_green {
			label = "ap-105:green:wlan5g";
			gpios = <&ath9k1 5 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};
	};

	i2c {
		compatible = "i2c-gpio";

		sda-gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		scl-gpios = <&gpio 4 GPIO_ACTIVE_LOW>;

		/* can be removed on 4.19 */
		gpios = <&gpio 5 GPIO_ACTIVE_LOW>,
			<&gpio 4 GPIO_ACTIVE_LOW>;

		#address-cells = <1>;
		#size-cells = <0>;

		tpm@29 {
			compatible = "atmel,at97sc3203s";
			reg = <0x29>;

			/* triggering it, will also kill system */
			reset-gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
		};
	};
};

&pcie0 {
	status = "okay";

	ath9k0: wifi@0,11 { /* 2.4 GHz */
		compatible = "pci168c,0029";
		mtd-mac-address = <&hwinfo 0x1c>;
		mtd-mac-address-increment = <1>;
		reg = <0x8800 0 0 0 0>;
		#gpio-cells = <2>;
		gpio-controller;
	};

	ath9k1: wifi@0,12 { /* 5 GHz */
		compatible = "pci168c,0029";
		mtd-mac-address = <&hwinfo 0x1c>;
		mtd-mac-address-increment = <2>;
		reg = <0x9000 0 0 0 0>;
		#gpio-cells = <2>;
		gpio-controller;
	};
};

&uart {
	status = "okay";
};

&mdio0 {
	status = "okay";

	phy-mask = <0x1>;

	phy0: ethernet-phy@0 {
		reg = <0>;
	};
};

&eth0 {
	status = "okay";
	mtd-mac-address = <&hwinfo 0x1c>;

	pll-data = <0x00110000 0x00001099 0x00991099>;

	phy-mode = "rgmii";
	phy-handle = <&phy0>;
};

&spi {
	status = "okay";
	num-cs = <1>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x40000>;
				read-only;
			};

			partition@40000 {
				label = "firmware";
				reg = <0x40000 0xfa0000>;
				compatible = "denx,uimage";
			};

			hwinfo: partition@fe0000 {
				label = "hwinfo";
				reg = <0xfe0000 0x10000>;
				read-only;
			};

			partition@ff0000 {
				label = "u-boot-env";
				reg = <0xff0000 0x10000>;
				read-only;
			};
		};
	};
};
