// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "qca953x.dtsi"

/ {
	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
	};

	gpio_leds: leds {
		compatible = "gpio-leds";

		led_system: system {
			label = "tp-link:blue:system";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		switch_b0 {
			label = "switch_b0";
			linux,input-type = <EV_SW>;
			linux,code = <BTN_0>;
			gpios = <&gpio 1 GPIO_ACTIVE_HIGH>;
			debounce-interval = <60>;
		};

		switch_b1 {
			label = "switch_b1";
			linux,input-type = <EV_SW>;
			linux,code = <BTN_1>;
			gpios = <&gpio 0 GPIO_ACTIVE_HIGH>;
			debounce-interval = <60>;
		};
	};
};

&uart {
	status = "okay";
};

&spi {
	status = "okay";
	num-cs = <1>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot:	partition@0 {
				label = "u-boot";
				reg = <0x000000 0x020000>;
				read-only;
			};

			partition@20000 {
				compatible = "tplink,firmware";
				label = "firmware";
				reg = <0x020000 0x7d0000>;
			};

			art: partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x010000>;
				read-only;
			};
		};
	};
};

&eth1 {
	mtd-mac-address = <&uboot 0x1fc00>;
};

&eth0 {
	status = "okay";
	phy-handle = <&swphy4>;

	mtd-mac-address = <&uboot 0x1fc00>;
	mtd-mac-address-increment = <1>;
};

&wmac {
	status = "okay";
	mtd-cal-data = <&art 0x1000>;
	mtd-mac-address = <&uboot 0x1fc00>;
};
