#!/bin/sh

. /lib/functions/system.sh
. /lib/functions/uci-defaults.sh
. /lib/functions/k2t.sh

ath79_setup_interfaces()
{
	local board="$1"

	case "$board" in
	aruba,ap-105|\
	avm,fritz300e|\
	devolo,dvl1200i|\
	devolo,dvl1750c|\
	devolo,dvl1750i|\
	devolo,dvl1750x|\
	engenius,ecb1750|\
	glinet,gl-ar300m-lite|\
	netgear,ex6400|\
	netgear,ex7300|\
	ocedo,koala|\
	ocedo,raccoon|\
	pcs,cap324|\
	pisen,wmm003n|\
	pqi,air-pen|\
	tplink,cpe210-v2|\
	tplink,cpe210-v3|\
	tplink,re350k-v1|\
	tplink,re450-v2|\
	tplink,tl-mr10u|\
	tplink,tl-mr3020-v1|\
	tplink,tl-mr3040-v2|\
	tplink,tl-wa901nd-v2|\
	tplink,tl-wr703n|\
	ubnt,bullet-m|\
	ubnt,bullet-m-xw|\
	ubnt,lap-120|\
	ubnt,nanobeam-ac|\
	ubnt,nanostation-ac-loco|\
	ubnt,rocket-m|\
	ubnt,unifiac-lite|\
	ubnt,unifiac-lr|\
	ubnt,unifiac-mesh|\
	ubnt,unifi|\
	wd,mynet-wifi-rangeextender|\
	winchannel,wb2000)
		ucidef_set_interface_lan "eth0"
		;;
	avm,fritz4020|\
	pcs,cr3000|\
	tplink,archer-c58-v1|\
	tplink,archer-c59-v1)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:1" "2:lan:4" "3:lan:3" "4:lan:2"
		;;
	buffalo,bhr-4grv|\
	buffalo,wzr-hp-g450h)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan" "3:lan" "4:lan" "5:lan" "1:wan"
		;;
	buffalo,bhr-4grv2)
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan" "2:lan" "3:lan" "4:lan" "5:wan" "6@eth0"
		;;
	buffalo,whr-g301n)
		ucidef_set_interface_wan "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1"
		;;
	buffalo,wzr-hp-ag300h|\
	tplink,archer-c25-v1|\
	tplink,tl-mr3220-v1|\
	tplink,tl-mr3420-v1|\
	tplink,tl-wr841-v7|\
	tplink,tl-wr841-v9|\
	tplink,tl-wr841-v10|\
	tplink,tl-wr841-v11|\
	tplink,tl-wr841-v12|\
	tplink,tl-wr842n-v1|\
	tplink,tl-wr842n-v3|\
	ubnt,airrouter)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1"
		;;
	buffalo,wzr-hp-g302h-a1a0)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:1" "3:lan:4" "4:lan:3" "5:lan:2" "2:wan"
		;;
	comfast,cf-e110n-v2|\
	comfast,cf-e120a-v3|\
	tplink,cpe220-v3|\
	ubnt,nanostation-m|\
	ubnt,routerstation)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		;;
	devolo,dvl1200e|\
	devolo,dvl1750e|\
	ocedo,ursus)
		ucidef_set_interface_lan "eth0 eth1"
		;;
	dlink,dir-825-b1)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0:lan" "1:lan" "2:lan" "3:lan" "5@eth0"
		;;
	dlink,dir-825-c1|\
	dlink,dir-835-a1|\
	dlink,dir-859-a1|\
	engenius,epg5000|\
	tplink,archer-c2-v3|\
	tplink,tl-wr1043nd-v4|\
	tplink,tl-wr1043n-v5)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1" "5:wan"
		;;
	elecom,wrc-1750ghbk2-i|\
	elecom,wrc-300ghbk2-i)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:4" "3:lan:3" "4:lan:2" "5:lan:1" "1:wan"
		;;
	embeddedwireless,dorin)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:wan" "2:lan:3" "3:lan:2"
		;;
	engenius,ews511ap)
		ucidef_set_interface_lan "eth0 eth1" "dhcp"
		;;
	etactica,eg200)
		ucidef_set_interface_lan "eth0" "dhcp"
		;;
	glinet,gl-ar750s)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:2" "3:lan:1" "1:wan"
		;;
	iodata,etg3-r|\
	iodata,wn-ac1167dgr|\
	iodata,wn-ac1600dgr|\
	iodata,wn-ac1600dgr2|\
	iodata,wn-ag300dgr|\
	pcs,cr5000|\
	wd,mynet-n750)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "2:lan" "3:lan" "4:lan" "5:wan"
	;;
	librerouter,librerouter-v1)
		ucidef_add_switch "switch0" \
			"0@eth0" "5:wan" "6@eth1" "4:lan"
	;;
	nec,wg1200cr|\
	ubnt,nanostation-ac|\
	ubnt,unifiac-mesh-pro|\
	ubnt,unifiac-pro|\
	yuncore,a782|\
	yuncore,xd4200)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan" "3:wan"
		;;
	nec,wg800hp)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan" "3:lan" "4:lan" "1:wan"
		;;
	netgear,wndr3700|\
	netgear,wndr3700v2|\
	netgear,wndr3800)
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		ucidef_add_switch "switch0" \
			"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "5u@eth0"
		ucidef_add_switch_attr "switch0" "blinkrate" 2
		ucidef_add_switch_port_attr "switch0" 1 led 6
		ucidef_add_switch_port_attr "switch0" 2 led 9
		ucidef_add_switch_port_attr "switch0" 5 led 2
		;;
	netgear,wnr612-v2|\
	on,n150r|\
	tplink,tl-wr740n-v1|\
	tplink,tl-wr740n-v3|\
	tplink,tl-wr741-v1|\
	tplink,tl-wr743nd-v1|\
	tplink,tl-wr841-v5|\
	tplink,tl-wr941-v4)
		ucidef_set_interface_wan "eth0"
		ucidef_add_switch "switch0" \
		"0@eth1" "1:lan" "2:lan" "3:lan" "4:lan"
		;;
	phicomm,k2t)
		ucidef_add_switch "switch0" \
			"0@eth0" "3:lan:1" "5:lan:2" "4:wan"
		;;
	rosinson,wr818)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "2:lan" "3:wan"
		;;
	tplink,archer-a7-v5|\
	tplink,archer-c6-v2|\
	tplink,archer-c7-v4|\
	tplink,archer-c7-v5|\
	tplink,tl-wdr3600-v1|\
	tplink,tl-wdr4300-v1|\
	tplink,tl-wdr4300-v1-il|\
	tplink,tl-wr941n-v7-cn)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:1" "3:lan:2" "4:lan:3" "5:lan:4" "1:wan"
		;;
	tplink,archer-c5-v1|\
	tplink,archer-c7-v1|\
	tplink,archer-c7-v2|\
	tplink,tl-wdr4900-v2)
		ucidef_add_switch "switch0" \
			"0@eth1" "2:lan" "3:lan" "4:lan" "5:lan" "6@eth0" "1:wan"
		;;
	tplink,archer-c60-v1|\
	tplink,archer-c60-v2)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "2:lan" "3:lan" "4:lan"
		;;
	tplink,archer-d50-v1)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:3" "3:lan:2" "4:lan:1" "1:wan"
		;;
	tplink,tl-wr1043nd-v1)
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "3:lan" "4:lan" "0:wan" "5@eth0"
		;;
	tplink,tl-wr1043nd-v2|\
	tplink,tl-wr1043nd-v3)
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1" "5:wan" "6@eth0"
		;;
	tplink,tl-wr2543-v1)
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "3:lan" "4:lan" "0:wan" "9@eth0"
		;;
	tplink,tl-wr740n-v4|\
	tplink,tl-wr741nd-v4|\
	tplink,tl-wr841-v8|\
	tplink,tl-wr842n-v2)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:4" "2:lan:1" "3:lan:2" "4:lan:3"
		;;
	tplink,tl-wr941-v2)
		ucidef_set_interfaces_lan_wan "lan1 lan2 lan3 lan4" "wan"
		;;
	ubnt,acb-isp)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:1" "3:lan:3" "4:lan:2"
		;;
	ubnt,routerstation-pro)
		ucidef_set_interface_wan "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "2:lan:3" "3:lan:2" "4:lan:1"
		;;
	ubnt,nanostation-m-xw)
		ucidef_add_switch "switch0" \
			"0@eth0" "5:lan" "1:wan"
		;;
	zbtlink,zbt-wd323|\
	xiaomi,mi-router-4q)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "3:lan:1" "4:lan:2"
		;;
	*)
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		;;
	esac
}

ath79_setup_macs()
{
	local board="$1"

	case "$board" in
	avm,fritz300e)
		lan_mac=$(fritz_tffs -n maca -i $(find_mtd_part "tffs (1)"))
		;;
	avm,fritz4020)
		lan_mac=$(fritz_tffs -n maca -i $(find_mtd_part "tffs (1)"))
		wan_mac=$(fritz_tffs -n macb -i $(find_mtd_part "tffs (1)"))
		;;
	dlink,dir-825-b1)
		lan_mac=$(mtd_get_mac_text "caldata" 65440)
		wan_mac=$(mtd_get_mac_text "caldata" 65460)
		;;
	dlink,dir-825-c1|\
	dlink,dir-835-a1)
		lan_mac=$(mtd_get_mac_text "mac" 4)
		wan_mac=$(mtd_get_mac_text "mac" 24)
		;;
	dlink,dir-859-a1|\
	nec,wg1200cr|\
	wd,mynet-n750)
		lan_mac=$(mtd_get_mac_ascii devdata "lanmac")
		wan_mac=$(mtd_get_mac_ascii devdata "wanmac")
		;;
	elecom,wrc-1750ghbk2-i|\
	elecom,wrc-300ghbk2-i)
		wan_mac=$(macaddr_add "$(mtd_get_mac_binary art 4098)" -2)
		;;
	engenius,ecb1750)
		lan_mac=$(mtd_get_mac_ascii u-boot-env ethaddr)
		;;
	engenius,epg5000|\
	iodata,wn-ac1167dgr|\
	iodata,wn-ac1600dgr|\
	iodata,wn-ac1600dgr2|\
	iodata,wn-ag300dgr)
		lan_mac=$(mtd_get_mac_ascii u-boot-env ethaddr)
		wan_mac=$(mtd_get_mac_ascii u-boot-env wanaddr)
		;;
	engenius,ews511ap)
		lan_mac=$(mtd_get_mac_text "u-boot-env" 233)
		eth1_mac=$(macaddr_add "$lan_mac" 1)
		ucidef_set_interface "eth0" ifname "eth0" protocol "none" macaddr "$lan_mac"
		ucidef_set_interface "eth1" ifname "eth1" protocol "none" macaddr "$eth1_mac"
		;;
	iodata,etg3-r)
		lan_mac=$(mtd_get_mac_ascii u-boot-env ethaddr)
		wan_mac=$(macaddr_add "$lan_mac" -1)
		;;
	jjplus,ja76pf2)
		wan_mac=$(fconfig -s -r -d $(find_mtd_part "RedBoot config") -n alias/ethaddr)
		lan_mac=$(macaddr_add "$wan_mac" 1)
		;;
	nec,wg800hp)
		lan_mac=$(mtd_get_mac_text board_data 640)
		wan_mac=$(mtd_get_mac_text board_data 1152)
		;;
	netgear,wndr3700|\
	netgear,wndr3700v2|\
	netgear,wndr3800)
		lan_mac=$(macaddr_setbit_la "$(mtd_get_mac_binary art 0)")
		;;
	phicomm,k2t)
		lan_mac=$(k2t_get_mac "lan_mac")
		wan_mac=$(k2t_get_mac "wan_mac")
		;;
	rosinson,wr818)
		wan_mac=$(mtd_get_mac_binary factory 0)
		lan_mac=$(macaddr_setbit_la "$wan_mac")
		;;
	tplink,archer-a7-v5|\
	tplink,archer-c7-v4|\
	tplink,archer-c7-v5|\
	tplink,tl-wr1043nd-v4|\
	tplink,tl-wr1043n-v5)
		base_mac=$(mtd_get_mac_binary info 8)
		wan_mac=$(macaddr_add "$base_mac" 1)
		;;
	tplink,tl-wdr3600-v1|\
	tplink,tl-wdr4300-v1|\
	tplink,tl-wdr4300-v1-il)
		base_mac=$(mtd_get_mac_binary u-boot 0x1fc00)
		wan_mac=$(macaddr_add "$base_mac" 1)
		;;
	tplink,tl-wr941-v2|\
	tplink,tl-wr941n-v7-cn)
		base_mac=$(mtd_get_mac_binary u-boot 130048)
		wan_mac=$(macaddr_add "$base_mac" 1)
		;;
	ubnt,routerstation|\
	ubnt,routerstation-pro)
		wan_mac=$(fconfig -s -r -d $(find_mtd_part "RedBoot config") -n ar7100_esa)
		lan_mac=$(macaddr_add "$wan_mac" 1)
		;;
	wd,mynet-wifi-rangeextender)
		lan_mac=$(nvram get et0macaddr)
		;;
	esac

	[ -n "$lan_mac" ] && ucidef_set_interface_macaddr "lan" $lan_mac
	[ -n "$wan_mac" ] && ucidef_set_interface_macaddr "wan" $wan_mac
}

board_config_update
board=$(board_name)
ath79_setup_interfaces $board
ath79_setup_macs $board
board_config_flush

exit 0
