#!/bin/sh
#
# Copyright (C) 2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
cpe210|\
cpe510|\
wbs210|\
wbs510)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "20"
	;;
nanostation-m)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "8"
	;;
nanostation-m-xw)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "2"
	;;
rb-912uag-2hpnd|\
rb-912uag-5hpnd)
	ucidef_add_gpio_switch "usb_power_switch" "USB Power Switch" "61" "1"
	;;
rb-750up-r2|\
rb-951ui-2nd|\
rb-952ui-5ac2nd)
	ucidef_add_gpio_switch "usb_power_switch" "USB Power Switch" "45" "1"
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "14"
	;;
rb-750p-pbr2)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "14"
	;;
esac

board_config_flush

exit 0
