// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "qca9557.dtsi"

/ {
	compatible = "engenius,ecb1750", "qca,qca9557";
	model = "EnGenius ECB1750";

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	aliases {
		led-boot = &power_orange;
		led-failsafe = &power_orange;
		led-running = &power_orange;
		led-upgrade = &power_orange;
	};

	leds {
		compatible = "gpio-leds";

		power_orange: power_orange {
			label = "ecb1750:orange:power";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wlan2g {
			label = "ecb1750:blue:wlan2g";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		wlan5g {
			label = "ecb1750:blue:wlan5g";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		lan {
			label = "ecb1750:blue:lan";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};
	};
};

&pcie0 {
	status = "okay";
};

&uart {
	status = "okay";
};

&spi {
	status = "okay";
	num-cs = <1>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x050000 0xf50000>;
			};

			partition@fa0000 {
				label = "userconfig";
				reg = <0xfa0000 0x050000>;
				read-only;
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;
			};

		};
	};
};

&wmac {
	status = "okay";

	qca,no-eeprom;
};

&mdio0 {
	status = "okay";

	phy5: ethernet-phy@5 {
		reg = <5>;
		at803x-disable-smarteee;
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x9a000000 0x80000101 0x80001313>;

	phy-handle = <&phy5>;
	phy-mode = "rgmii";

	gmac-config {
		device = <&gmac>;
		rgmii-gmac0 = <1>;
		rxd-delay = <3>;
		rxdv-delay = <3>;
	};
};
