/dts-v1/;

#include "rt3050.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "netgear,wnce2001", "ralink,rt3052-soc";
	model = "Netgear WNCE2001";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_green;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	leds {
		compatible = "gpio-leds";

		led_power_green: power-green {
			label = "wnce2001:green:power";
			gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
		};

		power-red {
			label = "wnce2001:red:power";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
		};

		wlan-green {
			label = "wnce2001:green:wlan";
			gpios = <&gpio0 12 GPIO_ACTIVE_HIGH>;
		};

		wlan-red {
			label = "wnce2001:red:wlan";
			gpios = <&gpio0 13 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		rt {
			label = "rt";
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
		};

		ap {
			label = "ap";
			gpios = <&gpio0 7 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_1>;
		};
	};
};

&spi0 {
	status = "okay";

	m25p80@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			factory: partition@30000 {
				label = "factory";
				reg = <0x30000 0x10000>;
				read-only;
			};

			partition@40000 {
				label = "config";
				reg = <0x40000 0x20000>;
				read-only;
			};

			partition@60000 {
				label = "language";
				reg = <0x60000 0x30000>;
				read-only;
			};

			partition@90000 {
				label = "pot";
				reg = <0x90000 0x10000>;
				read-only;
			};

			partition@a0000 {
				label = "checksum";
				reg = <0xa0000 0x10000>;
			};

			partition@b0000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0xb0000 0x350000>;
			};
		};
	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "i2c", "jtag", "rgmii", "mdio", "uartf";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x28>;
};

&wmac {
	ralink,mtd-eeprom = <&factory 0>;
};
