/dts-v1/;

#include "mt7628an.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "hiwifi,hc5861b", "mediatek,mt7628an-soc";
	model = "HiWiFi HC5861B";

	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x8000000>;
	};

	leds {
		compatible = "gpio-leds";

		led_system: system {
			label = "hc5861b:green:system";
			gpios = <&gpio1 5 GPIO_ACTIVE_LOW>;
		};
		wlan2g {
			label = "hc5861b:green:wlan2g";
			gpios = <&gpio1 12 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio1 6 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "refclk", "wdt", "wled_an";
			ralink,function = "gpio";
		};
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "hw_panic";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0xf70000>;
			};

			partition@fc0000 {
				label = "oem";
				reg = <0xfc0000 0x20000>;
				read-only;
			};

			bdinfo: partition@fe0000 {
				label = "bdinfo";
				reg = <0xfe0000 0x10000>;
				read-only;
			};

			partition@ff0000 {
				label = "backup";
				reg = <0xff0000 0x10000>;
				read-only;
			};
		};
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x4>;
};

&wmac {
	status = "okay";
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x8000>;
		mtd-mac-address = <&factory 0x2e>;
		ieee80211-freq-limit = <5000000 6000000>;

		led {
			led-sources = <2>;
			led-active-low;
		};
	};
};
