# flash u-boot-with-spl.imx
# using fixed size of 1M for U-Boot + SPL
mmc dev 0 1
mmc write 0x12100000 0x2 0x800

# flash openwrt-imx6-apalis-squashfs.combined.bin
run set_blkcnt
mmc dev 0 0
mmc write 0x12500000 0 ${blkcnt}

env default -f -a
saveenv

reset
