/dts-v1/;

#include "rt3883.dtsi"

/ {
	compatible = "loewe,wmdr-143n", "ralink,rt3883-soc";
	model = "Loewe WMDR-143N";
};

&spi0 {
	status = "okay";

	m25p80@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x00010000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x7b0000>;
			};
		};
	};
};

&ethernet {
	port@0 {
		phy-handle = <&phy0>;
		phy-mode = "mii";
	};
	mdio-bus {
		status = "okay";

		phy0: ethernet-phy@0 {
			reg = <0>;
			phy-mode = "mii";
		};
	};
};

&wmac {
	status = "okay";
	ralink,mtd-eeprom = <&factory 0>;
	mtd-mac-address = <&factory 0x4>;
};
