/dts-v1/;

#include "HC5X61.dtsi"

/ {
	compatible = "hiwifi,hc5861", "hiwifi,hc5x61", "ralink,mt7620a-soc";
	model = "HiWiFi HC5861";

	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
	};

	leds {
		compatible = "gpio-leds";

		led_system: system {
			label = "hc5861:blue:system";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
		};

		wlan2g {
			label = "hc5861:blue:wlan2g";
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
		};

		internet {
			label = "hc5861:blue:internet";
			gpios = <&gpio3 0 GPIO_ACTIVE_LOW>;
		};

		wlan5g {
			label = "hc5861:blue:wlan5g";
			gpios = <&gpio0 7 GPIO_ACTIVE_LOW>;
		};

		turbo {
			label = "hc5861:blue:turbo";
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
		};
	};

	gpio_export {
		compatible = "gpio-export";
		#size-cells = <0>;

		usbpower {
			gpio-export,name = "usbpower";
			gpio-export,output = <0>;
			gpios = <&gpio0 13 GPIO_ACTIVE_LOW>;
		};

		sdpower {
			gpio-export,name = "sdpower";
			gpio-export,output = <0>;
			gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
		};
	};
};

&ehci {
	status = "okay";
};

&ohci {
	status = "okay";
};

&ethernet {
	status = "okay";
	mtd-mac-address = <&factory 0x4>;
	pinctrl-names = "default";
	pinctrl-0 = <&rgmii1_pins &mdio_pins>;
	mediatek,portmap = "wllll";

	port@5 {
		status = "okay";
		phy-handle = <&phy5>;
		phy-mode = "rgmii";
	};

	mdio-bus {
		status = "okay";

		phy5: ethernet-phy@5 {
			reg = <5>;
			phy-mode = "rgmii";
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "pci14c3,7662";
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x8000>;
		ieee80211-freq-limit = <5000000 6000000>;
	};
};
