// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "ar7100.dtsi"

/ {
	model = "jjPlus JA76PF2";
	compatible = "jjplus,ja76pf2", "qca,ar7161";

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x4000000>;
	};

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	aliases {
		led-boot = &d2;
		led-failsafe = &d2;
		led-running = &d2;
		led-upgrade = &d2;
	};

	extosc: ref {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-output-names = "ref";
		clock-frequency = <40000000>;
	};

	leds {
		compatible = "gpio-leds";

		d2: d2 {
			label = "ja76pf2:green:d2";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};

		d3 {
			label = "ja76pf2:green:d3";
			gpios = <&gpio 4 GPIO_ACTIVE_HIGH>;
		};

		d4 {
			label = "ja76pf2:green:d4";
			gpios = <&gpio 3 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		sw1 {
			label = "sw1";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		sw2 {
			label = "sw2";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};
};

&mdio0 {
	status = "okay";

	phy-mask = <0x1>;

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "rgmii";
	};

	phy4: ethernet-phy@4 {
		reg = <4>;
		phy-mode = "rgmii";
	};
};

&eth0 {
	status = "okay";

	phy-handle = <&phy0>;
};

&eth1 {
	status = "okay";

	phy-handle = <&phy4>;
};

&pcie0 {
	status = "okay";
};

&spi {
	status = "okay";
	num-cs = <1>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			#address-cells = <1>;
			#size-cells = <1>;
			compatible = "ecoscentric,redboot-fis-partitions";
		};
	};
};

&uart {
	status = "okay";
};
