Package: kmod-3c59x
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mii
Source: package/kernel/linux
SourceName: kmod-3c59x
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 19711
Filename: kmod-3c59x_4.14.167-1_mipsel_24kc.ipk
Size: 20644
SHA256sum: 4334b967d8c9c5064c7812fb154ffee50065524539a9aa4164689bc848a61bcc
Description:  This option enables driver support for a large number of 10mbps and
 10/100mbps EISA, PCI and PCMCIA 3Com Ethernet adapters:
 - "Vortex"    (Fast EtherLink 3c590/3c592/3c595/3c597) EISA and PCI
 - "Boomerang" (EtherLink XL 3c900 or 3c905)            PCI
 - "Cyclone"   (3c540/3c900/3c905/3c980/3c575/3c656)    PCI and Cardbus
 - "Tornado"   (3c905)                                  PCI
 - "Hurricane" (3c555/3cSOHO)                           PCI

Package: kmod-6lowpan
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-6lowpan
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10473
Filename: kmod-6lowpan_4.14.167-1_mipsel_24kc.ipk
Size: 11241
SHA256sum: a4f42e6c0acb81aaab750473dc1ae0013685a37f0bf2c1fd213d9323b6e60d23
Description:  Shared 6lowpan code for IEEE 802.15.4 and Bluetooth.

Package: kmod-8139cp
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mii
Source: package/kernel/linux
SourceName: kmod-8139cp
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10596
Filename: kmod-8139cp_4.14.167-1_mipsel_24kc.ipk
Size: 11363
SHA256sum: 316bde52544aee423b8dd2d41f3b9874ea1d70adea78b7948941e9d7a2feb35b
Description:  Kernel module for RealTek RTL-8139C+ PCI Fast Ethernet adapters

Package: kmod-8139too
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mii
Source: package/kernel/linux
SourceName: kmod-8139too
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10674
Filename: kmod-8139too_4.14.167-1_mipsel_24kc.ipk
Size: 11455
SHA256sum: 1005308460efbd125e395d3299ca76f157964af6c22a98085673a35b2b00de69
Description:  Kernel modules for RealTek RTL-8139 PCI Fast Ethernet adapters

Package: kmod-ac97
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core
Source: package/kernel/linux
SourceName: kmod-ac97
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 43111
Filename: kmod-ac97_4.14.167-1_mipsel_24kc.ipk
Size: 43361
SHA256sum: 16785f74a56834bcab31669dc33c8d12b4d943a94873aa888cc6f81150271ea4
Description:  The ac97 controller

Package: kmod-acx-mac80211
Version: 4.14.167+2014-02-16-b6fc3149-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211
Source: package/kernel/acx-mac80211
SourceName: kmod-acx-mac80211
Section: kernel
Maintainer: Florian Fainelli <florian@openwrt.org>
Architecture: mipsel_24kc
Installed-Size: 177502
Filename: kmod-acx-mac80211_4.14.167+2014-02-16-b6fc3149-1_mipsel_24kc.ipk
Size: 175417
SHA256sum: ce59b48a251bbf16550ea66538a636873b6246d53ed8b93b779600398d86d1e5
Description:  Driver for acx111 cards (mac80211 version)

Package: kmod-adm8211
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-eeprom-93cx6
Source: package/kernel/mac80211
SourceName: kmod-adm8211
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 13826
Filename: kmod-adm8211_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 14564
SHA256sum: 80a3acd0490545ee71698ce9c8e0ad4173d406a44ffa22e248d2f2c25c03425d
Description:  ADMTek 8211 support

Package: kmod-aoe
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-aoe
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 22315
Filename: kmod-aoe_4.14.167-1_mipsel_24kc.ipk
Size: 22942
SHA256sum: 5c2f636d903d6420e5818f7f19d1d1f320d084f64cc8fc41a181b7aa58d26ba6
Description:  Kernel support for ATA over Ethernet

Package: kmod-arptables
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-arptables
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 8577
Filename: kmod-arptables_4.14.167-1_mipsel_24kc.ipk
Size: 9348
SHA256sum: 687b282fea65526c9d368e06fdb745f9e04cf25e2fd640db21ece088932dd665
Description:  Kernel modules for ARP firewalling

Package: kmod-asn1-decoder
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-asn1-decoder
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2542
Filename: kmod-asn1-decoder_4.14.167-1_mipsel_24kc.ipk
Size: 3288
SHA256sum: cd36fdcdafdc4275a5c2e484bb729abc1dd6a1d70a8c18f655c3626bb680f2f1
Description:  Simple ASN1 decoder

Package: kmod-at86rf230
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac802154, kmod-regmap-spi
Source: package/kernel/linux
SourceName: kmod-at86rf230
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9622
Filename: kmod-at86rf230_4.14.167-1_mipsel_24kc.ipk
Size: 10342
SHA256sum: c13bfa66173653777a8b3bb17391e468528f40ae67c671bf379522baa93db5b2
Description:  AT86RF230 transceiver driver

Package: kmod-ata-ahci
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ata-core
Source: package/kernel/linux
SourceName: kmod-ata-ahci
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6119
Filename: kmod-ata-ahci_4.14.167-1_mipsel_24kc.ipk
Size: 6826
SHA256sum: 2763c10e59c42a93a42766e72d24b7ffebbf37dbccdd106f1c37021d5f11dc1c
Description:  Support for AHCI Serial ATA controllers

Package: kmod-ata-artop
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ata-core
Source: package/kernel/linux
SourceName: kmod-ata-artop
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2569
Filename: kmod-ata-artop_4.14.167-1_mipsel_24kc.ipk
Size: 3316
SHA256sum: 2783ec8dc5abb7c03456df666313f87a3f7dad4cdc910200779559c1244dd058
Description:  PATA support for ARTOP 6210/6260 host controllers

Package: kmod-ata-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-scsi-core
Source: package/kernel/linux
SourceName: kmod-ata-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 98645
Filename: kmod-ata-core_4.14.167-1_mipsel_24kc.ipk
Size: 98486
SHA256sum: a52e16e53ccac19645c2d628a6a1f641d2b5366a861f74adef6719c037fb2786
Description:  Serial and Parallel ATA support

Package: kmod-ata-marvell-sata
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ata-core
Source: package/kernel/linux
SourceName: kmod-ata-marvell-sata
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 15789
Filename: kmod-ata-marvell-sata_4.14.167-1_mipsel_24kc.ipk
Size: 16493
SHA256sum: 5b433fdb4ccf2743c3063319e5a900450c783c7f4a4cca01697359f9ad96d289
Description:  SATA support for marvell chipsets

Package: kmod-ata-nvidia-sata
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ata-core
Source: package/kernel/linux
SourceName: kmod-ata-nvidia-sata
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 11672
Filename: kmod-ata-nvidia-sata_4.14.167-1_mipsel_24kc.ipk
Size: 12416
SHA256sum: 9f7ea7f11de5f805abd19e025d5438aeaa5cabb3064d85b9f161c1661e9de91a
Description:  Nvidia Serial ATA support

Package: kmod-ata-pdc202xx-old
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ata-core
Source: package/kernel/linux
SourceName: kmod-ata-pdc202xx-old
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2657
Filename: kmod-ata-pdc202xx-old_4.14.167-1_mipsel_24kc.ipk
Size: 3435
SHA256sum: 0bec9b186dff383f317ffcce1e6671d7feab04c66caa4cd37ceb5c91d5bcf064
Description:  This option enables support for the Promise 20246, 20262, 20263,
 20265 and 20267 adapters

Package: kmod-ata-piix
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ata-core
Source: package/kernel/linux
SourceName: kmod-ata-piix
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5923
Filename: kmod-ata-piix_4.14.167-1_mipsel_24kc.ipk
Size: 6672
SHA256sum: e36007f8f700da81c7e35321fd0cb08b5ca8a04571ba7b3ee8ac4ee65cf04939
Description:  SATA support for Intel ICH5/6/7/8 series host controllers and
 PATA support for Intel ESB/ICH/PIIX3/PIIX4 series host controllers

Package: kmod-ata-sil24
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ata-core
Source: package/kernel/linux
SourceName: kmod-ata-sil24
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7212
Filename: kmod-ata-sil24_4.14.167-1_mipsel_24kc.ipk
Size: 7983
SHA256sum: 8aa032deb7e1d38fd807ab105cb549ea278e52988c9cb4fe0dd783bfead59718
Description:  Support for Silicon Image 3124/3132 Serial ATA controllers

Package: kmod-ata-sil
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ata-core
Source: package/kernel/linux
SourceName: kmod-ata-sil
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4810
Filename: kmod-ata-sil_4.14.167-1_mipsel_24kc.ipk
Size: 5553
SHA256sum: 50b1df23cf834fe6b9ab3efc1e1ceab7542bcdd5f2ef3ea540da1d560d532775
Description:  Support for Silicon Image Serial ATA controllers

Package: kmod-ata-via-sata
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ata-core
Source: package/kernel/linux
SourceName: kmod-ata-via-sata
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5047
Filename: kmod-ata-via-sata_4.14.167-1_mipsel_24kc.ipk
Size: 5805
SHA256sum: d26b8dbca4e1ce219291699fbe6068e63426c0cd22bcb4bbdcf2e788c672cb1c
Description:  This option enables support for VIA Serial ATA

Package: kmod-ath10k-ct-smallbuffers
Version: 4.14.167+2019-09-09-5e8cd86f-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-ath, kmod-hwmon-core
Provides: kmod-ath10k
Source: package/kernel/ath10k-ct
SourceName: kmod-ath10k-ct-smallbuffers
License: GPLv2
Section: kernel
Maintainer: Ben Greear <greearb@candelatech.com>
Architecture: mipsel_24kc
Installed-Size: 210702
Filename: kmod-ath10k-ct-smallbuffers_4.14.167+2019-09-09-5e8cd86f-1_mipsel_24kc.ipk
Size: 209001
SHA256sum: 33732e6f940740fd3f27d819c1a9f624e45088af7946fcf0e95194ed1cdee640
Description:  ath10k-ct driver optimized for CT ath10k firmware (small buffers for low-RAM devices)

Package: kmod-ath10k-ct
Version: 4.14.167+2019-09-09-5e8cd86f-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-ath, kmod-hwmon-core
Provides: kmod-ath10k
Source: package/kernel/ath10k-ct
SourceName: kmod-ath10k-ct
License: GPLv2
Section: kernel
Maintainer: Ben Greear <greearb@candelatech.com>
Architecture: mipsel_24kc
Installed-Size: 210689
Filename: kmod-ath10k-ct_4.14.167+2019-09-09-5e8cd86f-1_mipsel_24kc.ipk
Size: 209084
SHA256sum: 9bd14265ab4f0017a1ca7b7cc879338f013312ffff13303fa792d455be8bee9c
Description:  ath10k-ct driver optimized for CT ath10k firmware

Package: kmod-ath10k
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ath
Source: package/kernel/mac80211
SourceName: kmod-ath10k
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 171647
Filename: kmod-ath10k_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 171044
SHA256sum: e2fbfbf98f6fedffdcc8e663d84dd2f572d199dad5d3a704ed99ee70f988e664
Description:  This module adds support for wireless adapters based on
 Atheros IEEE 802.11ac family of chipsets. For now only
 PCI is supported.

Package: kmod-ath3k
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-bluetooth, ar3k-firmware
Source: package/kernel/linux
SourceName: kmod-ath3k
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3840
Filename: kmod-ath3k_4.14.167-1_mipsel_24kc.ipk
Size: 4509
SHA256sum: 0e89a7cd36df9585daea825daa37cae8e4105da797db5f7f1c4e8d4f275007f3
Description:  Kernel support for ATH3K Module

Package: kmod-ath5k
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ath
Source: package/kernel/mac80211
SourceName: kmod-ath5k
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 82288
Filename: kmod-ath5k_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 82645
SHA256sum: 307dc57206e0002e6a794b07bca0270acadc412fadf42037d1bcdc4e26542a4f
Description:  This module adds support for wireless adapters based on
 Atheros 5xxx chipset.

Package: kmod-ath6kl-sdio
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mmc, kmod-ath6kl
Source: package/kernel/mac80211
SourceName: kmod-ath6kl-sdio
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 8231
Filename: kmod-ath6kl-sdio_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 9042
SHA256sum: d4916cd6cfb79100bdbea1983f44281f12107625d2969cc986e218295ade3e3b
Description:  This module adds support for wireless adapters based on
 Atheros IEEE 802.11n AR6003 and AR6004 family of chipsets.

Package: kmod-ath6kl-usb
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core, kmod-ath6kl
Source: package/kernel/mac80211
SourceName: kmod-ath6kl-usb
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 6013
Filename: kmod-ath6kl-usb_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 6839
SHA256sum: 28f27e718659fe4e4d65e95779c28babd4206883343c56c47a9bd92d0a6a5ea9
Description:  This module adds support for wireless adapters based on the
 Atheros IEEE 802.11n AR6004 chipset.

Package: kmod-ath6kl
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ath
Source: package/kernel/mac80211
SourceName: kmod-ath6kl
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 107332
Filename: kmod-ath6kl_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 107381
SHA256sum: beb5155cd6117dd8f619d721584045b9b95810947cf17fbdd1117268f3339698
Description:  Atheros FullMAC wireless devices (common code for ath6kl_sdio and ath6kl_usb)

Package: kmod-ath9k-common
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ath
Source: package/kernel/mac80211
SourceName: kmod-ath9k-common
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 125486
Filename: kmod-ath9k-common_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 123145
SHA256sum: d70f4dfd79ad910d8b62d388cfe02741558feb83c33904c827ad0322d7d53bbe
Description:  Atheros 802.11n wireless devices (common code for ath9k and ath9k_htc)

Package: kmod-ath9k-htc
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ath9k-common, kmod-usb-core, ath9k-htc-firmware
Source: package/kernel/mac80211
SourceName: kmod-ath9k-htc
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 35521
Filename: kmod-ath9k-htc_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 36284
SHA256sum: eae2850635769f4b13279765dbe6f29033d02de5afbbd689b9d676a756a695de
Description:  This module adds support for wireless adapters based on
 Atheros USB AR9271 and AR7010 family of chipsets.

Package: kmod-ath9k
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ath9k-common
Source: package/kernel/mac80211
SourceName: kmod-ath9k
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 60016
Filename: kmod-ath9k_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 60539
SHA256sum: adf3a5e5e15482217ee90c97d9409370ae9b96b6c5343361777008543e1fdb89
Description:  This module adds support for wireless adapters based on
 Atheros IEEE 802.11n AR5008 and AR9001 family of chipsets.

Package: kmod-ath
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211
Source: package/kernel/mac80211
SourceName: kmod-ath
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 12257
Filename: kmod-ath_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 13004
SHA256sum: b54c78bda39a6061b6b185ae77cbef3af9a630d6df3c87191f08b30c2e5263d2
Description:  This module contains some common parts needed by Atheros Wireless drivers.

Package: kmod-atl1
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mii
Source: package/kernel/linux
SourceName: kmod-atl1
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 16436
Filename: kmod-atl1_4.14.167-1_mipsel_24kc.ipk
Size: 17133
SHA256sum: 069949c2e99d53a0f51e7da8692d1fd833fd951e555e1c4123e3adbd65aae7c0
Description:  Atheros L1 Gigabit Ethernet support

Package: kmod-atl1c
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-atl1c
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 18625
Filename: kmod-atl1c_4.14.167-1_mipsel_24kc.ipk
Size: 19342
SHA256sum: 2379f60d898c3c6531b476bb4a7ca34a984e7766efa36eb60ac391bb9e76603c
Description:  Atheros L1C

Package: kmod-atl1e
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-atl1e
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 15716
Filename: kmod-atl1e_4.14.167-1_mipsel_24kc.ipk
Size: 16414
SHA256sum: 13cd959b7efa3a81b9660a677fcac691b7d3e94ce0a8bf87f957ad3193973c46
Description:  Atheros L1E

Package: kmod-atl2
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-atl2
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 12890
Filename: kmod-atl2_4.14.167-1_mipsel_24kc.ipk
Size: 13547
SHA256sum: 742157b81bcbce62fb6fbd5d320d652ff1bd3eb6d63757a580cf0b3ff5cd44c7
Description:  Atheros L2 Fast Ethernet support

Package: kmod-atm
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-atm
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 26775
Filename: kmod-atm_4.14.167-1_mipsel_24kc.ipk
Size: 27416
SHA256sum: b51c1c55dfe047fa3df7b5bbe956bfc3dc25858e33d3bb37995d0a759e8ba186
Description:  Kernel modules for ATM support

Package: kmod-atmtcp
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-atm
Source: package/kernel/linux
SourceName: kmod-atmtcp
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3909
Filename: kmod-atmtcp_4.14.167-1_mipsel_24kc.ipk
Size: 4642
SHA256sum: 65a5c5c85398e48bfda1276156d97a5270931ff2571ad11b9503232365634521
Description:  Kernel module for ATM over TCP support

Package: kmod-atusb
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core, kmod-mac802154
Source: package/kernel/linux
SourceName: kmod-atusb
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5580
Filename: kmod-atusb_4.14.167-1_mipsel_24kc.ipk
Size: 6323
SHA256sum: 3f5d5859d58b8da02aaf39b6220f111bd2006ad1e6d0d940ce2fe04fc194ec36
Description:  ATUSB transceiver driver

Package: kmod-ax25
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-crc16
Source: package/kernel/linux
SourceName: kmod-ax25
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 32039
Filename: kmod-ax25_4.14.167-1_mipsel_24kc.ipk
Size: 32758
SHA256sum: ef1ac3685329dee78e1c58f8998e37722f3a52872cf1640a1d2b3d8f08a3341a
Description:  Kernel modules for AX25 support

Package: kmod-b43
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-ssb, kmod-bcma
Source: package/kernel/mac80211
SourceName: kmod-b43
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 284328
Filename: kmod-b43_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 280142
SHA256sum: 5dda6592fdbb1e70ba46217887d65832f9ff6c0f41234fe3883339c732dc8bf9
Description:  Kernel module for Broadcom 43xx wireless support (mac80211 stack) new

Package: kmod-b43legacy
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-ssb, b43legacy-firmware
Source: package/kernel/mac80211
SourceName: kmod-b43legacy
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 52327
Filename: kmod-b43legacy_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 53150
SHA256sum: c60316278ae7532a782a6ec9c8fee0fa7432099e3183da999870b4dc5a1da463
Description:  Kernel module for Broadcom 43xx-legacy wireless support (mac80211 stack) new

Package: kmod-b44
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ssb, kmod-mii, kmod-libphy
Source: package/kernel/linux
SourceName: kmod-b44
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 14883
Filename: kmod-b44_4.14.167-1_mipsel_24kc.ipk
Size: 15598
SHA256sum: 08fe9d0aca4f5ca492159798106e7a41fc4eff4773cb164257210ad0b574ad8b
Description:  Kernel modules for Broadcom 44xx Ethernet adapters.

Package: kmod-batman-adv
Version: 4.14.167+2019.2-5
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-crc16, kmod-lib-crc32c, kmod-cfg80211, batctl
Source: feeds/routing/batman-adv
SourceName: kmod-batman-adv
License: GPL-2.0
Section: kernel
Maintainer: Simon Wunderlich <sw@simonwunderlich.de>
Architecture: mipsel_24kc
Installed-Size: 89720
Filename: kmod-batman-adv_4.14.167+2019.2-5_mipsel_24kc.ipk
Size: 90524
SHA256sum: caf4440571b42d3e68ffeac82279a050059d2d0c9ccfa512b7fbcecbd9c29cb0
Description:  B.A.T.M.A.N. (better approach to mobile ad-hoc networking) is
 a routing protocol for multi-hop ad-hoc mesh networks. The
 networks may be wired or wireless. See
 https://www.open-mesh.org/ for more information and user space
 tools. This package builds version 2019.2 of the kernel
 module.

Package: kmod-bcma
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-bcma
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 18334
Filename: kmod-bcma_4.14.167-1_mipsel_24kc.ipk
Size: 19120
SHA256sum: 59ec665638a613b4da4497f33644ed119da8510f790318e974028f4716ab2e5d
Description:  Bus driver for Broadcom specific Advanced Microcontroller Bus Architecture

Package: kmod-be2net
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core
Source: package/kernel/linux
SourceName: kmod-be2net
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 65313
Filename: kmod-be2net_4.14.167-1_mipsel_24kc.ipk
Size: 65877
SHA256sum: 6621d7b277da1b972237fdadcd2304ed84fda00549854d967197cdecd71a5ba8
Description:  Broadcom Emulex OneConnect 10Gbit SFP+ support, OneConnect OCe10xxx OCe11xxx OCe14xxx, LightPulse LPe12xxx

Package: kmod-block2mtd
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-block2mtd
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3698
Filename: kmod-block2mtd_4.14.167-1_mipsel_24kc.ipk
Size: 4409
SHA256sum: 870d28e0e10f9d78e4035bdf1bc45c12d4410b6430470216603bb5322aea7dfc
Description:  Block device MTD emulation

Package: kmod-bluetooth
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core, kmod-crypto-hash, kmod-crypto-ecb, kmod-lib-crc16, kmod-hid, kmod-crypto-cmac, kmod-regmap-core, kmod-crypto-ecdh
Source: package/kernel/linux
SourceName: kmod-bluetooth
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 217537
Filename: kmod-bluetooth_4.14.167-1_mipsel_24kc.ipk
Size: 217866
SHA256sum: 1e05918a6a9601a14b06f7e5cf8ecfaa4f4026945e2ec86af46d95fd4c8e1fd2
Description:  Kernel support for Bluetooth devices

Package: kmod-bluetooth_6lowpan
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-6lowpan, kmod-bluetooth
Source: package/kernel/linux
SourceName: kmod-bluetooth_6lowpan
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6600
Filename: kmod-bluetooth_6lowpan_4.14.167-1_mipsel_24kc.ipk
Size: 7414
SHA256sum: 53b5f3c3de673a16fc499d2d29f639701fe2a804b0e85a5fa822140e7557d267
Description:  Kernel support for 6LoWPAN over Bluetooth Low Energy devices

Package: kmod-bmp085-i2c
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-bmp085
Source: package/kernel/linux
SourceName: kmod-bmp085-i2c
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-bmp085-i2c_4.14.167-1_mipsel_24kc.ipk
Size: 870
SHA256sum: a0730ab87ecfccf412d228d858873dd62db69269bb4411397c2df2360e184c70
Description:  This driver adds support for Bosch Sensortec's digital pressure
 sensor connected via I2C.

Package: kmod-bmp085-spi
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-bmp085
Source: package/kernel/linux
SourceName: kmod-bmp085-spi
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-bmp085-spi_4.14.167-1_mipsel_24kc.ipk
Size: 872
SHA256sum: 14e0d574066a7c22d8150daaff5980ede74bb1e2760a7cb728a40885265dc164
Description:  This driver adds support for Bosch Sensortec's digital pressure
 sensor connected via SPI.

Package: kmod-bmp085
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-regmap-core
Source: package/kernel/linux
SourceName: kmod-bmp085
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-bmp085_4.14.167-1_mipsel_24kc.ipk
Size: 879
SHA256sum: 0b8d0acb736b4581f1510ae32c31e558183e2ffe4c103466994a7ec75550144d
Description:  This driver adds support for Bosch Sensortec's digital pressure
 sensors BMP085 and BMP18x.

Package: kmod-bnx2
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), bnx2-firmware
Source: package/kernel/linux
SourceName: kmod-bnx2
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 38941
Filename: kmod-bnx2_4.14.167-1_mipsel_24kc.ipk
Size: 39681
SHA256sum: b866f1d08a46e318c1dec2f54a7079e3733a7a5bf62a29fb7dad3a602e9e46c8
Description:  Kernel module for the BCM5706/5708/5709/5716 ethernet adapter

Package: kmod-bonding
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-bonding
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 59116
Filename: kmod-bonding_4.14.167-1_mipsel_24kc.ipk
Size: 59719
SHA256sum: be5cb24f68edbefe05cf91f97ab1f84346cbc901125f2eb18f0162d9bce74b97
Description:  Kernel module for NIC bonding.

Package: kmod-bpf-test
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-bpf-test
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 20711
Filename: kmod-bpf-test_4.14.167-1_mipsel_24kc.ipk
Size: 18890
SHA256sum: 3948c9386e3146c36dec6b196e35815ed58f8f5415d3ea6e5af63b355b1f9233
Description:  Test Berkeley Packet Filter functionality

Package: kmod-br-netfilter
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-br-netfilter
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9048
Filename: kmod-br-netfilter_4.14.167-1_mipsel_24kc.ipk
Size: 9812
SHA256sum: e9d4fff1dda2538472c32dbefb1bdf58d20dcfd47202ef631f2f6646fe398aa8
Description:  Bridge netfilter support modules

Package: kmod-brcmfmac
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-cfg80211, kmod-brcmutil, kmod-usb-core, brcmfmac-firmware-usb
Source: package/kernel/mac80211
SourceName: kmod-brcmfmac
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 106127
Filename: kmod-brcmfmac_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 106388
SHA256sum: 541469cd4d6d23a85b237d6d36908f3a3793ee26fe292a631818c9154a9343d5
Description:  Kernel module for Broadcom IEEE802.11n USB Wireless cards

Package: kmod-brcmsmac
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-bcma, kmod-lib-cordic, kmod-lib-crc8, kmod-brcmutil
Source: package/kernel/mac80211
SourceName: kmod-brcmsmac
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 229462
Filename: kmod-brcmsmac_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 226015
SHA256sum: 46ec526304708b38dc49d51a766df8cc98b9e442dd2fcfc820a6c5c22a85c281
Description:  Kernel module for Broadcom IEEE802.11n PCIe Wireless cards

Package: kmod-brcmutil
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/mac80211
SourceName: kmod-brcmutil
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 3570
Filename: kmod-brcmutil_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 4352
SHA256sum: b51fe77fc1c21954dc68d2f20c48f62fabe6dcfc8c2129d01aa776447d665240
Description:  This module contains some common parts needed by Broadcom Wireless drivers brcmsmac and brcmfmac.

Package: kmod-btmrvl
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mmc, kmod-bluetooth, mwifiex-sdio-firmware
Source: package/kernel/linux
SourceName: kmod-btmrvl
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 15593
Filename: kmod-btmrvl_4.14.167-1_mipsel_24kc.ipk
Size: 16314
SHA256sum: 398dfa79176faad1cccaa08dc855da928a20566bbf358295a7848b72f90a5771
Description:  Kernel support for Marvell SDIO Bluetooth Module

Package: kmod-button-hotplug
Version: 4.14.167-3
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-input-core
Source: package/kernel/button-hotplug
SourceName: kmod-button-hotplug
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2883
Filename: kmod-button-hotplug_4.14.167-3_mipsel_24kc.ipk
Size: 3669
SHA256sum: 496a870d1c808924cef76acc0818d42973d6f0cb76f3ec64793e75b47a598728
Description:  Kernel module to generate button uevent-s from input subsystem events.
 If your device uses GPIO buttons, see gpio-button-hotplug.

Package: kmod-can-bcm
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-can
Source: package/kernel/linux
SourceName: kmod-can-bcm
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10116
Filename: kmod-can-bcm_4.14.167-1_mipsel_24kc.ipk
Size: 10908
SHA256sum: e5e5419a0ea832c26ba057cbd76378e4bb452a95eb22bfe848d3a663033523c4
Description:  The Broadcast Manager offers content filtering, timeout monitoring,
 sending of RTR frames, and cyclic CAN messages without permanent user
 interaction.

Package: kmod-can-c-can-pci
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-can-c-can, kmod-can
Source: package/kernel/linux
SourceName: kmod-can-c-can-pci
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2205
Filename: kmod-can-c-can-pci_4.14.167-1_mipsel_24kc.ipk
Size: 2956
SHA256sum: d9f69e279542f6ec3d3e34b835fa66ac699714f3bad14a1b40076acea9c2fa11
Description:  This driver adds support for the C_CAN/D_CAN chips connected
 to the PCI bus.

Package: kmod-can-c-can-platform
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-can-c-can, kmod-regmap-core, kmod-can
Source: package/kernel/linux
SourceName: kmod-can-c-can-platform
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3060
Filename: kmod-can-c-can-platform_4.14.167-1_mipsel_24kc.ipk
Size: 4001
SHA256sum: 8f43c2048d358b56820e7323887856659183fc37bab49ad2dcad1fbe5c744a1a
Description:  This driver adds support for the C_CAN/D_CAN chips connected
 to the "platform bus" (Linux abstraction for directly to the
 processor attached devices) which can be found on various
 boards from ST Microelectronics (http://www.st.com) like the
 SPEAr1310 and SPEAr320 evaluation boards & TI (www.ti.com)
 boards like am335x, dm814x, dm813x and dm811x.

Package: kmod-can-c-can
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-can
Source: package/kernel/linux
SourceName: kmod-can-c-can
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5661
Filename: kmod-can-c-can_4.14.167-1_mipsel_24kc.ipk
Size: 6425
SHA256sum: d599374a71181a039c517af579a770387f1d80de5a3bc3f97d3289b4e52ca165
Description:  This driver adds generic support for the C_CAN/D_CAN chips.

Package: kmod-can-gw
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-can
Source: package/kernel/linux
SourceName: kmod-can-gw
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6004
Filename: kmod-can-gw_4.14.167-1_mipsel_24kc.ipk
Size: 6760
SHA256sum: 9a145702f757678219ed560f6ed5d8181c4eb5b7046958f8285552d41a236772
Description:  The CAN Gateway/Router is used to route (and modify) CAN frames.

Package: kmod-can-raw
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-can
Source: package/kernel/linux
SourceName: kmod-can-raw
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5201
Filename: kmod-can-raw_4.14.167-1_mipsel_24kc.ipk
Size: 5964
SHA256sum: 1fc26038b000153e59ec495d4e87327737cc1a1fa2a1dc295f3f8773a1cadfea
Description:  The raw CAN protocol option offers access to the CAN bus via
 the BSD  socket API.

Package: kmod-can-slcan
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-can
Source: package/kernel/linux
SourceName: kmod-can-slcan
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4511
Filename: kmod-can-slcan_4.14.167-1_mipsel_24kc.ipk
Size: 5306
SHA256sum: 1887e5a887364d4f5461aa27ba7a59bd6eb814af3f098b73ac2f6d69763c3022
Description:  CAN driver for several 'low cost' CAN interfaces that are attached
 via serial lines or via USB-to-serial adapters using the LAWICEL
 ASCII protocol.

Package: kmod-can-usb-8dev
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-can, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-can-usb-8dev
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6157
Filename: kmod-can-usb-8dev_4.14.167-1_mipsel_24kc.ipk
Size: 6987
SHA256sum: e77a6d36782cc554e978cc460a1f57a5f0fd213f5b36c086f796b39a1279e6e3
Description:  This driver supports the USB2CAN interface
 from 8 devices (http://www.8devices.com).

Package: kmod-can-usb-ems
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-can, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-can-usb-ems
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5883
Filename: kmod-can-usb-ems_4.14.167-1_mipsel_24kc.ipk
Size: 6703
SHA256sum: e419a08b338ea24aa6876be8578d099a7763a4b991cb84335262d49f020fe595
Description:  This driver is for the one channel CPC-USB/ARM7 CAN/USB interface
 from EMS Dr. Thomas Wuensche (http://www.ems-wuensche.de).

Package: kmod-can-usb-esd
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-can, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-can-usb-esd
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6469
Filename: kmod-can-usb-esd_4.14.167-1_mipsel_24kc.ipk
Size: 7323
SHA256sum: 83d275d7453ac06354f60949848ff6774f4f9bb659786e8047b0976c31855502
Description:  This driver supports the CAN-USB/2 interface
 from esd electronic system design gmbh (http://www.esd.eu).

Package: kmod-can-usb-kvaser
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-can, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-can-usb-kvaser
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9279
Filename: kmod-can-usb-kvaser_4.14.167-1_mipsel_24kc.ipk
Size: 10054
SHA256sum: b9c79f5d2f26b927e66d3751afbde00314e262158247a517a7037db21dc145aa
Description:  This driver adds support for Kvaser CAN/USB devices like Kvaser
 Leaf Light.

Package: kmod-can-usb-peak
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-can, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-can-usb-peak
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 16507
Filename: kmod-can-usb-peak_4.14.167-1_mipsel_24kc.ipk
Size: 17275
SHA256sum: bebf70bea94ef71bf0d9d1ee843264cc25ac6f765625b6b8f9907c9dfae58d22
Description:  This driver supports the PCAN-USB and PCAN-USB Pro adapters
 from PEAK-System Technik (http://www.peak-system.com).

Package: kmod-can-vcan
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-can
Source: package/kernel/linux
SourceName: kmod-can-vcan
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1802
Filename: kmod-can-vcan_4.14.167-1_mipsel_24kc.ipk
Size: 2601
SHA256sum: ef78e7c7fe295859ee2e0d90e2a10e2d9eb857039aceaee8e4e5e9cacfce2d5c
Description:  Similar to the network loopback devices, vcan offers a
 virtual local CAN interface.

Package: kmod-can
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-can
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 17137
Filename: kmod-can_4.14.167-1_mipsel_24kc.ipk
Size: 17882
SHA256sum: 4f31c5651f8d4029fcbe8c1f4d5e21ec67a7faf3c37e6980e042793e2e34ad10
Description:  Kernel module for CAN bus support.

Package: kmod-capi
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-capi
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 20778
Filename: kmod-capi_4.14.167-1_mipsel_24kc.ipk
Size: 21481
SHA256sum: 11b145f8aefbd9e00b8158b0e26021c9ec35be48c60feb6c023d478512accc40
Description:  Kernel module for basic CAPI (ISDN) support

Package: kmod-carl9170
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-ath, kmod-usb-core, kmod-input-core, carl9170-firmware
Source: package/kernel/mac80211
SourceName: kmod-carl9170
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 50879
Filename: kmod-carl9170_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 51545
SHA256sum: 867e8d2ff6b94abbfaa8a45f0d19f22931281649acceab5d3355d6954ad4ac59
Description:  Driver for Atheros AR9170 USB sticks

Package: kmod-cc2520
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac802154
Source: package/kernel/linux
SourceName: kmod-cc2520
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5130
Filename: kmod-cc2520_4.14.167-1_mipsel_24kc.ipk
Size: 5850
SHA256sum: 295e0e3a6ef8425dd98e761947db2ed2d416929542516afbd1fdaa89db0eb1e0
Description:  CC2520 transceiver driver

Package: kmod-cfg80211
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), iw, wireless-regdb
Source: package/kernel/mac80211
SourceName: kmod-cfg80211
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 139036
Filename: kmod-cfg80211_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 139452
SHA256sum: 022fa1642f2ff4d7108651d0a4e551442ba467c58610dbab79ff9064407416f3
Description:  cfg80211 is the Linux wireless LAN (802.11) configuration API.

Package: kmod-chaoskey
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-random-core, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-chaoskey
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3348
Filename: kmod-chaoskey_4.14.167-1_mipsel_24kc.ipk
Size: 4106
SHA256sum: da1fc6a8b601ad97d247e449954e567bf5bfc7a23c88b8777e382d33c182574c
Description:  Kernel module for chaoskey, USB attached true random number generator

Package: kmod-crypto-acompress
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-crypto-acompress
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3321
Filename: kmod-crypto-acompress_4.14.167-1_mipsel_24kc.ipk
Size: 4050
SHA256sum: 4999a8f2682e6185e1ed11c2ad37e7833fa72c730764be76fdc8f1a1f7e85ee8
Description:  Asynchronous Compression operations

Package: kmod-crypto-aead
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-null
Source: package/kernel/linux
SourceName: kmod-crypto-aead
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3227
Filename: kmod-crypto-aead_4.14.167-1_mipsel_24kc.ipk
Size: 3961
SHA256sum: 33acd443285b558e631e18051fda196409a172cd7b4b5af4e705c29e0d1f78c4
Description:  CryptoAPI AEAD support

Package: kmod-crypto-authenc
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-manager, kmod-crypto-null
Source: package/kernel/linux
SourceName: kmod-crypto-authenc
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3331
Filename: kmod-crypto-authenc_4.14.167-1_mipsel_24kc.ipk
Size: 4071
SHA256sum: 3ab2dc483b197b1b66e90c3b751856d080fbc397766729abb958ededeeed7710
Description:  Combined mode wrapper for IPsec

Package: kmod-crypto-cbc
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-manager
Source: package/kernel/linux
SourceName: kmod-crypto-cbc
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2175
Filename: kmod-crypto-cbc_4.14.167-1_mipsel_24kc.ipk
Size: 2945
SHA256sum: 16a733235936b510a59bd177749702456315b1401375373bc1e312b152786aa2
Description:  Cipher Block Chaining CryptoAPI module

Package: kmod-crypto-ccm
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-ctr, kmod-crypto-aead
Source: package/kernel/linux
SourceName: kmod-crypto-ccm
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6184
Filename: kmod-crypto-ccm_4.14.167-1_mipsel_24kc.ipk
Size: 6990
SHA256sum: 2523f2f30daba0919c0321a76046474a10dcef8978e526a7577937c2402635c9
Description:  Support for Counter with CBC MAC (CCM)

Package: kmod-crypto-cmac
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-hash
Source: package/kernel/linux
SourceName: kmod-crypto-cmac
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2152
Filename: kmod-crypto-cmac_4.14.167-1_mipsel_24kc.ipk
Size: 2939
SHA256sum: 59dc00c29642d24b85986bff3a9aa5f23201c06a6ae0f85789de277fa53040e1
Description:  Support for Cipher-based Message Authentication Code (CMAC)

Package: kmod-crypto-crc32
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-hash
Source: package/kernel/linux
SourceName: kmod-crypto-crc32
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 989
Filename: kmod-crypto-crc32_4.14.167-1_mipsel_24kc.ipk
Size: 1747
SHA256sum: 17a53cbaea8c62877b8e225b9e3c7f4ed7146ad12ed2e6af889a00ffbc6b33cc
Description:  CRC32 CRC module

Package: kmod-crypto-crc32c
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-hash
Source: package/kernel/linux
SourceName: kmod-crypto-crc32c
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1007
Filename: kmod-crypto-crc32c_4.14.167-1_mipsel_24kc.ipk
Size: 1765
SHA256sum: ef618483a3bbc6169b8f345368e583bf5f9c003a73f29cbe2588e61eca085efa
Description:  CRC32c CRC module

Package: kmod-crypto-ctr
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-manager, kmod-crypto-seqiv, kmod-crypto-iv
Source: package/kernel/linux
SourceName: kmod-crypto-ctr
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2937
Filename: kmod-crypto-ctr_4.14.167-1_mipsel_24kc.ipk
Size: 3668
SHA256sum: abfa483355e9356c708ea7ea8e6a4bedb115dedd81e734daec68993c45972315
Description:  Counter Mode CryptoAPI module

Package: kmod-crypto-cts
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-manager
Source: package/kernel/linux
SourceName: kmod-crypto-cts
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2943
Filename: kmod-crypto-cts_4.14.167-1_mipsel_24kc.ipk
Size: 3676
SHA256sum: d967d9e7202521e72060dc3a83227f394f404eb1bfdf191c235a5aa650343e76
Description:  Cipher Text Stealing CryptoAPI module

Package: kmod-crypto-deflate
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-zlib-inflate, kmod-lib-zlib-deflate, kmod-crypto-acompress
Source: package/kernel/linux
SourceName: kmod-crypto-deflate
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2032
Filename: kmod-crypto-deflate_4.14.167-1_mipsel_24kc.ipk
Size: 2784
SHA256sum: 3d0380c29116b205b492c02c0fc57b4489b119abafa5f9ddeb09687da1558767
Description:  Deflate compression CryptoAPI module

Package: kmod-crypto-des
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-crypto-des
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9040
Filename: kmod-crypto-des_4.14.167-1_mipsel_24kc.ipk
Size: 9560
SHA256sum: e66044b1bb30fa2d661017f778b3ded7e9da80ad2099d4ea3100d8bc018ce59d
Description:  DES/3DES cipher CryptoAPI module

Package: kmod-crypto-ecb
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-manager
Source: package/kernel/linux
SourceName: kmod-crypto-ecb
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1557
Filename: kmod-crypto-ecb_4.14.167-1_mipsel_24kc.ipk
Size: 2329
SHA256sum: f11caa3d4da10a18c2acb20eb59d302d0056356844cfad01cf370ca2a37c46a9
Description:  Electronic CodeBook CryptoAPI module

Package: kmod-crypto-ecdh
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-kpp
Source: package/kernel/linux
SourceName: kmod-crypto-ecdh
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10099
Filename: kmod-crypto-ecdh_4.14.167-1_mipsel_24kc.ipk
Size: 10832
SHA256sum: 0b7001699cacef63b36f2bf16d095b2fb376763bbe752705d6e7d548c78fed8f
Description:  ECDH algorithm

Package: kmod-crypto-echainiv
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-aead
Source: package/kernel/linux
SourceName: kmod-crypto-echainiv
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1732
Filename: kmod-crypto-echainiv_4.14.167-1_mipsel_24kc.ipk
Size: 2499
SHA256sum: cb15176666bce338d505014e682bce189c6cba8d8ecd3fb8ed7a38295ee5a4c7
Description:  Encrypted Chain IV Generator

Package: kmod-crypto-fcrypt
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-crypto-fcrypt
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3977
Filename: kmod-crypto-fcrypt_4.14.167-1_mipsel_24kc.ipk
Size: 4706
SHA256sum: 52d8086d09af511fa534061ac1d4a143aa43d6238afb9731270ae8cce2c12646
Description:  FCRYPT cipher CryptoAPI module

Package: kmod-crypto-gcm
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-ctr, kmod-crypto-ghash, kmod-crypto-null
Source: package/kernel/linux
SourceName: kmod-crypto-gcm
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6764
Filename: kmod-crypto-gcm_4.14.167-1_mipsel_24kc.ipk
Size: 7518
SHA256sum: 8fba3941175cb91c6c1d68e13f41795541b07f9a504af325b12e89599fef2b75
Description:  GCM/GMAC CryptoAPI module

Package: kmod-crypto-gf128
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-crypto-gf128
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4651
Filename: kmod-crypto-gf128_4.14.167-1_mipsel_24kc.ipk
Size: 5390
SHA256sum: 4180351081dc7e38773bf146f3e6250f475afe8fdbea520ddbd4062ec054ca1a
Description:  GF(2^128) multiplication functions CryptoAPI module

Package: kmod-crypto-ghash
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-gf128, kmod-crypto-hash
Source: package/kernel/linux
SourceName: kmod-crypto-ghash
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1462
Filename: kmod-crypto-ghash_4.14.167-1_mipsel_24kc.ipk
Size: 2230
SHA256sum: 16a91c73b791cf9ad123e1eec00ee4fc18b4964bc7705369e81d02931cb1785a
Description:  GHASH digest CryptoAPI module

Package: kmod-crypto-hash
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-crypto-hash
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6383
Filename: kmod-crypto-hash_4.14.167-1_mipsel_24kc.ipk
Size: 7087
SHA256sum: 8b7551c099aa1b0af904ca7aa9cee15ffd51561f14e5816fc1b9cf444efd785b
Description:  CryptoAPI hash support

Package: kmod-crypto-hmac
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-hash, kmod-crypto-manager
Source: package/kernel/linux
SourceName: kmod-crypto-hmac
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2272
Filename: kmod-crypto-hmac_4.14.167-1_mipsel_24kc.ipk
Size: 3005
SHA256sum: 31b37af7b99331d49ad539da12d615945b9c86be6985645c18107550d4cad975
Description:  HMAC digest CryptoAPI module

Package: kmod-crypto-hw-ccp
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-authenc, kmod-crypto-hash, kmod-crypto-manager, kmod-random-core, kmod-crypto-sha1, kmod-crypto-sha256, kmod-crypto-rsa
Source: package/kernel/linux
SourceName: kmod-crypto-hw-ccp
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-crypto-hw-ccp_4.14.167-1_mipsel_24kc.ipk
Size: 873
SHA256sum: eaed67fa14d00fd4dd292c4640d5c99d2825aefce122186bbcb6d5b23481d860
Description:  AMD Cryptographic Coprocessor

Package: kmod-crypto-hw-geode
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-manager
Source: package/kernel/linux
SourceName: kmod-crypto-hw-geode
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-crypto-hw-geode_4.14.167-1_mipsel_24kc.ipk
Size: 844
SHA256sum: f96fcbb9200f90547755ab1ff8cbd0779c3d9813051c3c1ed27ce42ba339cd0e
Description:  AMD Geode hardware crypto module

Package: kmod-crypto-hw-hifn-795x
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-random-core, kmod-crypto-manager, kmod-crypto-des
Source: package/kernel/linux
SourceName: kmod-crypto-hw-hifn-795x
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10348
Filename: kmod-crypto-hw-hifn-795x_4.14.167-1_mipsel_24kc.ipk
Size: 11127
SHA256sum: 8884d51205a8d365eb14a99c836aa410af5fa350dcce85dbaf18a7021b75b312
Description:  HIFN 795x crypto accelerator

Package: kmod-crypto-hw-padlock
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-manager
Source: package/kernel/linux
SourceName: kmod-crypto-hw-padlock
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-crypto-hw-padlock_4.14.167-1_mipsel_24kc.ipk
Size: 856
SHA256sum: 75a4428b543a4339d4932a46db5a557b94fae172c2deac00b10fc91c610d7ef5
Description:  VIA PadLock ACE with AES/SHA hw crypto module

Package: kmod-crypto-hw-talitos
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-manager, kmod-crypto-hash, kmod-random-core, kmod-crypto-authenc, kmod-crypto-des
Source: package/kernel/linux
SourceName: kmod-crypto-hw-talitos
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-crypto-hw-talitos_4.14.167-1_mipsel_24kc.ipk
Size: 885
SHA256sum: 19b4be3710cdac37afee34df906a536139625412c1b4e9818ec2b31fed989298
Description:  Freescale integrated security engine (SEC) driver

Package: kmod-crypto-iv
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-manager, kmod-crypto-rng, kmod-crypto-wq
Source: package/kernel/linux
SourceName: kmod-crypto-iv
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 202
Filename: kmod-crypto-iv_4.14.167-1_mipsel_24kc.ipk
Size: 948
SHA256sum: c76b877e33fb27be31bd03f842b2894abe83ba9e6135f7ffb76bad4f7f4a248f
Description:  CryptoAPI initialization vectors

Package: kmod-crypto-kpp
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-crypto-kpp
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1157
Filename: kmod-crypto-kpp_4.14.167-1_mipsel_24kc.ipk
Size: 1911
SHA256sum: f16e10c78c2997f404f68895c4b33631c7b0be612b6a516bc8b0d899530b5284
Description:  Key-agreement Protocol Primitives

Package: kmod-crypto-manager
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-aead, kmod-crypto-hash, kmod-crypto-pcompress
Source: package/kernel/linux
SourceName: kmod-crypto-manager
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2359
Filename: kmod-crypto-manager_4.14.167-1_mipsel_24kc.ipk
Size: 3104
SHA256sum: d3bf081a768b439f50d3cb1846450fe79a455e56d1974bfd73f14cd2786de3fb
Description:  CryptoAPI algorithm manager

Package: kmod-crypto-md4
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-hash
Source: package/kernel/linux
SourceName: kmod-crypto-md4
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2388
Filename: kmod-crypto-md4_4.14.167-1_mipsel_24kc.ipk
Size: 3160
SHA256sum: 715fb840a8c2e29f586edae7deeb37152f86d7b2273f02154afb5606b0e35f9c
Description:  MD4 digest CryptoAPI module

Package: kmod-crypto-md5
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-hash
Source: package/kernel/linux
SourceName: kmod-crypto-md5
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3333
Filename: kmod-crypto-md5_4.14.167-1_mipsel_24kc.ipk
Size: 4070
SHA256sum: af3a1b1e358671bcc361ca70b4159f6a2a62571b0d666f3f9ba463a16c59f363
Description:  MD5 digest CryptoAPI module

Package: kmod-crypto-michael-mic
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-hash
Source: package/kernel/linux
SourceName: kmod-crypto-michael-mic
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1337
Filename: kmod-crypto-michael-mic_4.14.167-1_mipsel_24kc.ipk
Size: 2111
SHA256sum: a8de1bb64da13057bbcac138743f5bfa723c8b8324225698041a7acb58ac6b37
Description:  Michael MIC keyed digest CryptoAPI module

Package: kmod-crypto-misc
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-xts
Source: package/kernel/linux
SourceName: kmod-crypto-misc
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 110094
Filename: kmod-crypto-misc_4.14.167-1_mipsel_24kc.ipk
Size: 105010
SHA256sum: 8ce704f51151b842a77efa04c23936530346b85aac8433126b4e0dd785fe0f4d
Description:  Other CryptoAPI modules

Package: kmod-crypto-null
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-hash
Source: package/kernel/linux
SourceName: kmod-crypto-null
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1705
Filename: kmod-crypto-null_4.14.167-1_mipsel_24kc.ipk
Size: 2432
SHA256sum: 2870f20c669005fd43ba43ef6aad4107e925324240bd005736fd04b1a30a0ad5
Description:  Null CryptoAPI module

Package: kmod-crypto-pcbc
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-manager
Source: package/kernel/linux
SourceName: kmod-crypto-pcbc
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2032
Filename: kmod-crypto-pcbc_4.14.167-1_mipsel_24kc.ipk
Size: 2805
SHA256sum: 817df041ba0388ff08222a1cdbb3043e52d82dd9e7267b1a233ec5cba7ec82c4
Description:  Propagating Cipher Block Chaining CryptoAPI module

Package: kmod-crypto-pcompress
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-crypto-pcompress
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-crypto-pcompress_4.14.167-1_mipsel_24kc.ipk
Size: 838
SHA256sum: 0984f16b23ea8018496cebc6e0ddd8d5610631aebaf27b04c113f63208050854
Description:  CryptoAPI Partial (de)compression operations

Package: kmod-crypto-rmd160
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-hash
Source: package/kernel/linux
SourceName: kmod-crypto-rmd160
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5526
Filename: kmod-crypto-rmd160_4.14.167-1_mipsel_24kc.ipk
Size: 6248
SHA256sum: 45c7c3e901d55fed87d57ee598087dd715adc8335c4fb5643f1d7e19729a83ad
Description:  RIPEMD160 digest CryptoAPI module

Package: kmod-crypto-rng
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-hash, kmod-crypto-hmac, kmod-crypto-sha256
Source: package/kernel/linux
SourceName: kmod-crypto-rng
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 8570
Filename: kmod-crypto-rng_4.14.167-1_mipsel_24kc.ipk
Size: 9333
SHA256sum: 6a723bc0ea89d16cf2673506409d0a6550f44877da6e9a80d69f70a6ca4db9da
Description:  CryptoAPI random number generation

Package: kmod-crypto-rsa
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-manager, kmod-asn1-decoder
Source: package/kernel/linux
SourceName: kmod-crypto-rsa
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 13841
Filename: kmod-crypto-rsa_4.14.167-1_mipsel_24kc.ipk
Size: 14594
SHA256sum: f46f9fe28a81915c08b741781293b55c49d36c5a8d1284fb5dd9813fa41e3639
Description:  RSA algorithm

Package: kmod-crypto-seqiv
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-aead, kmod-crypto-rng
Source: package/kernel/linux
SourceName: kmod-crypto-seqiv
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1927
Filename: kmod-crypto-seqiv_4.14.167-1_mipsel_24kc.ipk
Size: 2703
SHA256sum: 023f5776949771f910eaf826d3dcf74e47d73dbdc7a862f347bad435f79b4dd1
Description:  CryptoAPI Sequence Number IV Generator

Package: kmod-crypto-sha1
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-hash
Source: package/kernel/linux
SourceName: kmod-crypto-sha1
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1805
Filename: kmod-crypto-sha1_4.14.167-1_mipsel_24kc.ipk
Size: 2574
SHA256sum: 0a1cb680715d745549af13bf85ec9d0d87671fb71929c0dd3bd8b9d38b3e6e4d
Description:  SHA1 digest CryptoAPI module

Package: kmod-crypto-sha256
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-hash
Source: package/kernel/linux
SourceName: kmod-crypto-sha256
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4842
Filename: kmod-crypto-sha256_4.14.167-1_mipsel_24kc.ipk
Size: 5596
SHA256sum: f52a6966f7a2523b2c88f870b89108b0bbcab6384a0f7dfdb3651274a459e758
Description:  SHA224 SHA256 digest CryptoAPI module

Package: kmod-crypto-sha512
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-hash
Source: package/kernel/linux
SourceName: kmod-crypto-sha512
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7008
Filename: kmod-crypto-sha512_4.14.167-1_mipsel_24kc.ipk
Size: 7803
SHA256sum: 05fbd1b989982cdb31de2690321f91a7977a153880f19232a9b4d6c178c7acf5
Description:  SHA512 digest CryptoAPI module

Package: kmod-crypto-test
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-manager
Source: package/kernel/linux
SourceName: kmod-crypto-test
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 17293
Filename: kmod-crypto-test_4.14.167-1_mipsel_24kc.ipk
Size: 16966
SHA256sum: 867d2e6a6ede1db0b8b786b3bbec79db0d87a422584c445d3870864a928538f6
Description:  Test CryptoAPI module

Package: kmod-crypto-user
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-hash, kmod-crypto-manager
Source: package/kernel/linux
SourceName: kmod-crypto-user
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 12029
Filename: kmod-crypto-user_4.14.167-1_mipsel_24kc.ipk
Size: 12780
SHA256sum: 950637a5f96d8cf25907aa810f2449e3a43229193ce2e952554cadffcf4898e7
Description:  CryptoAPI userspace interface

Package: kmod-crypto-wq
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-crypto-wq
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 194
Filename: kmod-crypto-wq_4.14.167-1_mipsel_24kc.ipk
Size: 925
SHA256sum: 924e2c7871fab60763d8a8fbb5f8938a1142b97844cc7d6f93e00623c7ea3e69
Description:  CryptoAPI work queue handling

Package: kmod-crypto-xcbc
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-hash, kmod-crypto-manager
Source: package/kernel/linux
SourceName: kmod-crypto-xcbc
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2037
Filename: kmod-crypto-xcbc_4.14.167-1_mipsel_24kc.ipk
Size: 2802
SHA256sum: 1b2b5617da75c479f8ed44914a367fe93c9afa02926a9410823a4d1977d3d0cd
Description:  XCBC CryptoAPI module

Package: kmod-crypto-xts
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-gf128, kmod-crypto-manager
Source: package/kernel/linux
SourceName: kmod-crypto-xts
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3973
Filename: kmod-crypto-xts_4.14.167-1_mipsel_24kc.ipk
Size: 4698
SHA256sum: 84698f5924bc4930af1e10109e07cbaf744a315588bf6c432b0587c3154c84ba
Description:  XTS cipher CryptoAPI module

Package: kmod-cryptodev
Version: 4.14.167+1.10-ramips-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-authenc, kmod-crypto-hash
Source: package/kernel/cryptodev-linux
SourceName: kmod-cryptodev
License: GPL-2.0
LicenseFiles: COPYING
Section: kernel
Maintainer: Ansuel Smith <ansuelsmth@gmail.com>
Architecture: mipsel_24kc
Installed-Size: 20383
Filename: kmod-cryptodev_4.14.167+1.10-ramips-1_mipsel_24kc.ipk
Size: 21125
SHA256sum: b252f84706a40140f4d05273842f44900fba98b6f885418465769ebddd074690
Description:  This is a driver for that allows to use the Linux kernel supported
 hardware ciphers by user-space applications.

Package: kmod-dahdi-dummy
Version: 4.14.167+2.11.1-20180111-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-dahdi
Source: feeds/telephony/libs/dahdi-linux
SourceName: kmod-dahdi-dummy
License: GPL-2.0
LicenseFiles: LICENSE
Section: kernel
Maintainer: Vittorio Gambaletta <openwrt@vittgam.net>
Architecture: mipsel_24kc
Installed-Size: 2291
Filename: kmod-dahdi-dummy_4.14.167+2.11.1-20180111-2_mipsel_24kc.ipk
Size: 3136
SHA256sum: 6811be4a017a89cd147248a8902cc4bf43b03347bc9d98bacd87de623e10f798
Description:  This package contains the dummy DAHDI driver providing only DAHDI timing
 without any real telephony hardware.

Package: kmod-dahdi-echocan-oslec
Version: 4.14.167+2.11.1-20180111-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-dahdi, kmod-echo
Source: feeds/telephony/libs/dahdi-linux
SourceName: kmod-dahdi-echocan-oslec
License: GPL-2.0
LicenseFiles: LICENSE
Section: kernel
Maintainer: Vittorio Gambaletta <openwrt@vittgam.net>
Architecture: mipsel_24kc
Installed-Size: 1430
Filename: kmod-dahdi-echocan-oslec_4.14.167+2.11.1-20180111-2_mipsel_24kc.ipk
Size: 2295
SHA256sum: f534d1f31092643ce5980fbac07c9eab06610c4737b6f327ec2dab5e0130ed19
Description:  This package contains DAHDI OSLEC echo canceller support.

Package: kmod-dahdi-hfcs
Version: 4.14.167+2.11.1-20180111-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-dahdi
Source: feeds/telephony/libs/dahdi-linux
SourceName: kmod-dahdi-hfcs
License: GPL-2.0
LicenseFiles: LICENSE
Section: kernel
Maintainer: Vittorio Gambaletta <openwrt@vittgam.net>
Architecture: mipsel_24kc
Installed-Size: 10385
Filename: kmod-dahdi-hfcs_4.14.167+2.11.1-20180111-2_mipsel_24kc.ipk
Size: 11233
SHA256sum: 46c62dcb626b82dca60cd75115d1ff433afe24ff02650c15c3b04493b37a79ee
Description:  This package contains DAHDI driver for HFC-S based PCI BRI adapters.

Package: kmod-dahdi
Version: 4.14.167+2.11.1-20180111-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-crc-ccitt
Source: feeds/telephony/libs/dahdi-linux
SourceName: kmod-dahdi
License: GPL-2.0
LicenseFiles: LICENSE
Section: kernel
Maintainer: Vittorio Gambaletta <openwrt@vittgam.net>
Architecture: mipsel_24kc
Installed-Size: 59690
Filename: kmod-dahdi_4.14.167+2.11.1-20180111-2_mipsel_24kc.ipk
Size: 59897
SHA256sum: be92a96f2066487028e186be42d76c7643b7a086541a65e9a0f809fe183d2431
Description:  This package contains DAHDI basic infrastructure.

Package: kmod-dax
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-dax
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4196
Filename: kmod-dax_4.14.167-1_mipsel_24kc.ipk
Size: 4917
SHA256sum: 91bde167a4d41047c4b35e8ec2d1a07a3ae05c02d36e8cc4a581bdbb159bdb49
Description:  DAX: direct access to differentiated memory

Package: kmod-dm9000
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mii
Source: package/kernel/linux
SourceName: kmod-dm9000
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 8655
Filename: kmod-dm9000_4.14.167-1_mipsel_24kc.ipk
Size: 9408
SHA256sum: 1e51d6176b68a2282b618229adacaf3782a7804448dfb50e219b1321c968f1d3
Description:  Kernel driver for Davicom 9000 Ethernet adapters.

Package: kmod-dm
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-manager, kmod-dax
Source: package/kernel/linux
SourceName: kmod-dm
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 88118
Filename: kmod-dm_4.14.167-1_mipsel_24kc.ipk
Size: 88750
SHA256sum: b36177ba43823e99bc37223d0423e8fb6287054ed813a6c0aeccd957aa2b2e18
Description:  Kernel module necessary for LVM2 support

Package: kmod-dma-buf
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-dma-buf
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10795
Filename: kmod-dma-buf_4.14.167-1_mipsel_24kc.ipk
Size: 11554
SHA256sum: 02c255d16ddc94ef4e99a3d1d25b8b16659c369fced9d638db335a9cd97ae347
Description:  DMA shared buffer support

Package: kmod-dma-ralink
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-dma-ralink
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6452
Filename: kmod-dma-ralink_4.14.167-1_mipsel_24kc.ipk
Size: 7209
SHA256sum: dcd09efa883fc4a2148c700e391aa1c60bc7b60ea4820e0a43c18416b6211c59
Description:  Kernel modules for enable ralink dma engine.

Package: kmod-dnsresolver
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-dnsresolver
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4007
Filename: kmod-dnsresolver_4.14.167-1_mipsel_24kc.ipk
Size: 4719
SHA256sum: 7a1a177f10a6d32983bf545012cd3dae88b8582c7796797b17514194f833a476
Description:  In-kernel DNS Resolver

Package: kmod-dummy
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-dummy
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3061
Filename: kmod-dummy_4.14.167-1_mipsel_24kc.ipk
Size: 3778
SHA256sum: bd6d7a79e9bac31867158e3a020cc7d964d2c54db71697638e3c569b37e29717
Description:  The dummy network device

Package: kmod-e1000
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-e1000
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 50463
Filename: kmod-e1000_4.14.167-1_mipsel_24kc.ipk
Size: 51187
SHA256sum: 1f380168b6d9fc37fd2969c47f4272a57f94b56f5e2f4fabf5e7e286465fb74d
Description:  Kernel modules for Intel(R) PRO/1000 PCI Ethernet adapters.

Package: kmod-e100
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mii, e100-firmware
Source: package/kernel/linux
SourceName: kmod-e100
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 16348
Filename: kmod-e100_4.14.167-1_mipsel_24kc.ipk
Size: 17028
SHA256sum: 28e78b7b4b39b770e19818896aa8daff5866192e6797f97b9d2c7b52513cfbf6
Description:  Kernel modules for Intel(R) PRO/100+ Ethernet adapters

Package: kmod-ebtables-ipv4
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ebtables
Source: package/kernel/linux
SourceName: kmod-ebtables-ipv4
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3943
Filename: kmod-ebtables-ipv4_4.14.167-1_mipsel_24kc.ipk
Size: 4721
SHA256sum: 9513d480bc6b1a151d5c24f6d3d22fd40062b019db5b1a9ce131684dd3d5bd97
Description:  This option adds the IPv4 support to ebtables, which allows basic
 IPv4 header field filtering, ARP filtering as well as SNAT, DNAT targets.

Package: kmod-ebtables-ipv6
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ebtables
Source: package/kernel/linux
SourceName: kmod-ebtables-ipv6
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1667
Filename: kmod-ebtables-ipv6_4.14.167-1_mipsel_24kc.ipk
Size: 2473
SHA256sum: 0dcad195950c7e67c247ecf9a11ede31c389cf839eeec9272049106ba8bf9942
Description:  This option adds the IPv6 support to ebtables, which allows basic
 IPv6 header field filtering and target support.

Package: kmod-ebtables-watchers
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ebtables
Source: package/kernel/linux
SourceName: kmod-ebtables-watchers
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2830
Filename: kmod-ebtables-watchers_4.14.167-1_mipsel_24kc.ipk
Size: 3591
SHA256sum: 52392ae4f1457314324f68ea2d8805c254c0307dd3922cde69d2cc76ecae5b78
Description:  This option adds the log watchers, that you can use in any rule
 in any ebtables table.

Package: kmod-ebtables
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-ebtables
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 16081
Filename: kmod-ebtables_4.14.167-1_mipsel_24kc.ipk
Size: 16831
SHA256sum: ae2870d73d4a1a67779e6e9e144a78c826df513c897953586a527782f04065a7
Description:  ebtables is a general, extensible frame/packet identification
 framework. It provides you to do Ethernet
 filtering/NAT/brouting on the Ethernet bridge.

Package: kmod-echo
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-echo
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2660
Filename: kmod-echo_4.14.167-1_mipsel_24kc.ipk
Size: 3416
SHA256sum: 9002d7f75939a606bf9b440676deb47d2657ebee2136a65dcb9d92018c943803
Description:  This driver provides line echo cancelling support for mISDN and
 DAHDI drivers

Package: kmod-eeprom-93cx6
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-eeprom-93cx6
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1660
Filename: kmod-eeprom-93cx6_4.14.167-1_mipsel_24kc.ipk
Size: 2428
SHA256sum: 1ab4a0d3326dc21b02975ced62f3919b5c457910408be7fb09293673511a2912
Description:  Kernel module for EEPROM 93CX6 support

Package: kmod-eeprom-at24
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core, kmod-nvmem
Source: package/kernel/linux
SourceName: kmod-eeprom-at24
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4928
Filename: kmod-eeprom-at24_4.14.167-1_mipsel_24kc.ipk
Size: 5674
SHA256sum: 44eb4bd9a94a3f32ae586680bd4f0ec925545874116eb9ca564874e52fe26896
Description:  Kernel module for most I2C EEPROMs

Package: kmod-eeprom-at25
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nvmem
Source: package/kernel/linux
SourceName: kmod-eeprom-at25
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3330
Filename: kmod-eeprom-at25_4.14.167-1_mipsel_24kc.ipk
Size: 4065
SHA256sum: d89d2a0bdd52634a5a8f0e5c2008732ac055205a85dd6bf702b03dcc078b4135
Description:  Kernel module for most SPI EEPROMs

Package: kmod-et131x
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-libphy
Source: package/kernel/linux
SourceName: kmod-et131x
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 14908
Filename: kmod-et131x_4.14.167-1_mipsel_24kc.ipk
Size: 15619
SHA256sum: b985f2f2628c7719d7c2ca38ed2092f8c3930705849a26625f8bcd3be8927c3c
Description:  This package contains the et131x kernel module

Package: kmod-ethoc
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-libphy
Source: package/kernel/linux
SourceName: kmod-ethoc
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7608
Filename: kmod-ethoc_4.14.167-1_mipsel_24kc.ipk
Size: 8373
SHA256sum: 05cc96f2e306bbdbb6307c106ef088aa0116144409f51a987acf290fa9dc5191
Description:  Kernel module for the Opencores.org ethernet adapter

Package: kmod-fakelb
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac802154
Source: package/kernel/linux
SourceName: kmod-fakelb
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2486
Filename: kmod-fakelb_4.14.167-1_mipsel_24kc.ipk
Size: 3256
SHA256sum: 53b047df8859b83e141946f96b5b6612af953e5534ccb2e5b66a4d6b8e3c8dc5
Description:  Say Y here to enable the fake driver that can emulate a net
 of several interconnected radio devices.

Package: kmod-firewire-net
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-firewire
Source: package/kernel/linux
SourceName: kmod-firewire-net
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7803
Filename: kmod-firewire-net_4.14.167-1_mipsel_24kc.ipk
Size: 8565
SHA256sum: 6dbf25536d329a5ad6d47bae895960677c13f0fbbe6e0efc2ac3392fe6d7562f
Description:  Kernel support for IPv4 over FireWire

Package: kmod-firewire-ohci
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-firewire
Source: package/kernel/linux
SourceName: kmod-firewire-ohci
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 19093
Filename: kmod-firewire-ohci_4.14.167-1_mipsel_24kc.ipk
Size: 19793
SHA256sum: 00708ba2e28059c7584ecb7d2301988b27199feb1e2290cb4b49cf42c5b8e7ed
Description:  Kernel support for FireWire OHCI-1394 controllers

Package: kmod-firewire-sbp2
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-firewire, kmod-scsi-core
Source: package/kernel/linux
SourceName: kmod-firewire-sbp2
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 8129
Filename: kmod-firewire-sbp2_4.14.167-1_mipsel_24kc.ipk
Size: 8906
SHA256sum: 195580b81e223647f70644bc81bda053b5d97e1d06f56d0548b3a3050142b3e0
Description:  Kernel support for SBP-2 devices over FireWire

Package: kmod-firewire
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-crc-itu-t
Source: package/kernel/linux
SourceName: kmod-firewire
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 28362
Filename: kmod-firewire_4.14.167-1_mipsel_24kc.ipk
Size: 29081
SHA256sum: 020d5e5d23727458a3115c98eadd76683177bd67a05c89894b238645a6ed06b1
Description:  Kernel support for FireWire (new stack)

Package: kmod-forcedeth
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-forcedeth
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 24332
Filename: kmod-forcedeth_4.14.167-1_mipsel_24kc.ipk
Size: 25030
SHA256sum: 91b1d28887f8176cfb35cf7d931268253fbab9eeb7ac03ec9a07c5bb76df47b9
Description:  Kernel driver for Nvidia Ethernet support

Package: kmod-fou6
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-fou, kmod-ip6-tunnel
Source: package/kernel/linux
SourceName: kmod-fou6
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1324
Filename: kmod-fou6_4.14.167-1_mipsel_24kc.ipk
Size: 2145
SHA256sum: 935cbc742fa183bc4c6bb3a1a6a51e1cf29c7e394a4f2be6df0b158b73c317be
Description:  Kernel module for FOU (Foo over UDP) and GUE (Generic UDP Encapsulation) tunnelling over IPv6.
 Requires Kernel 3.18 or newer.

Package: kmod-fou
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-iptunnel, kmod-udptunnel4, kmod-udptunnel6
Source: package/kernel/linux
SourceName: kmod-fou
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6979
Filename: kmod-fou_4.14.167-1_mipsel_24kc.ipk
Size: 7828
SHA256sum: 85ca0137a4eb69efa769450269115b8dd61f436eb7124de44a8d5039e4d3fba3
Description:  Kernel module for FOU (Foo over UDP) and GUE (Generic UDP Encapsulation) tunnelling.
 Requires Kernel 3.18 or newer.

Package: kmod-fs-autofs4
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-fs-autofs4
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 13672
Filename: kmod-fs-autofs4_4.14.167-1_mipsel_24kc.ipk
Size: 14384
SHA256sum: 8dcc259ee745102ce0618386b4acc9344979ecceb532e6a2f1e67e5c54b1390c
Description:  Kernel module for AutoFS4 support

Package: kmod-fs-btrfs
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-crc32c, kmod-lib-lzo, kmod-lib-zlib-inflate, kmod-lib-zlib-deflate, kmod-lib-raid6, kmod-lib-xor, kmod-lib-zstd
Source: package/kernel/linux
SourceName: kmod-fs-btrfs
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 551115
Filename: kmod-fs-btrfs_4.14.167-1_mipsel_24kc.ipk
Size: 550549
SHA256sum: 980188438bd0ce64f598c94c4a66c8460d88b2b6a5bfc74bcb7572b1aa6367f1
Description:  Kernel module for BTRFS support

Package: kmod-fs-cifs
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base, kmod-crypto-hmac, kmod-crypto-md5, kmod-crypto-md4, kmod-crypto-des, kmod-crypto-ecb, kmod-crypto-sha256
Source: package/kernel/linux
SourceName: kmod-fs-cifs
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 184228
Filename: kmod-fs-cifs_4.14.167-1_mipsel_24kc.ipk
Size: 181163
SHA256sum: 5636c998a70c5f22c3c72b9d512b906bd6513a9ded7f40552f21ff9910d1a287
Description:  Kernel module for CIFS support

Package: kmod-fs-configfs
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-fs-configfs
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 13223
Filename: kmod-fs-configfs_4.14.167-1_mipsel_24kc.ipk
Size: 13951
SHA256sum: ce83f3fe0d2ef423f51fc48f8ae260434d2d2483a30dd298bb44a1f6bc6efb2a
Description:  Kernel module for configfs support

Package: kmod-fs-cramfs
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-zlib-inflate
Source: package/kernel/linux
SourceName: kmod-fs-cramfs
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4967
Filename: kmod-fs-cramfs_4.14.167-1_mipsel_24kc.ipk
Size: 5697
SHA256sum: 5104b312787dd11872c23b68c35339eee7103c2485845eaa7ceafa1293d0b6a3
Description:  Kernel module for cramfs support

Package: kmod-fs-exfat
Version: 4.14.167+2018-04-17-01c30ad5-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: feeds/packages/kernel/exfat-nofuse
SourceName: kmod-fs-exfat
License: GPL-2.0
LicenseFiles: LICENSE
Section: kernel
Maintainer: Yousong Zhou <yszhou4tech@gmail.com>
Architecture: mipsel_24kc
Installed-Size: 49015
Filename: kmod-fs-exfat_4.14.167+2018-04-17-01c30ad5-2_mipsel_24kc.ipk
Size: 49637
SHA256sum: 85934625f150166bc87d46625236a3e18a34dd1a5998c17af1071da96b5b5b04
Description:  Kernel module for ExFAT Filesytems

Package: kmod-fs-exportfs
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-fs-exportfs
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 233
Filename: kmod-fs-exportfs_4.14.167-1_mipsel_24kc.ipk
Size: 974
SHA256sum: 8b271dc4e9c724e5c6b73de477165a233b0aaac351f15c8d85857ba6f38bcf5d
Description:  Kernel module for exportfs. Needed for some other modules.

Package: kmod-fs-ext4
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-crc16, kmod-crypto-hash, kmod-crypto-crc32c
Source: package/kernel/linux
SourceName: kmod-fs-ext4
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 257304
Filename: kmod-fs-ext4_4.14.167-1_mipsel_24kc.ipk
Size: 257317
SHA256sum: fb19318261f59bb5f0919df96a75b55d5b1a7cdf5327becdf34aa6e9578da40a
Description:  Kernel module for EXT4 filesystem support

Package: kmod-fs-f2fs
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-hash, kmod-crypto-crc32
Source: package/kernel/linux
SourceName: kmod-fs-f2fs
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 147652
Filename: kmod-fs-f2fs_4.14.167-1_mipsel_24kc.ipk
Size: 147883
SHA256sum: 540424a3b7549a6672ced7f036faa79f65cf91c0f8c460b0f327a916efe71167
Description:  Kernel module for F2FS filesystem support

Package: kmod-fs-fscache
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-fs-fscache
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 23636
Filename: kmod-fs-fscache_4.14.167-1_mipsel_24kc.ipk
Size: 24296
SHA256sum: 68e358cdaa9a07965a823c353b668afa312c62a405aa5f889cf3524b6e56c01c
Description:  General filesystem local cache manager

Package: kmod-fs-hfs
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-fs-hfs
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 29254
Filename: kmod-fs-hfs_4.14.167-1_mipsel_24kc.ipk
Size: 29881
SHA256sum: 41a0923099c330ca8f331e7f7695b213d1ba8db160867c3c9254517d668561e7
Description:  Kernel module for HFS filesystem support

Package: kmod-fs-hfsplus
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base, kmod-nls-utf8
Source: package/kernel/linux
SourceName: kmod-fs-hfsplus
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 57034
Filename: kmod-fs-hfsplus_4.14.167-1_mipsel_24kc.ipk
Size: 57536
SHA256sum: 8684fbc2ab96bf5c4598f9692bf5f78c7864799cdde104dbd4a25f5808cd59c9
Description:  Kernel module for HFS+ filesystem support

Package: kmod-fs-isofs
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-zlib-inflate, kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-fs-isofs
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 16004
Filename: kmod-fs-isofs_4.14.167-1_mipsel_24kc.ipk
Size: 16718
SHA256sum: 9ea9991ab164b75cc71aae697d1e2e66a4122998ff4de2cff5a4845f43def63c
Description:  Kernel module for ISO9660 filesystem support

Package: kmod-fs-jfs
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-fs-jfs
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 94859
Filename: kmod-fs-jfs_4.14.167-1_mipsel_24kc.ipk
Size: 95255
SHA256sum: c84fb20ca6269ad9566ad2550d703b55e6fa0886baac54edc892dec5ddb9b79d
Description:  Kernel module for JFS support

Package: kmod-fs-ksmbd
Version: 4.14.167+3.1.1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base, kmod-nls-utf8, kmod-crypto-md4, kmod-crypto-md5, kmod-crypto-hmac, kmod-crypto-ecb, kmod-crypto-des, kmod-crypto-sha256, kmod-crypto-cmac, kmod-crypto-sha512, kmod-crypto-aead, kmod-crypto-ccm, kmod-crypto-gcm
Source: feeds/packages/kernel/ksmbd
SourceName: kmod-fs-ksmbd
License: GPL-2.0-or-later
LicenseFiles: COPYING
Section: kernel
Maintainer: Andy Walsh <andy.walsh44+github@gmail.com>
Architecture: mipsel_24kc
Installed-Size: 84349
Filename: kmod-fs-ksmbd_4.14.167+3.1.1-1_mipsel_24kc.ipk
Size: 85060
SHA256sum: 5685d05dcfc904cd03e9a667ce6a2e807f5c55f2751ffe94a567cda5715a3292
Description:  Ksmbd is an In-kernel SMB2/3 fileserver.
 It's an implementation of the SMB protocol in kernel space for sharing files and IPC services over network.

Package: kmod-fs-minix
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-fs-minix
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 14336
Filename: kmod-fs-minix_4.14.167-1_mipsel_24kc.ipk
Size: 15055
SHA256sum: 687468937800e6738f1466825b424ec46d3937a66a44259f8d5596876dda01c0
Description:  Kernel module for Minix filesystem support

Package: kmod-fs-msdos
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-fs-vfat, kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-fs-msdos
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5028
Filename: kmod-fs-msdos_4.14.167-1_mipsel_24kc.ipk
Size: 5766
SHA256sum: ebed37642c9ca7d263db3aee6a8e0e3d44135f8ad4958c1fae1620c663f962b1
Description:  Kernel module for MSDOS filesystem support

Package: kmod-fs-nfs-common-rpcsec
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-fs-nfs-common, kmod-crypto-des, kmod-crypto-cbc, kmod-crypto-cts, kmod-crypto-md5, kmod-crypto-sha1, kmod-crypto-hmac, kmod-crypto-ecb
Source: package/kernel/linux
SourceName: kmod-fs-nfs-common-rpcsec
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 37816
Filename: kmod-fs-nfs-common-rpcsec_4.14.167-1_mipsel_24kc.ipk
Size: 38633
SHA256sum: 5f60be80c01460e5cd7cc61a6191a704f19cf7f745c7a22349e1140101a7ef41
Description:  Kernel modules for NFS Secure RPC

Package: kmod-fs-nfs-common
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-fs-nfs-common
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 117084
Filename: kmod-fs-nfs-common_4.14.167-1_mipsel_24kc.ipk
Size: 117615
SHA256sum: d7cd906b876ea7112e98ec701c159e1187db7bcb7a937a40ce7f2aeb500ea3a4
Description:  Common NFS filesystem modules

Package: kmod-fs-nfs-v3
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-fs-nfs
Source: package/kernel/linux
SourceName: kmod-fs-nfs-v3
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10428
Filename: kmod-fs-nfs-v3_4.14.167-1_mipsel_24kc.ipk
Size: 11147
SHA256sum: 8442b54084a6d2fc8a45f2d81a823170248313e3f2e0d0379972b9ea0e085dfb
Description:  Kernel module for NFS v3 client support

Package: kmod-fs-nfs-v4
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-fs-nfs
Source: package/kernel/linux
SourceName: kmod-fs-nfs-v4
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 71628
Filename: kmod-fs-nfs-v4_4.14.167-1_mipsel_24kc.ipk
Size: 72298
SHA256sum: 8ae9db97d86a64885cf680227066dd0904279fb6e9a085ffddf9ae0e5ff972e2
Description:  Kernel module for NFS v4 support

Package: kmod-fs-nfs
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-fs-nfs-common, kmod-dnsresolver
Source: package/kernel/linux
SourceName: kmod-fs-nfs
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 69863
Filename: kmod-fs-nfs_4.14.167-1_mipsel_24kc.ipk
Size: 70423
SHA256sum: 23a0620c9dcd4ecafe2727e6bfd22a9ce29dc9a7aeb766d39eec37302aa7b2d8
Description:  Kernel module for NFS client support

Package: kmod-fs-nfsd
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-fs-nfs-common, kmod-fs-exportfs, kmod-fs-nfs-common-rpcsec
Source: package/kernel/linux
SourceName: kmod-fs-nfsd
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 113283
Filename: kmod-fs-nfsd_4.14.167-1_mipsel_24kc.ipk
Size: 113577
SHA256sum: a7dac8279cb6c5a02dabb36340b6f921fc956c9d8a16cbd4af731f9a840b47a8
Description:  Kernel module for NFS kernel server support

Package: kmod-fs-ntfs
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-fs-ntfs
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 55717
Filename: kmod-fs-ntfs_4.14.167-1_mipsel_24kc.ipk
Size: 56252
SHA256sum: 0ad60ab67c90a6cc862650353061ec5717c883586276c4627e85dc065f3fc204
Description:  Kernel module for NTFS filesystem support

Package: kmod-fs-reiserfs
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-fs-reiserfs
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 123357
Filename: kmod-fs-reiserfs_4.14.167-1_mipsel_24kc.ipk
Size: 123583
SHA256sum: f6876132369fe004e91d529f9529560aac916d1b3bd584b538f29f209c8449df
Description:  Kernel module for ReiserFS support

Package: kmod-fs-squashfs
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-fs-squashfs
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 234
Filename: kmod-fs-squashfs_4.14.167-1_mipsel_24kc.ipk
Size: 969
SHA256sum: c00e2d5d477dbedfd1f443036b22f30ba199ba93d9ab4a325ffcfab91c6b49a9
Description:  Kernel module for SquashFS 4.0 support

Package: kmod-fs-udf
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-crc-itu-t, kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-fs-udf
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 51041
Filename: kmod-fs-udf_4.14.167-1_mipsel_24kc.ipk
Size: 51713
SHA256sum: 0803a357e30824566af6bc1bf474f701dd4fad3b5b635b269096aa616ebd1973
Description:  Kernel module for UDF filesystem support

Package: kmod-fs-vfat
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base, kmod-nls-cp437, kmod-nls-iso8859-1, kmod-nls-utf8
Source: package/kernel/linux
SourceName: kmod-fs-vfat
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 41163
Filename: kmod-fs-vfat_4.14.167-1_mipsel_24kc.ipk
Size: 41897
SHA256sum: c9fb5ec35dd8b8471bbdfae558ef9844e6318ca141014903edc4d05be6f02b90
Description:  Kernel module for VFAT filesystem support

Package: kmod-fs-xfs
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-fs-exportfs, kmod-lib-crc32c
Source: package/kernel/linux
SourceName: kmod-fs-xfs
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 339493
Filename: kmod-fs-xfs_4.14.167-1_mipsel_24kc.ipk
Size: 339047
SHA256sum: cf5b2413c291d380a35765e3ec3bc1f4b2bbd6c7c7475f4c3330188a6b5b05fe
Description:  Kernel module for XFS support

Package: kmod-fuse
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-fuse
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 47720
Filename: kmod-fuse_4.14.167-1_mipsel_24kc.ipk
Size: 48337
SHA256sum: a7e8ac148142f2536fb0e2e726918063874c18b99b212732ceb3c6700daa5673
Description:  Kernel module for userspace filesystem support

Package: kmod-geneve
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-iptunnel, kmod-udptunnel4, kmod-udptunnel6
Source: package/kernel/linux
SourceName: kmod-geneve
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 11382
Filename: kmod-geneve_4.14.167-1_mipsel_24kc.ipk
Size: 12186
SHA256sum: 46cebbf783c1c5742cb4eaf140915fad7991464a25bc5e5f239aa85c4c7acecf
Description:  Kernel module for supporting Geneve in the Kernel.
 Requires Kernel 3.18 or newer.

Package: kmod-gigaset
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-isdn4linux, kmod-lib-crc-ccitt, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-gigaset
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 51146
Filename: kmod-gigaset_4.14.167-1_mipsel_24kc.ipk
Size: 51985
SHA256sum: 6f51d43ffc64164530a49206037a1d4da340a85f056a9017fc831e63abbc1971
Description:  This driver supports the Siemens Gigaset SX205/255 family of
 ISDN DECT bases, including the predecessors Gigaset 3070/3075
 and 4170/4175 and their T-Com versions Sinus 45isdn and Sinus
 721X.

Package: kmod-gpio-beeper
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-input-core
Source: package/kernel/linux
SourceName: kmod-gpio-beeper
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1301
Filename: kmod-gpio-beeper_4.14.167-1_mipsel_24kc.ipk
Size: 2086
SHA256sum: 24ca998c70535c30ca0b74f9f1570633b057d5a1812e566caad22dfa25893c6e
Description:  This enables playing beeps through an GPIO-connected buzzer

Package: kmod-gpio-button-hotplug
Version: 4.14.167-3
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/gpio-button-hotplug
SourceName: kmod-gpio-button-hotplug
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5806
Filename: kmod-gpio-button-hotplug_4.14.167-3_mipsel_24kc.ipk
Size: 6711
SHA256sum: a7ab389f320a9e1323c975d0be439baa871d9adbbd9d200d23a27f1cbaf265e0
Description:  This is a replacement for the following in-kernel drivers:
 1) gpio_keys (KEYBOARD_GPIO)
 2) gpio_keys_polled (KEYBOARD_GPIO_POLLED)
 
 Instead of generating input events (like in-kernel drivers do) it generates
 uevent-s and broadcasts them. This allows disabling input subsystem which is
 an overkill for OpenWrt simple needs.

Package: kmod-gpio-dev
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-gpio-dev
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-gpio-dev_4.14.167-1_mipsel_24kc.ipk
Size: 852
SHA256sum: 96ad0183ab354fe3325747c3c01af3b947ec9809cb47c1bf318126d9e4c808d7
Description:  Kernel module to allows control of GPIO pins using a character device.

Package: kmod-gpio-mcp23s08
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core, kmod-regmap-i2c
Source: package/kernel/linux
SourceName: kmod-gpio-mcp23s08
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6519
Filename: kmod-gpio-mcp23s08_4.14.167-1_mipsel_24kc.ipk
Size: 7295
SHA256sum: 06b0fd752a7961312a0f5f9b943b4dfdea5dea9ef645c1ea73e8b73162b56407
Description:  Kernel module for Microchip MCP23xxx SPI/I2C I/O expander

Package: kmod-gpio-nxp-74hc164
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-gpio-nxp-74hc164
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2152
Filename: kmod-gpio-nxp-74hc164_4.14.167-1_mipsel_24kc.ipk
Size: 2883
SHA256sum: 317583ce5344116fdda93f82af42858dc3d8aa0e26df021c5dd98dbcb2a79ac3
Description:  Kernel module for NXP 74HC164 GPIO expander

Package: kmod-gpio-pca953x
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-gpio-pca953x
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4121
Filename: kmod-gpio-pca953x_4.14.167-1_mipsel_24kc.ipk
Size: 4935
SHA256sum: 662eb7d958f3cbb1f8d79b11143caab9552b24f6b0cf628a88d258d9d7c36860
Description:  Kernel module for MAX731{0,2,3,5}, PCA6107, PCA953{4-9}, PCA955{4-7},
 PCA957{4,5} and TCA64{08,16} I2C GPIO expanders

Package: kmod-gpio-pcf857x
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-gpio-pcf857x
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2973
Filename: kmod-gpio-pcf857x_4.14.167-1_mipsel_24kc.ipk
Size: 3740
SHA256sum: 5ec71f6900c8774906c42447de02a95bcd498ccc995f6d0a9037a16adbc2a214
Description:  Kernel module for PCF857x, PCA{85,96}7x, and MAX732[89] I2C GPIO expanders

Package: kmod-gre6
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-iptunnel, kmod-ip6-tunnel, kmod-gre
Source: package/kernel/linux
SourceName: kmod-gre6
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10081
Filename: kmod-gre6_4.14.167-1_mipsel_24kc.ipk
Size: 10856
SHA256sum: 9efef09623afe1872404d5c5267442212bc1903d92fb6edb6d6b98fb30ccb84f
Description:  Generic Routing Encapsulation support over IPv6

Package: kmod-gre
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-iptunnel
Source: package/kernel/linux
SourceName: kmod-gre
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 11105
Filename: kmod-gre_4.14.167-1_mipsel_24kc.ipk
Size: 11814
SHA256sum: d5b08501d06fdc5835555c003e0bf3814832d3f54b5b92d536ed55a7db4d2273
Description:  Generic Routing Encapsulation support

Package: kmod-hermes-pci
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hermes
Source: package/kernel/mac80211
SourceName: kmod-hermes-pci
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 2300
Filename: kmod-hermes-pci_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 3061
SHA256sum: c0f1d247993e012d1d4064491722f9efadb4f7547e48b6e39c84338be2613d2d
Description:  Kernel modules for Intersil Prism 2.5 PCI support

Package: kmod-hermes-plx
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hermes
Source: package/kernel/mac80211
SourceName: kmod-hermes-plx
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 2838
Filename: kmod-hermes-plx_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 3598
SHA256sum: 7af41d6340ee6beb0bc38ec12a650b12b1657c2a250c228e91a624b421dca923
Description:  Kernel modules for Hermes in PLX9052 based PCI adaptors

Package: kmod-hermes
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-cfg80211, kmod-crypto-michael-mic
Source: package/kernel/mac80211
SourceName: kmod-hermes
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 32297
Filename: kmod-hermes_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 33107
SHA256sum: 28348e5b8fa7e3750503bab007c1c0a43423c7a70af115bfd871ea9a46f92eee
Description:  Kernel support for Hermes 802.11b chipsets

Package: kmod-hfcmulti
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-misdn
Source: package/kernel/linux
SourceName: kmod-hfcmulti
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 38225
Filename: kmod-hfcmulti_4.14.167-1_mipsel_24kc.ipk
Size: 38982
SHA256sum: 5e443c19a11d0dc535a4657024c26bf45b646a4290a70a319a86600312c53b8d
Description:  Kernel modules for Cologne AG's HFC multiport cards (HFC-4S/8S/E1)
 using the mISDN V2 stack

Package: kmod-hfcpci
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-misdn
Source: package/kernel/linux
SourceName: kmod-hfcpci
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 14917
Filename: kmod-hfcpci_4.14.167-1_mipsel_24kc.ipk
Size: 15690
SHA256sum: 2c61b8be7190577cc6e95b352f5d226caa99398931c9188f9a522f6a72d18cec
Description:  Kernel modules for Cologne AG's HFC pci cards (single port)
 using the mISDN V2 stack

Package: kmod-hid-generic
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hid
Source: package/kernel/linux
SourceName: kmod-hid-generic
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 788
Filename: kmod-hid-generic_4.14.167-1_mipsel_24kc.ipk
Size: 1532
SHA256sum: 6b3370c6f97064f923137662b6c77f203085e818ceb3a1475d2b596f2a80389a
Description:  Generic HID device support

Package: kmod-hid
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-input-core, kmod-input-evdev
Source: package/kernel/linux
SourceName: kmod-hid
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 44237
Filename: kmod-hid_4.14.167-1_mipsel_24kc.ipk
Size: 43164
SHA256sum: 0af6ee9c649627d4ff62204c14fa7a323e504b9c1cd969dd6297779174326185
Description:  Kernel modules for HID devices

Package: kmod-hwmon-adcxx
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core
Source: package/kernel/linux
SourceName: kmod-hwmon-adcxx
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2328
Filename: kmod-hwmon-adcxx_4.14.167-1_mipsel_24kc.ipk
Size: 3232
SHA256sum: dd115b823f0d43a941a9ed17f46f368360dbe2d7697c6f2ce4e7eba95689f625
Description:  Kernel module for the National Semiconductor
 ADC<bb><c>S<sss> chip family, where
 * bb  is the resolution in number of bits (8, 10, 12)
 * c   is the number of channels (1, 2, 4, 8)
 * sss is the maximum conversion speed (021 for 200 kSPS, 051 for 500
 kSPS and 101 for 1 MSPS)
 
 Examples : ADC081S101, ADC124S501, ...

Package: kmod-hwmon-ads1015
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-hwmon-ads1015
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2676
Filename: kmod-hwmon-ads1015_4.14.167-1_mipsel_24kc.ipk
Size: 3438
SHA256sum: a8023a027c0fdeb7dfb53139a00393b26177ce2e100827ec35a1d7eb0144b6d8
Description:  Kernel module for Texas Instruments ADS1015 Analog-to-Digital converter

Package: kmod-hwmon-adt7410
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-hwmon-adt7410
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3538
Filename: kmod-hwmon-adt7410_4.14.167-1_mipsel_24kc.ipk
Size: 4302
SHA256sum: bb240ebd60bbc560e1f38a97ae2d5016795cabff2a33d877340c0f1994b24266
Description:  Kernel module for ADT7410/7420 I2C thermal monitor chip

Package: kmod-hwmon-adt7475
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core, kmod-hwmon-vid
Source: package/kernel/linux
SourceName: kmod-hwmon-adt7475
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9565
Filename: kmod-hwmon-adt7475_4.14.167-1_mipsel_24kc.ipk
Size: 10342
SHA256sum: 944aa70d4f3f1efa87d63c2e8ee0299e2eb5c58ce71a29ea89df0c037c585406
Description:  Kernel module for ADT7473/7475/7476/7490 thermal monitor chip

Package: kmod-hwmon-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-hwmon-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4729
Filename: kmod-hwmon-core_4.14.167-1_mipsel_24kc.ipk
Size: 5448
SHA256sum: c063d58e920189fa87499397119d3f32ea4e63cb79b5360316f042324e75447a
Description:  Kernel modules for hardware monitoring

Package: kmod-hwmon-gpiofan
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-hwmon-gpiofan
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3777
Filename: kmod-hwmon-gpiofan_4.14.167-1_mipsel_24kc.ipk
Size: 4516
SHA256sum: 5ad01579533c0ba9f7df31d24971ad1026f25339cc64a355107cb557585d87f2
Description:  Kernel module for GPIO controlled FANs

Package: kmod-hwmon-ina209
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-hwmon-ina209
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3726
Filename: kmod-hwmon-ina209_4.14.167-1_mipsel_24kc.ipk
Size: 4458
SHA256sum: eaadaafefb222cca0441b113302367b1a00dc2dcd77549e53a49a68ab7a04eff
Description:  Kernel module for ina209 dc power monitor chips

Package: kmod-hwmon-ina2xx
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core, kmod-regmap-i2c
Source: package/kernel/linux
SourceName: kmod-hwmon-ina2xx
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3267
Filename: kmod-hwmon-ina2xx_4.14.167-1_mipsel_24kc.ipk
Size: 4017
SHA256sum: b4dd83ef62213cc3f70a1c7cdb30f566618ffb2f1443c9d8fd322fa0aec9fb6e
Description:  Kernel module for ina2xx dc current monitor chips

Package: kmod-hwmon-it87
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core, kmod-hwmon-vid
Source: package/kernel/linux
SourceName: kmod-hwmon-it87
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 16331
Filename: kmod-hwmon-it87_4.14.167-1_mipsel_24kc.ipk
Size: 16961
SHA256sum: e26a04c8b840fe1de51d8236997c30e10329c869dba7234bb887098fe904b25b
Description:  Kernel module for it87 thermal and voltage monitor chip

Package: kmod-hwmon-lm63
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core, kmod-regmap-i2c
Source: package/kernel/linux
SourceName: kmod-hwmon-lm63
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6181
Filename: kmod-hwmon-lm63_4.14.167-1_mipsel_24kc.ipk
Size: 6954
SHA256sum: eae8d7038a68485a236e37c1c8688372deb7e061ff8a1a1f956e194c19e1a6af
Description:  Kernel module for lm63 and lm64 thermal monitor chip

Package: kmod-hwmon-lm75
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core, kmod-regmap-i2c
Source: package/kernel/linux
SourceName: kmod-hwmon-lm75
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2896
Filename: kmod-hwmon-lm75_4.14.167-1_mipsel_24kc.ipk
Size: 3659
SHA256sum: 1481599c47d18fbee352d4c277eda198996b502c0f3afadfa07277128ec8cdc5
Description:  Kernel module for lm75 thermal monitor chip

Package: kmod-hwmon-lm77
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-hwmon-lm77
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2794
Filename: kmod-hwmon-lm77_4.14.167-1_mipsel_24kc.ipk
Size: 3547
SHA256sum: 834bc941cfc6caa9f0d9ea39b12d5e673ff4034e32a56675da3a7c962a59c5a1
Description:  Kernel module for LM77 thermal monitor chip

Package: kmod-hwmon-lm85
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core, kmod-hwmon-vid
Source: package/kernel/linux
SourceName: kmod-hwmon-lm85
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 8526
Filename: kmod-hwmon-lm85_4.14.167-1_mipsel_24kc.ipk
Size: 9227
SHA256sum: 222b820c6d00c04280b1e8c570ae5f58e907952bca6cc38151094b99ea1c8130
Description:  Kernel module for LM85 thermal monitor chip

Package: kmod-hwmon-lm90
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-hwmon-lm90
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7430
Filename: kmod-hwmon-lm90_4.14.167-1_mipsel_24kc.ipk
Size: 8207
SHA256sum: 81105675467bd37cf7a9898f367ae99cc1dd63e918672a9de66ff445750cf0e2
Description:  Kernel module for LM90 thermal monitor chip

Package: kmod-hwmon-lm92
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-hwmon-lm92
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2971
Filename: kmod-hwmon-lm92_4.14.167-1_mipsel_24kc.ipk
Size: 3712
SHA256sum: fef43d25adff4db9dce12454d2f6602618ce0f8a41ab5fbdd34d6cafe23747f7
Description:  Kernel module for LM92 thermal monitor chip

Package: kmod-hwmon-lm95241
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-hwmon-lm95241
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2530
Filename: kmod-hwmon-lm95241_4.14.167-1_mipsel_24kc.ipk
Size: 3275
SHA256sum: 080a017167492d92fd8fe5c02acecf63e9bfd6acdcb710f1e982be19c12d450b
Description:  Kernel module for LM95241 thermal monitor chip

Package: kmod-hwmon-ltc4151
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-hwmon-ltc4151
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1859
Filename: kmod-hwmon-ltc4151_4.14.167-1_mipsel_24kc.ipk
Size: 2666
SHA256sum: 6c47c2cb95d0e29d92924f9b4cecf8f305839837a803723ba1b06855f3d65612
Description:  Kernel module for Linear Technology LTC4151 current and voltage monitor chip

Package: kmod-hwmon-pwmfan
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core
Source: package/kernel/linux
SourceName: kmod-hwmon-pwmfan
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2309
Filename: kmod-hwmon-pwmfan_4.14.167-1_mipsel_24kc.ipk
Size: 3046
SHA256sum: 86fff301852c99e55a22710258bf99ef6b41fde88734fe2140ac99a51905387e
Description:  Kernel module for PWM controlled FANs

Package: kmod-hwmon-sch5627
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-hwmon-sch5627
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7226
Filename: kmod-hwmon-sch5627_4.14.167-1_mipsel_24kc.ipk
Size: 8008
SHA256sum: 1af6230b15915cde741fdd7cf7a16184bae07e979435f09fccb9ea1d9df53557
Description:  SMSC SCH5627 Super I/O chips include complete hardware monitoring

Package: kmod-hwmon-sht21
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-hwmon-sht21
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2050
Filename: kmod-hwmon-sht21_4.14.167-1_mipsel_24kc.ipk
Size: 2851
SHA256sum: a5259c50bc168464ac55290f932ab63e420b0322b32de78f72a785a30134f2d3
Description:  Kernel module for Sensirion SHT21 and SHT25 temperature and humidity sensors chip

Package: kmod-hwmon-tmp102
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core, kmod-regmap-i2c
Source: package/kernel/linux
SourceName: kmod-hwmon-tmp102
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1942
Filename: kmod-hwmon-tmp102_4.14.167-1_mipsel_24kc.ipk
Size: 2741
SHA256sum: d7bcbf216f03e99b3140505d43d9ad75d6e90c1807659fc368c71251db562532
Description:  Kernel module for Texas Instruments TMP102 temperature sensors chip

Package: kmod-hwmon-tmp103
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core, kmod-regmap-i2c
Source: package/kernel/linux
SourceName: kmod-hwmon-tmp103
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1593
Filename: kmod-hwmon-tmp103_4.14.167-1_mipsel_24kc.ipk
Size: 2401
SHA256sum: 7da060fcb14b72ac4b7f4366fae8bbf55f6bcc3ed52b7fa37f1ec576b8d5fc23
Description:  Kernel module for Texas Instruments TMP103 temperature sensors chip

Package: kmod-hwmon-tmp421
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-hwmon-tmp421
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2589
Filename: kmod-hwmon-tmp421_4.14.167-1_mipsel_24kc.ipk
Size: 3353
SHA256sum: 8b38c456121cd90750fdf7a727d33ce7b29d34a6c6f82fd54545272ac311a59b
Description:  Kernel module for the Texas Instruments TMP421 and compatible chips.

Package: kmod-hwmon-vid
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core
Source: package/kernel/linux
SourceName: kmod-hwmon-vid
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1706
Filename: kmod-hwmon-vid_4.14.167-1_mipsel_24kc.ipk
Size: 2490
SHA256sum: 14f9faea8256b0e74b7f15820b145e55e6dcb8d7903ddce62d76d39854ecec89
Description:  VID/VRM/VRD voltage conversion module for hardware monitoring

Package: kmod-hwmon-w83793
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core, kmod-hwmon-vid
Source: package/kernel/linux
SourceName: kmod-hwmon-w83793
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 14590
Filename: kmod-hwmon-w83793_4.14.167-1_mipsel_24kc.ipk
Size: 14930
SHA256sum: 516408678007388e9f9ecdd7966100ae7d8117abd0ed004ebe3e4afaa99a3eac
Description:  Kernel module for the Winbond W83793G and W83793R chips.

Package: kmod-i2c-algo-bit
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-i2c-algo-bit
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3533
Filename: kmod-i2c-algo-bit_4.14.167-1_mipsel_24kc.ipk
Size: 4273
SHA256sum: f909961355269741056f6113ee6bf35f2d1fda7cf59086a3beb4fa5b49169cf4
Description:  Kernel modules for I2C bit-banging interfaces

Package: kmod-i2c-algo-pca
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-i2c-algo-pca
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4180
Filename: kmod-i2c-algo-pca_4.14.167-1_mipsel_24kc.ipk
Size: 4910
SHA256sum: 28ece4566bd1016a2864693d1c5b7f8fef4cd5aff16f6837451b20ce319259c4
Description:  Kernel modules for I2C PCA 9564 interfaces

Package: kmod-i2c-algo-pcf
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-i2c-algo-pcf
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3272
Filename: kmod-i2c-algo-pcf_4.14.167-1_mipsel_24kc.ipk
Size: 4018
SHA256sum: 54bc4914e7a21dcaf4583361bd149099ecee68658e5240b2e447f98fd02cca99
Description:  Kernel modules for I2C PCF 8584 interfaces

Package: kmod-i2c-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-i2c-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 20161
Filename: kmod-i2c-core_4.14.167-1_mipsel_24kc.ipk
Size: 20830
SHA256sum: 0fc3863f5efe4c52c6d12420dce4d669021090775a0128cb0cd32614c1ef9620
Description:  Kernel modules for I2C support

Package: kmod-i2c-gpio-custom
Version: 4.14.167-3
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core, kmod-i2c-gpio
Source: package/kernel/i2c-gpio-custom
SourceName: kmod-i2c-gpio-custom
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1631
Filename: kmod-i2c-gpio-custom_4.14.167-3_mipsel_24kc.ipk
Size: 2395
SHA256sum: 0a3c5c46fa0a6ddd068710305469342cb5a7861f01417a8c28a04b4db6b2eeda
Description:  Kernel module for register a custom i2c-gpio platform device.

Package: kmod-i2c-gpio
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-algo-bit
Source: package/kernel/linux
SourceName: kmod-i2c-gpio
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2753
Filename: kmod-i2c-gpio_4.14.167-1_mipsel_24kc.ipk
Size: 3546
SHA256sum: bf4123bf2f2a27393d32d31436f6fa2f1cdcd12325503343a72a6edb7e226fb6
Description:  Kernel modules for a very simple bitbanging I2C driver utilizing the
 arch-neutral GPIO API to control the SCL and SDA lines.

Package: kmod-i2c-mt7628
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-i2c-mt7628
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2390
Filename: kmod-i2c-mt7628_4.14.167-1_mipsel_24kc.ipk
Size: 3127
SHA256sum: ce997f5deec933ebb4d3975d5c160fc6bba6dffac337abb3426363542fc882d0
Description:  Kernel modules for enable mt7621 i2c controller.

Package: kmod-i2c-mux-gpio
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-mux
Source: package/kernel/linux
SourceName: kmod-i2c-mux-gpio
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2900
Filename: kmod-i2c-mux-gpio_4.14.167-1_mipsel_24kc.ipk
Size: 3652
SHA256sum: 0e38ea9272913e202198cb4cff1d31dd0d4b3fd2bb27cbc9ac6c5025dea8ab69
Description:  Kernel modules for GENERIC_GPIO I2C bus mux/switching devices

Package: kmod-i2c-mux-pca9541
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-mux
Source: package/kernel/linux
SourceName: kmod-i2c-mux-pca9541
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2072
Filename: kmod-i2c-mux-pca9541_4.14.167-1_mipsel_24kc.ipk
Size: 2849
SHA256sum: 4013afbc529c749e0921d0fa15e0acebd19889d3f0b0d7c77ae9344d5725b721
Description:  Kernel modules for PCA9541 I2C bus mux/switching devices

Package: kmod-i2c-mux-pca954x
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-mux
Source: package/kernel/linux
SourceName: kmod-i2c-mux-pca954x
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3048
Filename: kmod-i2c-mux-pca954x_4.14.167-1_mipsel_24kc.ipk
Size: 3797
SHA256sum: 064440c482f0bf4428b30978e5f999f847956f265258e59b30eb40561e253636
Description:  Kernel modules for PCA954x I2C bus mux/switching devices

Package: kmod-i2c-mux
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-i2c-mux
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3451
Filename: kmod-i2c-mux_4.14.167-1_mipsel_24kc.ipk
Size: 4177
SHA256sum: 3a0f8569db6d5f173ddae99f64a0a895d4f9f8df5431ed98233e219aa1e0c4d9
Description:  Kernel modules for I2C bus multiplexing support

Package: kmod-i2c-smbus
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-i2c-smbus
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2111
Filename: kmod-i2c-smbus_4.14.167-1_mipsel_24kc.ipk
Size: 2886
SHA256sum: 1a44a7f93930d0b54cfb4ddf1276d45eb0fb7130fc189b0bf43e8d405eb27a01
Description:  Support for the SMBus extensions to the I2C specification.

Package: kmod-i2c-tiny-usb
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-i2c-tiny-usb
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2495
Filename: kmod-i2c-tiny-usb_4.14.167-1_mipsel_24kc.ipk
Size: 3283
SHA256sum: 536c431be02129894fa41b49efc77fb69c4d27ea7d70988a514b8f695ad0ad5a
Description:  Kernel module for the I2C Tiny USB adaptor developed
 by Till Harbaum (http://www.harbaum.org/till/i2c_tiny_usb)

Package: kmod-ieee802154
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-ieee802154
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 23832
Filename: kmod-ieee802154_4.14.167-1_mipsel_24kc.ipk
Size: 24718
SHA256sum: 7c2377c48bd6fa062497c2b2189afe0d8cacb0d55337d22d2b2052df35528cc3
Description:  IEEE Std 802.15.4 defines a low data rate, low power and low
 complexity short range wireless personal area networks. It was
 designed to organise networks of sensors, switches, etc automation
 devices. Maximum allowed data rate is 250 kb/s and typical personal
 operating space around 10m.

Package: kmod-ieee802154_6lowpan
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-6lowpan, kmod-ieee802154
Source: package/kernel/linux
SourceName: kmod-ieee802154_6lowpan
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 8171
Filename: kmod-ieee802154_6lowpan_4.14.167-1_mipsel_24kc.ipk
Size: 8941
SHA256sum: 1d6ccbd413e9387af917cfb2b8dba6061e8906d8639001bc68546a964ade7101
Description:  IPv6 compression over IEEE 802.15.4

Package: kmod-ifb
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-ifb
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3081
Filename: kmod-ifb_4.14.167-1_mipsel_24kc.ipk
Size: 3792
SHA256sum: 93fdc82e9f8603cfb96c495727e0c8bbef9b0aa40b166ef8e473745fbd19dc89
Description:  The Intermediate Functional Block

Package: kmod-igb
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core, kmod-i2c-algo-bit, kmod-ptp, kmod-hwmon-core
Source: package/kernel/linux
SourceName: kmod-igb
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 75597
Filename: kmod-igb_4.14.167-1_mipsel_24kc.ipk
Size: 76211
SHA256sum: 2318c0e018fd799f9cfa07a5ec5d771f8854abbbaa999276e49a3edf2e1a9fd9
Description:  Kernel modules for Intel(R) 82575/82576 PCI-Express Gigabit Ethernet adapters.

Package: kmod-iio-ad799x
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core, kmod-iio-core
Source: package/kernel/linux
SourceName: kmod-iio-ad799x
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3959
Filename: kmod-iio-ad799x_4.14.167-1_mipsel_24kc.ipk
Size: 4755
SHA256sum: 694cb40704127a145410721ef06d756f5afc8f164cc69813f5f7d31618672bf8
Description:  support for Analog Devices:
 ad7991, ad7995, ad7999, ad7992, ad7993, ad7994, ad7997, ad7998
 i2c analog to digital converters (ADC).

Package: kmod-iio-am2315
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core, kmod-iio-core
Source: package/kernel/linux
SourceName: kmod-iio-am2315
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2336
Filename: kmod-iio-am2315_4.14.167-1_mipsel_24kc.ipk
Size: 3089
SHA256sum: d4e176d3980907b008b391ed9556ce7ca376c4b52751fe1efe1aaf74cca19620
Description:  Aosong AM2315 humidity/temperature sensor (I2C bus)

Package: kmod-iio-bh1750
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core, kmod-iio-core
Source: package/kernel/linux
SourceName: kmod-iio-bh1750
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2106
Filename: kmod-iio-bh1750_4.14.167-1_mipsel_24kc.ipk
Size: 2887
SHA256sum: f5f6f32a23132fce7592774c8ed31f9e1c290c81a5ae00fc487ee12880492d35
Description:  ROHM BH1750 ambient light sensor (i2c bus)

Package: kmod-iio-bmp280-i2c
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-iio-bmp280, kmod-i2c-core, kmod-regmap-i2c
Source: package/kernel/linux
SourceName: kmod-iio-bmp280-i2c
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1205
Filename: kmod-iio-bmp280-i2c_4.14.167-1_mipsel_24kc.ipk
Size: 2031
SHA256sum: 0a89c0d6c3c05051a201a3e6d04083c948453225ab43de706bb68abecfa96c99
Description:  This driver adds support for Bosch Sensortec's digital pressure and
 temperature sensor connected via I2C.

Package: kmod-iio-bmp280-spi
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-iio-bmp280, kmod-spi-bitbang
Source: package/kernel/linux
SourceName: kmod-iio-bmp280-spi
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1373
Filename: kmod-iio-bmp280-spi_4.14.167-1_mipsel_24kc.ipk
Size: 2191
SHA256sum: 2c4ffd48050d0ac1bcf3a1601125f7d287483b0173e06840bc3f36d75fe5fa25
Description:  This driver adds support for Bosch Sensortec's digital pressure and
 temperature sensor connected via SPI.

Package: kmod-iio-bmp280
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-iio-core, kmod-regmap-core
Source: package/kernel/linux
SourceName: kmod-iio-bmp280
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5969
Filename: kmod-iio-bmp280_4.14.167-1_mipsel_24kc.ipk
Size: 6802
SHA256sum: b8654dee119e48ca7c167244675691fae76da5e302d6ba0aa9065a1c8b2696bd
Description:  This driver adds support for Bosch Sensortec BMP180 and BMP280 pressure and
 temperature sensors. Also supports the BME280 with an additional humidity
 sensor channel.

Package: kmod-iio-ccs811
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core, kmod-iio-core
Source: package/kernel/linux
SourceName: kmod-iio-ccs811
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2384
Filename: kmod-iio-ccs811_4.14.167-1_mipsel_24kc.ipk
Size: 3143
SHA256sum: c6fec60680df548836352f2aa7c3aac5ecdd0b4b947256867374839c34a14a05
Description:  Support for the AMS CCS811 VOC (Volatile Organic Compounds) sensor

Package: kmod-iio-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-iio-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 29352
Filename: kmod-iio-core_4.14.167-1_mipsel_24kc.ipk
Size: 30098
SHA256sum: d832dd167985478624a7fccbe9fb9a1c3001a62fc8f9dfe402e24b30a6d77c0b
Description:  The industrial I/O subsystem provides a unified framework for
 drivers for many different types of embedded sensors using a
 number of different physical interfaces (i2c, spi, etc)

Package: kmod-iio-dht11
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-iio-core
Source: package/kernel/linux
SourceName: kmod-iio-dht11
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2876
Filename: kmod-iio-dht11_4.14.167-1_mipsel_24kc.ipk
Size: 3685
SHA256sum: cca732b6359097ba0631d0db278f19fae59595bf2679d597ed6f882aef86d95f
Description:  support for DHT11 and DHT22 digitial humidity and temperature sensors
 attached at GPIO lines. You will need a custom device tree file to
 specify the GPIO line to use.

Package: kmod-iio-hmc5843
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core, kmod-iio-core, kmod-regmap-i2c
Source: package/kernel/linux
SourceName: kmod-iio-hmc5843
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3952
Filename: kmod-iio-hmc5843_4.14.167-1_mipsel_24kc.ipk
Size: 4744
SHA256sum: b18dc0edfb11c6f46b0514a53618490ea39320dd86758e384dccc446ced0fc1a
Description:  Honeywell HMC5843/5883/5883L 3-Axis Magnetometer

Package: kmod-iio-htu21
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core, kmod-iio-core
Source: package/kernel/linux
SourceName: kmod-iio-htu21
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5391
Filename: kmod-iio-htu21_4.14.167-1_mipsel_24kc.ipk
Size: 6231
SHA256sum: 126d6aa7d474aaa64aaece47b15398c5b31cb40e701df8495a56ae7abc5271ed
Description:  support for the Measurement Specialties HTU21 humidity and
 temperature sensor.
 This driver is also used for MS8607 temperature, pressure & humidity
 sensor

Package: kmod-iio-si7020
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core, kmod-iio-core
Source: package/kernel/linux
SourceName: kmod-iio-si7020
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1318
Filename: kmod-iio-si7020_4.14.167-1_mipsel_24kc.ipk
Size: 2179
SHA256sum: 79740f54f62fb1c289895de94d28fd131c5d091abf8604b1487f53567a775ce0
Description:  Support for Silicon Labs Si7020 family of relative humidity and
 temperature sensors connected via I2C. Following models are usable:
 Si7013, Si7020, Si7021, Hoperf TH06.

Package: kmod-iio-tsl4531
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core, kmod-iio-core
Source: package/kernel/linux
SourceName: kmod-iio-tsl4531
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1719
Filename: kmod-iio-tsl4531_4.14.167-1_mipsel_24kc.ipk
Size: 2557
SHA256sum: 46f21c638ae214bcd75f48ac750acc461111c1d1f5f2c2326316681154a89971
Description:  Support for TAOS TSL4531x family of ambient light sensors
 connected via I2C. Following models are usable:
 TSL45311, TSL45313, TSL45315, TSL45317.

Package: kmod-ikconfig
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-ikconfig
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 32033
Filename: kmod-ikconfig_4.14.167-1_mipsel_24kc.ipk
Size: 32849
SHA256sum: b63adce9065cd274189bf4f7fb94e3b41173d7d2192a3f7773bb2fca3d3f3d09
Description:  Kernel configuration via /proc/config.gz

Package: kmod-input-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-input-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 17252
Filename: kmod-input-core_4.14.167-1_mipsel_24kc.ipk
Size: 17914
SHA256sum: a0b80e79239b7b25a71280f2f9fcdfee8ce560acc1d873f9e566872d49bf125b
Description:  Kernel modules for support of input device

Package: kmod-input-evdev
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-input-core
Source: package/kernel/linux
SourceName: kmod-input-evdev
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7559
Filename: kmod-input-evdev_4.14.167-1_mipsel_24kc.ipk
Size: 8303
SHA256sum: 8d628a608144457cadb4bfea0b61d20ee19651296eedbe1cc37cd451d75846b7
Description:  Kernel modules for support of input device events

Package: kmod-input-gpio-encoder
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-input-core
Source: package/kernel/linux
SourceName: kmod-input-gpio-encoder
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2903
Filename: kmod-input-gpio-encoder_4.14.167-1_mipsel_24kc.ipk
Size: 3625
SHA256sum: 2edab75c93c46df851ce8f67cc20983566bd05f07aedffae953842377122329b
Description:  GPIO rotary encoder

Package: kmod-input-gpio-keys-polled
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-input-polldev
Source: package/kernel/linux
SourceName: kmod-input-gpio-keys-polled
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3603
Filename: kmod-input-gpio-keys-polled_4.14.167-1_mipsel_24kc.ipk
Size: 4445
SHA256sum: 2557daa1b75441c9d5fa9787bb2599beb5166dd87a542f58c431dd669852f82a
Description:  Kernel module for support polled GPIO keys input device
 
 See also gpio-button-hotplug which is an alternative, lower overhead
 implementation that generates uevents instead of kernel input events.

Package: kmod-input-gpio-keys
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-input-core
Source: package/kernel/linux
SourceName: kmod-input-gpio-keys
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5342
Filename: kmod-input-gpio-keys_4.14.167-1_mipsel_24kc.ipk
Size: 6223
SHA256sum: 68917b50d7371f08a38212948811c8428f298eea55008ed49614afef8a9a9026
Description:  This driver implements support for buttons connected
 to GPIO pins of various CPUs (and some other chips).
 
 See also gpio-button-hotplug which is an alternative, lower overhead
 implementation that generates uevents instead of kernel input events.

Package: kmod-input-joydev
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-input-core
Source: package/kernel/linux
SourceName: kmod-input-joydev
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5699
Filename: kmod-input-joydev_4.14.167-1_mipsel_24kc.ipk
Size: 6456
SHA256sum: 39fcd418afc9590f1109651aafd94a994bfe1efd0aa8c52065204931c086d9a5
Description:  Kernel module for joystick support

Package: kmod-input-matrixkmap
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-input-core
Source: package/kernel/linux
SourceName: kmod-input-matrixkmap
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2162
Filename: kmod-input-matrixkmap_4.14.167-1_mipsel_24kc.ipk
Size: 2927
SHA256sum: abbbfb2f79674a89ead5b9872e77595b6e739190ea6d08c0e0d94fa3144848d2
Description:  Input matrix devices support

Package: kmod-input-polldev
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-input-core
Source: package/kernel/linux
SourceName: kmod-input-polldev
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2184
Filename: kmod-input-polldev_4.14.167-1_mipsel_24kc.ipk
Size: 2954
SHA256sum: 62022cd59d2142bc84892bee935d71f51951e5987e98b54fc156ca353b1a3057
Description:  Kernel module for support of polled input devices

Package: kmod-input-touchscreen-ads7846
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-input-core, kmod-spi-bitbang
Source: package/kernel/linux
SourceName: kmod-input-touchscreen-ads7846
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7570
Filename: kmod-input-touchscreen-ads7846_4.14.167-1_mipsel_24kc.ipk
Size: 8340
SHA256sum: 94bac124d1c7f12088a73498f57b07e0c5ed2a6dfde3487e7733bbc8872bac0f
Description:  Kernel module for ADS7846/TSC2046/AD7873 and AD(S)7843 based touchscreens

Package: kmod-input-uinput
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-input-core
Source: package/kernel/linux
SourceName: kmod-input-uinput
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5766
Filename: kmod-input-uinput_4.14.167-1_mipsel_24kc.ipk
Size: 6493
SHA256sum: 549ed3ffc6ce9c320d797db2d061860466f81f6c4015919fe1e8a665d1bb3237
Description:  user input modules needed for bluez

Package: kmod-ip-vti
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-iptunnel, kmod-iptunnel4, kmod-ipsec4
Source: package/kernel/linux
SourceName: kmod-ip-vti
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4977
Filename: kmod-ip-vti_4.14.167-1_mipsel_24kc.ipk
Size: 5722
SHA256sum: 1032e8d8d07c4722eb0e304481d9a345813ca1a25c8e3f4178f70da5befdf022
Description:  Kernel modules for IP VTI (Virtual Tunnel Interface)

Package: kmod-ip6-tunnel
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-iptunnel6
Source: package/kernel/linux
SourceName: kmod-ip6-tunnel
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 15710
Filename: kmod-ip6-tunnel_4.14.167-1_mipsel_24kc.ipk
Size: 16426
SHA256sum: 8385f49438a31f07dff17f864d93bdb710d27746fd84f975499207debf7d2ce1
Description:  Kernel modules for IPv6-in-IPv6 and IPv4-in-IPv6 tunnelling

Package: kmod-ip6-vti
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-iptunnel, kmod-ip6-tunnel, kmod-ipsec6
Source: package/kernel/linux
SourceName: kmod-ip6-vti
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7150
Filename: kmod-ip6-vti_4.14.167-1_mipsel_24kc.ipk
Size: 7955
SHA256sum: 066aba2f2cdfeb3926c1f5be41153ba23e341ea774fa4f8c9e74a89ac9795a90
Description:  Kernel modules for IPv6 VTI (Virtual Tunnel Interface)

Package: kmod-ip6tables-extra
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ip6tables
Source: package/kernel/linux
SourceName: kmod-ip6tables-extra
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4310
Filename: kmod-ip6tables-extra_4.14.167-1_mipsel_24kc.ipk
Size: 5033
SHA256sum: 932c80c41257d3866fd49c49df838428a771cd558935305a3f1beaced8f22bda
Description:  Netfilter IPv6 extra header matching modules

Package: kmod-ip6tables
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nf-reject6, kmod-nf-ipt6, kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-ip6tables
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6665
Filename: kmod-ip6tables_4.14.167-1_mipsel_24kc.ipk
Size: 7458
SHA256sum: a9a09e8d48c5fcb9a1de49cfe4fed3febd6efb6d1f59c1cd1ddfa082d03ffac6
Description:  Netfilter IPv6 firewalling support

Package: kmod-ipip
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-iptunnel, kmod-iptunnel4
Source: package/kernel/linux
SourceName: kmod-ipip
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4196
Filename: kmod-ipip_4.14.167-1_mipsel_24kc.ipk
Size: 4937
SHA256sum: 2648828364871a8a6e02de62d244d61d3d923684368f700bea117f207021baa6
Description:  Kernel modules for IP-in-IP encapsulation

Package: kmod-ipoa
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-atm
Source: package/kernel/linux
SourceName: kmod-ipoa
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6765
Filename: kmod-ipoa_4.14.167-1_mipsel_24kc.ipk
Size: 7575
SHA256sum: f8b9822c89276496d1c2e3ef73f4fd249ee4a899c97131ebea0d4f2b8823af5b
Description:  Kernel modules for IPoA (IP over ATM) support

Package: kmod-ipsec4
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipsec, kmod-iptunnel4
Source: package/kernel/linux
SourceName: kmod-ipsec4
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 14699
Filename: kmod-ipsec4_4.14.167-1_mipsel_24kc.ipk
Size: 15490
SHA256sum: beb135135273f3e99bfa36a3636b872bcea0c7bb55c862ef8637ac201af72e9b
Description:  Kernel modules for IPsec support in IPv4.
 Includes:
 - ah4
 - esp4
 - ipcomp4
 - xfrm4_mode_beet
 - xfrm4_mode_transport
 - xfrm4_mode_tunnel
 - xfrm4_tunnel

Package: kmod-ipsec6
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipsec, kmod-iptunnel6
Source: package/kernel/linux
SourceName: kmod-ipsec6
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 15723
Filename: kmod-ipsec6_4.14.167-1_mipsel_24kc.ipk
Size: 16493
SHA256sum: 0aed85440bec8c60b7f7ef0af01abf04fa25929b168415890d223a4d182d8c25
Description:  Kernel modules for IPsec support in IPv6.
 Includes:
 - ah6
 - esp6
 - ipcomp6
 - xfrm6_mode_beet
 - xfrm6_mode_transport
 - xfrm6_mode_tunnel
 - xfrm6_tunnel

Package: kmod-ipsec
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-authenc, kmod-crypto-cbc, kmod-crypto-deflate, kmod-crypto-des, kmod-crypto-echainiv, kmod-crypto-hmac, kmod-crypto-iv, kmod-crypto-md5, kmod-crypto-sha1
Source: package/kernel/linux
SourceName: kmod-ipsec
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 34776
Filename: kmod-ipsec_4.14.167-1_mipsel_24kc.ipk
Size: 35634
SHA256sum: f4bc4aff06aa935e8f40dd3d3a52acfbb31262cd2f60a7dec52d047c2025b9d3
Description:  Kernel modules for IPsec support in both IPv4 and IPv6.
 Includes:
 - af_key
 - xfrm_algo
 - xfrm_ipcomp
 - xfrm_user

Package: kmod-ipt-account
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-compat-xtables
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-account
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 7563
Filename: kmod-ipt-account_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 8354
SHA256sum: b007712c7a9deb6dbb55bded4463685151ecd21deed6915ef17a56427d4127d2
Description:  ACCOUNT netfilter module

Package: kmod-ipt-chaos
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-compat-xtables, kmod-ipt-delude, kmod-ipt-tarpit
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-chaos
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 2248
Filename: kmod-ipt-chaos_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 3035
SHA256sum: d4b26f5df128e650f74e1f116553a6b42551d70915bb67550212b768964c9ed8
Description:  CHAOS netfilter module

Package: kmod-ipt-checksum
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-ipt-checksum
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1012
Filename: kmod-ipt-checksum_4.14.167-1_mipsel_24kc.ipk
Size: 1775
SHA256sum: 42ed9d49d0e883886bf0acc5dfccac65763fb2f6032d03a8ad4a480e35f7804a
Description:  Kernel modules for CHECKSUM fillin target

Package: kmod-ipt-cluster
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-nf-conntrack
Source: package/kernel/linux
SourceName: kmod-ipt-cluster
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1686
Filename: kmod-ipt-cluster_4.14.167-1_mipsel_24kc.ipk
Size: 2759
SHA256sum: 0c501714d69265de00ce13dd03b4178521cb37c96a4b543689d039d7cd8a6745
Description:  Netfilter (IPv4/IPv6) module for matching cluster
 This option allows you to build work-load-sharing clusters of
 network servers/stateful firewalls without having a dedicated
 load-balancing router/server/switch. Basically, this match returns
 true when the packet must be handled by this cluster node. Thus,
 all nodes see all packets and this match decides which node handles
 what packets. The work-load sharing algorithm is based on source
 address hashing.
 
 This module is usable for ipv4 and ipv6.
 
 To use it also enable iptables-mod-cluster
 
 see `iptables -m cluster --help` for more information.

Package: kmod-ipt-clusterip
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-nf-conntrack
Source: package/kernel/linux
SourceName: kmod-ipt-clusterip
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5887
Filename: kmod-ipt-clusterip_4.14.167-1_mipsel_24kc.ipk
Size: 6796
SHA256sum: 573ffe506b05c14050116d258c65278600e31f5bc342a8a0cca068fa3b42a8b0
Description:  Netfilter (IPv4-only) module for CLUSTERIP
 The CLUSTERIP target allows you to build load-balancing clusters of
 network servers without having a dedicated load-balancing
 router/server/switch.
 
 To use it also enable iptables-mod-clusterip
 
 see `iptables -j CLUSTERIP --help` for more information.

Package: kmod-ipt-compat-xtables
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ip6tables
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-compat-xtables
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 776
Filename: kmod-ipt-compat-xtables_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 1590
SHA256sum: a5819ad35a94e6e9ec88d469f0fa5c305f431ede57a36d17af46961e2b0d1d17
Description:  API compatibilty layer netfilter module

Package: kmod-ipt-condition
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-condition
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 2828
Filename: kmod-ipt-condition_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 3594
SHA256sum: e75a283163c231d1f8e6b1821676bae8569d4d63b54ff99b3a1883493f703ea8
Description:  Condition netfilter module

Package: kmod-ipt-conntrack-extra
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-conntrack
Source: package/kernel/linux
SourceName: kmod-ipt-conntrack-extra
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 12275
Filename: kmod-ipt-conntrack-extra_4.14.167-1_mipsel_24kc.ipk
Size: 13083
SHA256sum: aa208ae01fb0e30a5da8e97423f82571969464856b53a1ced43895f1c6189710
Description:  Netfilter (IPv4) extra kernel modules for connection tracking
 Includes:
 - connbytes
 - connmark/CONNMARK
 - conntrack
 - helper
 - recent

Package: kmod-ipt-conntrack-label
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-conntrack
Source: package/kernel/linux
SourceName: kmod-ipt-conntrack-label
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1361
Filename: kmod-ipt-conntrack-label_4.14.167-1_mipsel_24kc.ipk
Size: 2160
SHA256sum: d069a44b111e8bc5d5748daa2e497c11482b0e9a0e65e674d240c772e119fb38
Description:  Netfilter (IPv4) module for handling connection tracking labels
 Includes:
 - connlabel

Package: kmod-ipt-conntrack
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-nf-conntrack
Source: package/kernel/linux
SourceName: kmod-ipt-conntrack
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4256
Filename: kmod-ipt-conntrack_4.14.167-1_mipsel_24kc.ipk
Size: 5066
SHA256sum: ab62ce1952e10eae2d7c79e8be381c58bc9d7f540a4ffabb4fc8fe7cdb334f53
Description:  Netfilter (IPv4) kernel modules for connection tracking
 Includes:
 - conntrack
 - defrag
 - iptables_raw
 - NOTRACK
 - state

Package: kmod-ipt-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nf-reject, kmod-nf-ipt
Source: package/kernel/linux
SourceName: kmod-ipt-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 15336
Filename: kmod-ipt-core_4.14.167-1_mipsel_24kc.ipk
Size: 16091
SHA256sum: 34481fbc4344b64e4c9915f72742df8bed185e798115acec7ac060d061c7b778
Description:  Netfilter core kernel modules
 Includes:
 - comment
 - limit
 - LOG
 - mac
 - multiport
 - REJECT
 - TCPMSS

Package: kmod-ipt-debug
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-raw, kmod-ipt-raw6
Source: package/kernel/linux
SourceName: kmod-ipt-debug
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 870
Filename: kmod-ipt-debug_4.14.167-1_mipsel_24kc.ipk
Size: 1662
SHA256sum: bdbb078bdc8fd6223139f96e8eec253a481728a0e1397ce899997b153a1e2bc0
Description:  Netfilter modules for debugging/development of the firewall
 Includes:
 - TRACE

Package: kmod-ipt-delude
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-compat-xtables
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-delude
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 1894
Filename: kmod-ipt-delude_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 2694
SHA256sum: 2f3816ccc3b994fad270d52ad7524e5219d690810a41ed1861714f45320b14ef
Description:  DELUDE netfilter module

Package: kmod-ipt-dhcpmac
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-compat-xtables
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-dhcpmac
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 1664
Filename: kmod-ipt-dhcpmac_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 2482
SHA256sum: 9fe28cdc0b440e19ecb67f5c29ab57167c92c8468dbf7bcfb4b72b83fb54108d
Description:  DHCPMAC netfilter module

Package: kmod-ipt-dnetmap
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-compat-xtables, kmod-ipt-nat
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-dnetmap
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 7811
Filename: kmod-ipt-dnetmap_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 8604
SHA256sum: acbab1f3bb73d75b6be86e8b5e3540543a32f032b6633e016660d7932a6cbc60
Description:  DNETMAP netfilter module

Package: kmod-ipt-extra
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-ipt-extra
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3616
Filename: kmod-ipt-extra_4.14.167-1_mipsel_24kc.ipk
Size: 4408
SHA256sum: c7d88a8f0f5146923d73f0b17a176acb8c5c3b7cee73b20201945b212035fb6a
Description:  Other Netfilter (IPv4) kernel modules
 Includes:
 - addrtype
 - owner
 - pkttype
 - quota

Package: kmod-ipt-filter
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-lib-textsearch, kmod-ipt-conntrack
Source: package/kernel/linux
SourceName: kmod-ipt-filter
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2140
Filename: kmod-ipt-filter_4.14.167-1_mipsel_24kc.ipk
Size: 2917
SHA256sum: 2b8cb1ea0389c5c9d0aa1120e55dbfb2817857e287ed82282aacb96d5c48d7ec
Description:  Netfilter (IPv4) kernel modules for packet content inspection
 Includes:
 - string
 - bpf

Package: kmod-ipt-fuzzy
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-fuzzy
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 1265
Filename: kmod-ipt-fuzzy_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 2073
SHA256sum: 59d8a7ed20adec513c4a8ffa51ea967057a74103a57959318ad5ba0db413696e
Description:  fuzzy netfilter module

Package: kmod-ipt-geoip
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-geoip
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 2871
Filename: kmod-ipt-geoip_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 3644
SHA256sum: a64ab70cabb47abccb5af4a65bec418d0b313fd0079d28e3dfea91a249407031
Description:  geoip netfilter module

Package: kmod-ipt-hashlimit
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-ipt-hashlimit
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7624
Filename: kmod-ipt-hashlimit_4.14.167-1_mipsel_24kc.ipk
Size: 8401
SHA256sum: f619e559a5fe64bf6c315a7e9eae4a23cdfef369c4bb61ab94d532ad69ebe6c2
Description:  Kernel modules support for the hashlimit bucket match module

Package: kmod-ipt-iface
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-iface
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 1095
Filename: kmod-ipt-iface_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 1897
SHA256sum: df236bedf46b2edaf1a29fdbca0a812e5600807a5e44adec48657170094ada97
Description:  iface netfilter module

Package: kmod-ipt-ipmark
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-compat-xtables
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-ipmark
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 1050
Filename: kmod-ipt-ipmark_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 1857
SHA256sum: 016a315d24cfd316894f5b4e4c12ed51bc369c439ff24cf51e1adcdf5f08a4a2
Description:  IPMARK netfilter module

Package: kmod-ipt-ipopt
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-ipt-ipopt
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6103
Filename: kmod-ipt-ipopt_4.14.167-1_mipsel_24kc.ipk
Size: 6947
SHA256sum: 2eaf35f49f6b6900ccd1580d5e5eaa8dd74f44177fd424a081634c9da5dacd1d
Description:  Netfilter (IPv4) modules for matching/changing IP packet options
 Includes:
 - CLASSIFY
 - dscp/DSCP
 - ecn/ECN
 - hl/HL
 - length
 - mark/MARK
 - statistic
 - tcpmss
 - time
 - ttl/TTL
 - unclean

Package: kmod-ipt-ipp2p
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-compat-xtables
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-ipp2p
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 5261
Filename: kmod-ipt-ipp2p_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 6049
SHA256sum: c86375a2d1266237ba36fbbca05c7ed480441c33814adbeb56422180448f083f
Description:  IPP2P netfilter module

Package: kmod-ipt-iprange
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-ipt-iprange
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1149
Filename: kmod-ipt-iprange_4.14.167-1_mipsel_24kc.ipk
Size: 1927
SHA256sum: 4628fc098b94653a8e04d19e696414621a39c196e238b9551595166a6080f4af
Description:  Netfilter (IPv4) module for matching ip ranges
 Includes:
 - iprange

Package: kmod-ipt-ipsec
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-ipt-ipsec
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2588
Filename: kmod-ipt-ipsec_4.14.167-1_mipsel_24kc.ipk
Size: 3368
SHA256sum: ce8a0f1c327c00fed5042f82210621d2947a15b1c70ebf583fa1cb6120e05191
Description:  Netfilter (IPv4) modules for matching IPSec packets
 Includes:
 - ah
 - esp
 - policy

Package: kmod-ipt-ipset
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-nfnetlink
Source: package/kernel/linux
SourceName: kmod-ipt-ipset
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 120697
Filename: kmod-ipt-ipset_4.14.167-1_mipsel_24kc.ipk
Size: 121183
SHA256sum: fcbb54224e1d333a2e3ab9309317972596f0b53cbe7d24c95351632fa4744388
Description:  IPset netfilter modules

Package: kmod-ipt-ipv4options
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-ipv4options
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 912
Filename: kmod-ipt-ipv4options_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 1712
SHA256sum: 4667e8e6bff59212fff42f4406760c583e02a77d13cdbfe05fbbde1b92997ad9
Description:  ipv4options netfilter module

Package: kmod-ipt-led
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-ipt-led
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1761
Filename: kmod-ipt-led_4.14.167-1_mipsel_24kc.ipk
Size: 2537
SHA256sum: d61e18f4fa8575faf0727e60e6f1f2b98773335de586febc738f12cdfe6547a9
Description:  Netfilter target to trigger a LED when a network packet is matched.

Package: kmod-ipt-length2
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-compat-xtables
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-length2
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 2053
Filename: kmod-ipt-length2_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 2860
SHA256sum: aa98f0dbd3c3a2d0fe477bc8720fe002a53b44f112b383914057d30c4985ee4a
Description:  length2 netfilter module

Package: kmod-ipt-logmark
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-compat-xtables
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-logmark
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 1915
Filename: kmod-ipt-logmark_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 2738
SHA256sum: 2a4609d99a45182b22b51cb65bffca123fc2fe4ea496247e3dba8831bedabf55
Description:  LOGMARK netfilter module

Package: kmod-ipt-lscan
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-lscan
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 2128
Filename: kmod-ipt-lscan_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 2893
SHA256sum: 4f376b9778ca7968c9c959e985a39bd82a1c20133e88d7e5e4711efc7df8f171
Description:  lscan netfilter module

Package: kmod-ipt-lua
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-conntrack-extra
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-lua
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 70393
Filename: kmod-ipt-lua_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 70788
SHA256sum: 0e2db0460c1e72b22e0776585a176eb9fa9dd1780340c7ff60ae5b2ea61fed3d
Description:  Lua PacketScript netfilter module

Package: kmod-ipt-nat-extra
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-nat
Source: package/kernel/linux
SourceName: kmod-ipt-nat-extra
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1665
Filename: kmod-ipt-nat-extra_4.14.167-1_mipsel_24kc.ipk
Size: 2474
SHA256sum: 475c9a8d120ec6c3a58e7c6c31e5ba83cca0270063e9cb3f1ddf3eacdd69ae04
Description:  Netfilter (IPv4) kernel modules for extra NAT targets
 Includes:
 - NETMAP
 - REDIRECT

Package: kmod-ipt-nat6
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-nf-nat6, kmod-ipt-core, kmod-ipt-conntrack, kmod-ipt-core, kmod-ipt-nat, kmod-ipt-core, kmod-ip6tables
Source: package/kernel/linux
SourceName: kmod-ipt-nat6
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2834
Filename: kmod-ipt-nat6_4.14.167-1_mipsel_24kc.ipk
Size: 3619
SHA256sum: 3e9def14b88c4f30bb045fd69ceb3f1bf01e541058a58ad7af523b9ab44e6490
Description:  Netfilter (IPv6) kernel modules for NAT targets

Package: kmod-ipt-nat
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-nf-nat
Source: package/kernel/linux
SourceName: kmod-ipt-nat
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3231
Filename: kmod-ipt-nat_4.14.167-1_mipsel_24kc.ipk
Size: 4026
SHA256sum: 56527737261f9191777f6c8990cd1c8e76e53c2a489dc6df71f67180ae4a443a
Description:  Netfilter (IPv4) kernel modules for basic NAT targets
 Includes:
 - MASQUERADE

Package: kmod-ipt-nathelper-rtsp
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-conntrack-extra, kmod-ipt-nat
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-nathelper-rtsp
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 9166
Filename: kmod-ipt-nathelper-rtsp_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 9959
SHA256sum: e89a6d83e6aff2af324f2b2ee2c921985b683c6281a433c9a44741b26b513356
Description:  RTSP Conntrack and NAT netfilter module

Package: kmod-ipt-nflog
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-nfnetlink-log
Source: package/kernel/linux
SourceName: kmod-ipt-nflog
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 951
Filename: kmod-ipt-nflog_4.14.167-1_mipsel_24kc.ipk
Size: 1738
SHA256sum: a5a23ac7594b2709bd0794fb9ef80081d50fa6b3639b611c3835d41749fda6b8
Description:  Netfilter module for user-space packet logging
 Includes:
 - NFLOG

Package: kmod-ipt-nfqueue
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-nfnetlink-queue
Source: package/kernel/linux
SourceName: kmod-ipt-nfqueue
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2750
Filename: kmod-ipt-nfqueue_4.14.167-1_mipsel_24kc.ipk
Size: 3516
SHA256sum: 3b9a42f505707f7408ab11b5b46ae3818ed9fa5ab4574ac60d32e7b9e043eb35
Description:  Netfilter module for user-space packet queuing
 Includes:
 - NFQUEUE

Package: kmod-ipt-offload
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-nf-flow
Source: package/kernel/linux
SourceName: kmod-ipt-offload
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3174
Filename: kmod-ipt-offload_4.14.167-1_mipsel_24kc.ipk
Size: 3903
SHA256sum: 97e35621d9c0cefeb8b557899ca7b8aec6da27061a407e54017af1ecbbb84497
Description:  Netfilter routing/NAT offload support

Package: kmod-ipt-physdev
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-br-netfilter
Source: package/kernel/linux
SourceName: kmod-ipt-physdev
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1508
Filename: kmod-ipt-physdev_4.14.167-1_mipsel_24kc.ipk
Size: 2285
SHA256sum: eef72a8d87d562419c8fe0b69ddca7b1dbc5c27502ac966c354bdd10da336c89
Description:  The iptables physdev kernel module

Package: kmod-ipt-psd
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-psd
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 2785
Filename: kmod-ipt-psd_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 3543
SHA256sum: 3b2187ddb2f8aa357b56fa4e3d75d93cbf8b7a254ff1b2630561c2dbf9907f77
Description:  psd netfilter module

Package: kmod-ipt-quota2
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-quota2
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 3262
Filename: kmod-ipt-quota2_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 4030
SHA256sum: b8df1cfa89a706a1f0c3c6f6cc1ede84aa9eea38107277d8daf403e47b50491f
Description:  quota2 netfilter module

Package: kmod-ipt-raw6
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ip6tables
Source: package/kernel/linux
SourceName: kmod-ipt-raw6
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1287
Filename: kmod-ipt-raw6_4.14.167-1_mipsel_24kc.ipk
Size: 2055
SHA256sum: 8f9b6156388765d244b7feb7642cdbe38fffe079cf791a225ba1144f36b1931f
Description:  Netfilter IPv6 raw table support

Package: kmod-ipt-raw
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-ipt-raw
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1277
Filename: kmod-ipt-raw_4.14.167-1_mipsel_24kc.ipk
Size: 2043
SHA256sum: cea5d17f3f37270040249d20b346db27a4934ace0e3854065a84be6ce2ee06bc
Description:  Netfilter IPv4 raw table support

Package: kmod-ipt-rpfilter
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-ipt-rpfilter
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2357
Filename: kmod-ipt-rpfilter_4.14.167-1_mipsel_24kc.ipk
Size: 3102
SHA256sum: 2326c2ad1c2f66426023efbdc94b39c971cb7cbded4ea3a7c2cdcef803c2b3da
Description:  Kernel modules support for the Netfilter rpfilter match

Package: kmod-ipt-sysrq
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-compat-xtables, kmod-crypto-hash
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-sysrq
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 3795
Filename: kmod-ipt-sysrq_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 4584
SHA256sum: 5f88a3a33f445ceaccde3ac48cfeec30ad24405c283c0957a1dbbf2e50cb79dd
Description:  SYSRQ netfilter module

Package: kmod-ipt-tarpit
Version: 4.14.167+2.14-8
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core, kmod-ipt-compat-xtables
Source: feeds/packages/net/xtables-addons
SourceName: kmod-ipt-tarpit
License: GPL-2.0
Section: kernel
Maintainer: Jo-Philipp Wich <jo@mein.io>
Architecture: mipsel_24kc
Installed-Size: 3551
Filename: kmod-ipt-tarpit_4.14.167+2.14-8_mipsel_24kc.ipk
Size: 4330
SHA256sum: e3be33c954df48bc1c01c274b82ec3d38e5f4f06a48410c38ff219c0341263c8
Description:  TARPIT netfilter module

Package: kmod-ipt-tee
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-conntrack, kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-ipt-tee
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3020
Filename: kmod-ipt-tee_4.14.167-1_mipsel_24kc.ipk
Size: 3753
SHA256sum: e62392faa478d2f9f884a309bb5a697593995090010bef182211d3efbc4ebdd4
Description:  Kernel modules for TEE

Package: kmod-ipt-tproxy
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-conntrack, kmod-nf-conntrack6, kmod-ip6tables, kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-ipt-tproxy
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6361
Filename: kmod-ipt-tproxy_4.14.167-1_mipsel_24kc.ipk
Size: 7168
SHA256sum: 2485e18fcd0f460b7594833fbb35ba1dd135b60ea354b6a3a3f4fdbb56bfed8a
Description:  Kernel modules for Transparent Proxying

Package: kmod-ipt-u32
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-ipt-u32
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1210
Filename: kmod-ipt-u32_4.14.167-1_mipsel_24kc.ipk
Size: 1954
SHA256sum: b9f5d23fa490a73cf9919dbfc5281918128446e43e3aa238c96ee2413fc3604f
Description:  Kernel modules for U32

Package: kmod-ipt-ulog
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-core
Source: package/kernel/linux
SourceName: kmod-ipt-ulog
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-ipt-ulog_4.14.167-1_mipsel_24kc.ipk
Size: 868
SHA256sum: 73965a5cb237482654b47d90b8c4617905ea9708e62c33c5fdfe1ebf10a375d8
Description:  Netfilter (IPv4) module for user-space packet logging
 Includes:
 - ULOG

Package: kmod-iptunnel4
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-iptunnel4
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1990
Filename: kmod-iptunnel4_4.14.167-1_mipsel_24kc.ipk
Size: 2712
SHA256sum: e2a83a175f93c06b4df46116f41919bf0b5c2c08f18a4d615d1f5efd349a7d6d
Description:  Kernel modules for IPv4 tunneling

Package: kmod-iptunnel6
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-iptunnel6
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1840
Filename: kmod-iptunnel6_4.14.167-1_mipsel_24kc.ipk
Size: 2593
SHA256sum: f76b185c84824f17972e7cfa3669106066bbaafeb18b68cd8e784f40c071973f
Description:  Kernel modules for IPv6 tunneling

Package: kmod-iptunnel
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-iptunnel
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 8383
Filename: kmod-iptunnel_4.14.167-1_mipsel_24kc.ipk
Size: 9122
SHA256sum: 25621945a470a8bb11dfe30ba65082c86212e6521f561855cc51b8d65de96c0a
Description:  Kernel module for generic IP tunnel support

Package: kmod-ipw2100
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-libipw
Source: package/kernel/mac80211
SourceName: kmod-ipw2100
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 280450
Filename: kmod-ipw2100_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 277460
SHA256sum: 0ecc7702054b58592c7fc97204e26b7b8edef1faf85d8e0d964069c27054f1e8
Description:  Kernel support for Intel IPW2100
 Includes:
 - ipw2100

Package: kmod-ipw2200
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-libipw
Source: package/kernel/mac80211
SourceName: kmod-ipw2200
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 323370
Filename: kmod-ipw2200_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 323509
SHA256sum: ae2a0db0d20c92e620be7b2fa2088cf81c991019321572b1c282c88d67d1193c
Description:  Kernel support for Intel IPW2200
 Includes:
 - ipw2200

Package: kmod-isdn4linux
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ppp
Source: package/kernel/linux
SourceName: kmod-isdn4linux
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 89373
Filename: kmod-isdn4linux_4.14.167-1_mipsel_24kc.ipk
Size: 89545
SHA256sum: 0605b12ee89bf6d42a703008ff4c388c55ab52936cd72adb7cff4880f3627047
Description:  This driver allows you to use an ISDN adapter for networking

Package: kmod-it87-wdt
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-it87-wdt
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-it87-wdt_4.14.167-1_mipsel_24kc.ipk
Size: 840
SHA256sum: 6abf5e63d58b32d8262699f07e43b337b3bf6f232ac5f60b0e9d6887d40b35ac
Description:  Kernel module for ITE IT87 Watchdog Timer

Package: kmod-itco-wdt
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-itco-wdt
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-itco-wdt_4.14.167-1_mipsel_24kc.ipk
Size: 845
SHA256sum: 3a4158b4e75e04a0705a879395ed6cba2be166a430fbb5d9137802fff3a9ba24
Description:  Kernel module for Intel iTCO Watchdog Timer

Package: kmod-iwl-legacy
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211
Source: package/kernel/mac80211
SourceName: kmod-iwl-legacy
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 26346
Filename: kmod-iwl-legacy_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 26938
SHA256sum: 68d19846b281764e3b34358384db1dd70e255c25c2d2a4593eb4f10c65eb4131
Description:  iwl-legacy kernel module for legacy Intel wireless support

Package: kmod-iwl3945
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-iwl-legacy, iwl3945-firmware
Source: package/kernel/mac80211
SourceName: kmod-iwl3945
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 33048
Filename: kmod-iwl3945_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 33761
SHA256sum: fb79e221806be98cbef6afc7d7e21a477ecb549b2222c740e9aa6351bf34302e
Description:  iwl3945 kernel module for Intel 3945 support

Package: kmod-iwl4965
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-iwl-legacy, iwl4965-firmware
Source: package/kernel/mac80211
SourceName: kmod-iwl4965
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 54806
Filename: kmod-iwl4965_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 55412
SHA256sum: b75df01ab49c51ad7a9ebcbef607a8ff3f7abd2ba14848fa14edea8d010213ef
Description:  iwl4965 kernel module for Intel 4965 support

Package: kmod-iwlwifi
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211
Source: package/kernel/mac80211
SourceName: kmod-iwlwifi
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 293251
Filename: kmod-iwlwifi_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 292360
SHA256sum: 00cd25f6cc167ae08c92f17274dddd69a6ed28be4d0433bb525e5034ef1dea54
Description:  iwlwifi kernel module for
 Intel Wireless WiFi Link 6250AGN Adapter
 Intel 6000 Series Wi-Fi Adapters (6200AGN and 6300AGN)
 Intel WiFi Link 1000BGN
 Intel Wireless WiFi 5150AGN
 Intel Wireless WiFi 5100AGN, 5300AGN, and 5350AGN
 Intel 6005 Series Wi-Fi Adapters
 Intel 6030 Series Wi-Fi Adapters
 Intel Wireless WiFi Link 6150BGN 2 Adapter
 Intel 100 Series Wi-Fi Adapters (100BGN and 130BGN)
 Intel 2000 Series Wi-Fi Adapters
 Intel 7260 Wi-Fi Adapter
 Intel 3160 Wi-Fi Adapter
 Intel 7265 Wi-Fi Adapter
 Intel 8260 Wi-Fi Adapter
 Intel 3165 Wi-Fi Adapter

Package: kmod-ixgbe
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mdio, kmod-ptp, kmod-hwmon-core
Source: package/kernel/linux
SourceName: kmod-ixgbe
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 111554
Filename: kmod-ixgbe_4.14.167-1_mipsel_24kc.ipk
Size: 112045
SHA256sum: bea8b1c965e150bfe85a909bc5ca2e9a83f5ad796a80c596a7b21a2493590ef1
Description:  Kernel modules for Intel(R) 82598/82599 PCI-Express 10 Gigabit Ethernet adapters.

Package: kmod-ixgbevf
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ixgbe
Source: package/kernel/linux
SourceName: kmod-ixgbevf
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-ixgbevf_4.14.167-1_mipsel_24kc.ipk
Size: 855
SHA256sum: 3cbbd9d1a393933d53797aa98434d3bd1f348920e2e09af5bbcc0f83ee9952ee
Description:  Kernel modules for Intel(R) 82599 Virtual Function Ethernet adapters.

Package: kmod-jool
Version: 4.14.167+3.5.7-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-md5, kmod-nf-conntrack, kmod-nf-conntrack6
Source: feeds/packages/net/jool
SourceName: kmod-jool
License: GPL-2.0
LicenseFiles: COPYING
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 117325
Filename: kmod-jool_4.14.167+3.5.7-2_mipsel_24kc.ipk
Size: 117187
SHA256sum: d8940639e7aea1ce6f05365f0f103900f5fae0cffb131ada50a25270e4e7e0fe
Description:  Jool is an Open Source SIIT and NAT64 for Linux.
 
 This package provides the kernel module for Jool.

Package: kmod-l2tp-eth
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-l2tp
Source: package/kernel/linux
SourceName: kmod-l2tp-eth
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2741
Filename: kmod-l2tp-eth_4.14.167-1_mipsel_24kc.ipk
Size: 3480
SHA256sum: 421381a892abdb81ce3e85cf8d0efb5c2e0c3189ff448ce4ec5fc7420a9ce1c9
Description:  Kernel modules for L2TP ethernet pseudowire support for L2TPv3

Package: kmod-l2tp-ip
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-l2tp
Source: package/kernel/linux
SourceName: kmod-l2tp-ip
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9171
Filename: kmod-l2tp-ip_4.14.167-1_mipsel_24kc.ipk
Size: 9920
SHA256sum: 538ee9076562b758de9a0319f0216d3be54a6d05d9764500ea8f11b7a77a448d
Description:  Kernel modules for L2TP IP encapsulation for L2TPv3

Package: kmod-l2tp
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-udptunnel4, kmod-udptunnel6
Source: package/kernel/linux
SourceName: kmod-l2tp
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 14417
Filename: kmod-l2tp_4.14.167-1_mipsel_24kc.ipk
Size: 15158
SHA256sum: c1adaf3d9165424a18a3fc5ed3c2936171153d8f536010ea2401ff578679698b
Description:  Kernel modules for L2TP V3 Support

Package: kmod-leds-gpio
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-leds-gpio
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2713
Filename: kmod-leds-gpio_4.14.167-1_mipsel_24kc.ipk
Size: 3437
SHA256sum: 126f6283b8182945523e14d13310a44eb4c40805145df5a88dadea4220396845
Description:  Kernel module for LEDs on GPIO lines

Package: kmod-leds-pca963x
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-leds-pca963x
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3612
Filename: kmod-leds-pca963x_4.14.167-1_mipsel_24kc.ipk
Size: 4349
SHA256sum: 25343f41c1249959cebae36d06794d1a8ae1d1ea9237ef0cfd34802a72108e80
Description:  Driver for the NXP PCA963x I2C LED controllers.

Package: kmod-ledtrig-default-on
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-ledtrig-default-on
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 240
Filename: kmod-ledtrig-default-on_4.14.167-1_mipsel_24kc.ipk
Size: 989
SHA256sum: a46bb85e6f87695ba70c74ec66913ad470f355fc3f26dd0cf3c18808b95fc439
Description:  Kernel module that allows LEDs to be initialised in the ON state

Package: kmod-ledtrig-gpio
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-ledtrig-gpio
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2050
Filename: kmod-ledtrig-gpio_4.14.167-1_mipsel_24kc.ipk
Size: 2825
SHA256sum: 861701e80ba37fbac1fefb793a991d37400542001fc2d340b5cda50e50bfdc63
Description:  Kernel module that allows LEDs to be controlled by gpio events

Package: kmod-ledtrig-heartbeat
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-ledtrig-heartbeat
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1838
Filename: kmod-ledtrig-heartbeat_4.14.167-1_mipsel_24kc.ipk
Size: 2615
SHA256sum: bcf4fc45877476cfe29bcb21cd0d2f29c9914de5bf0613ec058166b2c4ea4b25
Description:  Kernel module that allows LEDs to blink like heart beat

Package: kmod-ledtrig-netdev
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-ledtrig-netdev
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 194
Filename: kmod-ledtrig-netdev_4.14.167-1_mipsel_24kc.ipk
Size: 937
SHA256sum: 1da138f0e645f5eb9b2263f5234e229529171846d7ea0723dd4d3577dfcdbe86
Description:  Kernel module to drive LEDs based on network activity

Package: kmod-ledtrig-oneshot
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-ledtrig-oneshot
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1588
Filename: kmod-ledtrig-oneshot_4.14.167-1_mipsel_24kc.ipk
Size: 2387
SHA256sum: 5cfca8f864bf2a1282919465b92ba832576971f2b199b94956d14a7ab3bc4a55
Description:  Kernel module that allows LEDs to be triggered by sporadic events in
 one-shot pulses

Package: kmod-ledtrig-timer
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-ledtrig-timer
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 234
Filename: kmod-ledtrig-timer_4.14.167-1_mipsel_24kc.ipk
Size: 991
SHA256sum: 807bb1f70aac54dc17d97d61b7f9eb5a7c99010667aec8aa32deb0731d8a980c
Description:  Kernel module that allows LEDs to be controlled by a programmable timer
 via sysfs

Package: kmod-ledtrig-transient
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-ledtrig-transient
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1919
Filename: kmod-ledtrig-transient_4.14.167-1_mipsel_24kc.ipk
Size: 2670
SHA256sum: 9a2f5e26e2413533bcfb50d7f42e4795386b00ae051b7ae2071de1d7e7016ba5
Description:  Kernel module that allows LEDs one time activation of a transient state.

Package: kmod-lib-cordic
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-lib-cordic
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 973
Filename: kmod-lib-cordic_4.14.167-1_mipsel_24kc.ipk
Size: 1725
SHA256sum: 14d8445270b6265ed9a9c14dc02714bef18de4d3b1f1ca1de253ff65393a52b4
Description:  Kernel module for Cordic function support

Package: kmod-lib-crc-ccitt
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-lib-crc-ccitt
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1300
Filename: kmod-lib-crc-ccitt_4.14.167-1_mipsel_24kc.ipk
Size: 2054
SHA256sum: 95e04906d81807c816c06383746bd9a3875170ea89f9aeed8d25a58ad1b812ca
Description:  Kernel module for CRC-CCITT support

Package: kmod-lib-crc-itu-t
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-lib-crc-itu-t
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1304
Filename: kmod-lib-crc-itu-t_4.14.167-1_mipsel_24kc.ipk
Size: 2065
SHA256sum: eb8f4600214e8815b8f3d3d7a946a8634573982636f79f59e6287a5471a6b909
Description:  Kernel module for CRC ITU-T V.41 support

Package: kmod-lib-crc16
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-lib-crc16
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1270
Filename: kmod-lib-crc16_4.14.167-1_mipsel_24kc.ipk
Size: 2034
SHA256sum: f1d032f4e143c78a426a586041a82dad90549fb281c0b8d0f062fed7da464efa
Description:  Kernel module for CRC16 support

Package: kmod-lib-crc32c
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-crc32c
Source: package/kernel/linux
SourceName: kmod-lib-crc32c
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1074
Filename: kmod-lib-crc32c_4.14.167-1_mipsel_24kc.ipk
Size: 1834
SHA256sum: bf3f5d2a30ea80eaef1d203599b020d860002966d241739d7a323e0527d93b03
Description:  Kernel module for CRC32 support

Package: kmod-lib-crc7
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-lib-crc7
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1018
Filename: kmod-lib-crc7_4.14.167-1_mipsel_24kc.ipk
Size: 1766
SHA256sum: 1d2a4a5ca537a2876fbe4bf3f6f86f6ff1110129a44a1148c581000b82b4257c
Description:  Kernel module for CRC7 support

Package: kmod-lib-crc8
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-lib-crc8
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 880
Filename: kmod-lib-crc8_4.14.167-1_mipsel_24kc.ipk
Size: 1622
SHA256sum: bb8914e84c5f890b13209b9aed3aa49ef48af25f1ec13678409d34a6f6f42870
Description:  Kernel module for CRC8 support

Package: kmod-lib-lz4
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-acompress
Source: package/kernel/linux
SourceName: kmod-lib-lz4
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 20286
Filename: kmod-lib-lz4_4.14.167-1_mipsel_24kc.ipk
Size: 21039
SHA256sum: 221d110b4cf312193300c3aa87f21f9e6e33af5f34fcd59d7c708067992254ed
Description:  Kernel module for LZ4 compression/decompression support

Package: kmod-lib-lzo
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-acompress
Source: package/kernel/linux
SourceName: kmod-lib-lzo
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3586
Filename: kmod-lib-lzo_4.14.167-1_mipsel_24kc.ipk
Size: 4335
SHA256sum: 9fad427a0f0d5b03f2c1faf14cb8cc16c6580bbaadbc8d527731c6077156d16d
Description:  Kernel module for LZO compression/decompression support

Package: kmod-lib-raid6
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-lib-raid6
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 76322
Filename: kmod-lib-raid6_4.14.167-1_mipsel_24kc.ipk
Size: 77168
SHA256sum: 5464130f4d7d986b0eb84e0b1e7dd9cecbca2e0c35ba3e68c024035592bf12fa
Description:  Kernel module for RAID6 algorithms

Package: kmod-lib-textsearch
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-lib-textsearch
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3616
Filename: kmod-lib-textsearch_4.14.167-1_mipsel_24kc.ipk
Size: 4347
SHA256sum: 641dea3f1411e59b930ce8e5926db5c921da801185ec21b3b14a282d48833148
Description:  Textsearch support

Package: kmod-lib-xor
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-lib-xor
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4559
Filename: kmod-lib-xor_4.14.167-1_mipsel_24kc.ipk
Size: 5274
SHA256sum: b95ea99a8107b9cd8dab771fd56667df2ec7a78f501f56fda122690cad630107
Description:  Kernel module for XOR blocks algorithms

Package: kmod-lib-zlib-deflate
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-lib-zlib-deflate
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10096
Filename: kmod-lib-zlib-deflate_4.14.167-1_mipsel_24kc.ipk
Size: 10826
SHA256sum: dd13451a8e1f5ccf62853b2a46205283910e6bb99841128099e7609d54493c17
Description:  Zlib support

Package: kmod-lib-zlib-inflate
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-lib-zlib-inflate
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 8178
Filename: kmod-lib-zlib-inflate_4.14.167-1_mipsel_24kc.ipk
Size: 8899
SHA256sum: 43d738dc290840dcbb93a8e49f35718926fc4c70d9124bba61015526e0162c3d
Description:  Zlib support

Package: kmod-lib-zstd
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-lib-zstd
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 106944
Filename: kmod-lib-zstd_4.14.167-1_mipsel_24kc.ipk
Size: 107401
SHA256sum: 5dc4296f153e74beec96fe4d2c7cb7863bace17d05da8e94e061eb0cd124ca95
Description:  Kernel module for ZSTD compression/decompression support

Package: kmod-lib80211
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-cfg80211, kmod-crypto-hash
Source: package/kernel/mac80211
SourceName: kmod-lib80211
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 11429
Filename: kmod-lib80211_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 12239
SHA256sum: add9284ede80d0dec22d31c00d70bfc5e01b503eca57091e77ab44f701db63c6
Description:  Kernel modules for 802.11 Networking stack
 Includes:
 - lib80211
 - lib80211_crypt_wep
 - lib80211_crypt_tkip
 - lib80211_crytp_ccmp

Package: kmod-libertas-sdio
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-cfg80211, kmod-lib80211, kmod-mmc, libertas-sdio-firmware
Source: package/kernel/mac80211
SourceName: kmod-libertas-sdio
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 32739
Filename: kmod-libertas-sdio_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 33592
SHA256sum: 2822173849d4f1f17e7e1140cd4234557d3a2127673277c8e96992de98976d8d
Description:  Marvell 88W8686 Wireless Driver

Package: kmod-libertas-spi
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-cfg80211, kmod-lib80211, libertas-spi-firmware
Source: package/kernel/mac80211
SourceName: kmod-libertas-spi
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 32420
Filename: kmod-libertas-spi_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 33166
SHA256sum: b95091abb57a8fa9c985728d906fb440c59be158d315d678f1890432adff21b7
Description:  Marvell 88W8686 SPI Wireless Driver

Package: kmod-libertas-usb
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-cfg80211, kmod-usb-core, kmod-lib80211, libertas-usb-firmware
Source: package/kernel/mac80211
SourceName: kmod-libertas-usb
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 31045
Filename: kmod-libertas-usb_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 31795
SHA256sum: 79d792d6a5e388a872d67ea9c758cc5d1b1404b1c6235c879d5ebe0088e2847f
Description:  Marvell 88W8015 Wireless Driver

Package: kmod-libipw
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-michael-mic, kmod-crypto-ecb, kmod-lib80211, kmod-cfg80211
Source: package/kernel/mac80211
SourceName: kmod-libipw
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 14893
Filename: kmod-libipw_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 15649
SHA256sum: 08fd1ee10241bb0b01c7ae843ae4d031f026f21382a9a58f18e143da5014ecd2
Description:  Hardware independent IEEE 802.11 networking stack for ipw2100 and ipw2200.

Package: kmod-libphy
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-libphy
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 232
Filename: kmod-libphy_4.14.167-1_mipsel_24kc.ipk
Size: 951
SHA256sum: 5bcc94ae60d06b40560af20639bf8141a9d846246eca603e58ac45e4bf918673
Description:  PHY library

Package: kmod-loop
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-loop
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 13374
Filename: kmod-loop_4.14.167-1_mipsel_24kc.ipk
Size: 14067
SHA256sum: 3c878d2f569836f9ce321f8c03f3cd3830b415b2b2d648af843bab8e7e07226e
Description:  Kernel module for loopback device support

Package: kmod-lp
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ppdev
Source: package/kernel/linux
SourceName: kmod-lp
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6684
Filename: kmod-lp_4.14.167-1_mipsel_24kc.ipk
Size: 7469
SHA256sum: caf24419e0f91e981e40da3a5b973e64920227a97e715467e597a6ef427b1ec0
Description:  Parallel port line printer device support

Package: kmod-mac80211-hwsim
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211
Source: package/kernel/mac80211
SourceName: kmod-mac80211-hwsim
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 21317
Filename: kmod-mac80211-hwsim_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 22041
SHA256sum: ea3632c925a6d50305ecdaa25b814f82a052ea0da71dfaef57bb2ba1480362b7
Description:  mac80211 HW simulation device

Package: kmod-mac80211
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-cfg80211, hostapd-common
Source: package/kernel/mac80211
SourceName: kmod-mac80211
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 264831
Filename: kmod-mac80211_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 263823
SHA256sum: 0cb503db6d40d6a8a7ad31ee2b6de00fd6a691fe140345cc1a5d7bbc5bb6f5f1
Description:  Generic IEEE 802.11 Networking Stack (mac80211)

Package: kmod-mac802154
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ieee802154, kmod-crypto-aead, kmod-lib-crc-ccitt
Source: package/kernel/linux
SourceName: kmod-mac802154
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 14874
Filename: kmod-mac802154_4.14.167-1_mipsel_24kc.ipk
Size: 15780
SHA256sum: 6b3a890e8d0bc550fb5474ddf8da950f174c1ac400c61360aa0370f64072b09c
Description:  This option enables the hardware independent IEEE 802.15.4
 networking stack for SoftMAC devices (the ones implementing
 only PHY level of IEEE 802.15.4 standard).
 
 Note: this implementation is neither certified, nor feature
 complete! Compatibility with other implementations hasn't
 been tested yet!

Package: kmod-macremapper
Version: 4.14.167-ramips-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-cfg80211, kmod-br-netfilter
Source: feeds/packages/kernel/macremapper
SourceName: kmod-macremapper
License: GPL-2.0-only
LicenseFiles: kernelmod/COPYING
Section: kernel
Maintainer: Carey Sonsino <careys@edgewaterwireless.com>
Architecture: mipsel_24kc
Installed-Size: 8908
Filename: kmod-macremapper_4.14.167-ramips-1_mipsel_24kc.ipk
Size: 9760
SHA256sum: 6aa4c1765c68feeb5d6ced07be96b9deedc397d4aee532a00551220e7e348a62
Description:  Linux kernel module for implementation the DCW filtering mechanism

Package: kmod-macsec
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-crypto-gcm
Source: package/kernel/linux
SourceName: kmod-macsec
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 14195
Filename: kmod-macsec_4.14.167-1_mipsel_24kc.ipk
Size: 14900
SHA256sum: bf97eeaa4bd564d6e80f0ec947f282d0e307eebec05479bc86635b24a25428e9
Description:  MACsec is an encryption standard for Ethernet.

Package: kmod-macvlan
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-macvlan
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9302
Filename: kmod-macvlan_4.14.167-1_mipsel_24kc.ipk
Size: 10110
SHA256sum: 2b4f9374721fee2565db7ebab6383a5722285a30d5935d2f2570eed12744e35f
Description:  A kernel module which allows one to create virtual interfaces that
 map packets to or from specific MAC addresses to a particular interface

Package: kmod-md-linear
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-md-mod
Source: package/kernel/linux
SourceName: kmod-md-linear
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3232
Filename: kmod-md-linear_4.14.167-1_mipsel_24kc.ipk
Size: 3964
SHA256sum: f2ea4967ccc50d7c62be97b31b4db7d93cdf72f62837b446f2801232d7a0cb3d
Description:  RAID "Linear" or "Append" driver module (linear.ko)

Package: kmod-md-mod
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-md-mod
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 68022
Filename: kmod-md-mod_4.14.167-1_mipsel_24kc.ipk
Size: 68666
SHA256sum: a8e183eac5fd538a4eb134c222f4fad24c002b21107663fe4b48612b52f153fa
Description:  Kernel RAID md module (md-mod.ko).
 You will need to select at least one RAID level module below.

Package: kmod-md-multipath
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-md-mod
Source: package/kernel/linux
SourceName: kmod-md-multipath
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4490
Filename: kmod-md-multipath_4.14.167-1_mipsel_24kc.ipk
Size: 5201
SHA256sum: cf69117a4e0a3b2c9b75a4396d54bc0f74556f78ad9ccaf013b3e0452889ec7a
Description:  Multipath driver module (multipath.ko)

Package: kmod-md-raid0
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-md-mod
Source: package/kernel/linux
SourceName: kmod-md-raid0
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6508
Filename: kmod-md-raid0_4.14.167-1_mipsel_24kc.ipk
Size: 7301
SHA256sum: 8d5967492f10883a839a130aef741d3a0d3055db39e1792ebb2d1f037a4b2b71
Description:  RAID Level 0 (Striping) driver module (raid0.ko)

Package: kmod-md-raid10
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-md-mod
Source: package/kernel/linux
SourceName: kmod-md-raid10
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 28138
Filename: kmod-md-raid10_4.14.167-1_mipsel_24kc.ipk
Size: 28818
SHA256sum: d63d48a7f29d74d2ad6cbb1120494fdfa3c5236a2d1c2dc82996e06e1f91012b
Description:  RAID Level 10 (Mirroring+Striping) driver module (raid10.ko)

Package: kmod-md-raid1
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-md-mod
Source: package/kernel/linux
SourceName: kmod-md-raid1
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 19864
Filename: kmod-md-raid1_4.14.167-1_mipsel_24kc.ipk
Size: 20564
SHA256sum: 56a86f4fd4083a6b3a90653b1346185ef34bf24041a78882a645c14cc9331bb6
Description:  RAID Level 1 (Mirroring) driver (raid1.ko)

Package: kmod-md-raid456
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-md-mod, kmod-lib-raid6, kmod-lib-xor, kmod-lib-crc32c
Source: package/kernel/linux
SourceName: kmod-md-raid456
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 75447
Filename: kmod-md-raid456_4.14.167-1_mipsel_24kc.ipk
Size: 76170
SHA256sum: 6ff339ed47e41d78795d12a72ea5a7f5dc0b31b26816559407504e54250eb06a
Description:  RAID Level 4,5,6 kernel module (raid456.ko)
 
 Includes the following modules required by
 raid456.ko:
 xor.ko
 async_tx.ko
 async_xor.ko
 async_memcpy.ko
 async_pq.ko
 async_raid5_recov.ko
 raid6_pq.ko

Package: kmod-mdio-gpio
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-libphy
Source: package/kernel/linux
SourceName: kmod-mdio-gpio
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3187
Filename: kmod-mdio-gpio_4.14.167-1_mipsel_24kc.ipk
Size: 3912
SHA256sum: 35607d43dc8de26ad854c82f64d7c7c067fb652e634ff5e24e96dc1a2254df95
Description:  Supports GPIO lib-based MDIO busses

Package: kmod-mdio
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-mdio
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2773
Filename: kmod-mdio_4.14.167-1_mipsel_24kc.ipk
Size: 3507
SHA256sum: c7ea74d7e633ca371a073b6e787db7b2032ec2d2392194c373194c37a7b1a0be
Description:  Kernel modules for MDIO (clause 45) PHY support

Package: kmod-mii
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-mii
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3469
Filename: kmod-mii_4.14.167-1_mipsel_24kc.ipk
Size: 4172
SHA256sum: 7c7fd3b1a2fb57e24a8a64d15e0ef7735c7da96153ebf5b8ced149aad443898f
Description:  MII library

Package: kmod-misdn
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-misdn
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 90296
Filename: kmod-misdn_4.14.167-1_mipsel_24kc.ipk
Size: 90847
SHA256sum: aff7f775be0b6508a735dc6eed6f95d278cbcaf3b1f4c8ff772572c554db1006
Description:  Modular ISDN driver support

Package: kmod-mmc-spi
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mmc, kmod-lib-crc-itu-t, kmod-lib-crc7
Source: package/kernel/linux
SourceName: kmod-mmc-spi
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7987
Filename: kmod-mmc-spi_4.14.167-1_mipsel_24kc.ipk
Size: 8762
SHA256sum: a63dfb58ac8ba466ef99e470d359087a87ff00aa8a82c010eff3946210a3d72c
Description:  Kernel support for MMC/SD over SPI

Package: kmod-mmc
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-mmc
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 65096
Filename: kmod-mmc_4.14.167-1_mipsel_24kc.ipk
Size: 65628
SHA256sum: a3e6b7f312cac913c2e2bcddfd679027980de80ac36c998d67f5576310e7b3bb
Description:  Kernel support for MMC/SD cards

Package: kmod-mpls
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-mpls
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 16420
Filename: kmod-mpls_4.14.167-1_mipsel_24kc.ipk
Size: 17069
SHA256sum: 1781c51ae5508092677919887bc94dc8b4aaf448baaba8dc3008cddbb75599c2
Description:  Kernel support for MPLS

Package: kmod-mppe
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ppp, kmod-crypto-sha1, kmod-crypto-ecb
Source: package/kernel/linux
SourceName: kmod-mppe
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4918
Filename: kmod-mppe_4.14.167-1_mipsel_24kc.ipk
Size: 5664
SHA256sum: 92ae1cc9cc8872f16ce02cc225246777fa5fbfe5336234a81d60365553819563
Description:  Kernel modules for Microsoft PPP compression/encryption

Package: kmod-mrf24j40
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac802154, kmod-regmap-spi
Source: package/kernel/linux
SourceName: kmod-mrf24j40
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6628
Filename: kmod-mrf24j40_4.14.167-1_mipsel_24kc.ipk
Size: 7153
SHA256sum: d0588439ec8a2a1c454c8728225f7be694243874097f81075da2cb9b26f46f06
Description:  MRF24J40 transceiver driver

Package: kmod-mt76-core
Version: 4.14.167+2020-01-04-8a785679-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211
Source: package/kernel/mt76
SourceName: kmod-mt76-core
License: GPLv2
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 20826
Filename: kmod-mt76-core_4.14.167+2020-01-04-8a785679-1_mipsel_24kc.ipk
Size: 21577
SHA256sum: d5115c72b8922103b41d735230976d2e063d22645eaba54e56be383af7e8e5b8
Description:  MediaTek MT76xx wireless driver

Package: kmod-mt76-usb
Version: 4.14.167+2020-01-04-8a785679-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-usb-core, kmod-mt76-core
Source: package/kernel/mt76
SourceName: kmod-mt76-usb
License: GPLv2
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 7205
Filename: kmod-mt76-usb_4.14.167+2020-01-04-8a785679-1_mipsel_24kc.ipk
Size: 8046
SHA256sum: e0c9556600b8afb88b9da9cfbc25cafe45b22a5791e7868e52fdf7c31e06179e
Description:  MediaTek MT76xx wireless driver USB support

Package: kmod-mt7601u
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-usb-core, mt7601u-firmware
Source: package/kernel/mac80211
SourceName: kmod-mt7601u
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 30836
Filename: kmod-mt7601u_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 31512
SHA256sum: ee67798cddc3d70a4026e820ced7f9309db04a471b0014c16b46e1215b40837d
Description:  MT7601U-based USB dongles Wireless Driver

Package: kmod-mt7603
Version: 4.14.167+2020-01-04-8a785679-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-mt76-core
Source: package/kernel/mt76
SourceName: kmod-mt7603
License: GPLv2
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 95158
Filename: kmod-mt7603_4.14.167+2020-01-04-8a785679-1_mipsel_24kc.ipk
Size: 95970
SHA256sum: 0b4e7524b0a6ff6587fd9f54e017f8e0947b75087254cab37bbb356e1b92c253
Description:  MediaTek MT7603 wireless driver

Package: kmod-mt7615e
Version: 4.14.167+2020-01-04-8a785679-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-mt76-core
Source: package/kernel/mt76
SourceName: kmod-mt7615e
License: GPLv2
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 579885
Filename: kmod-mt7615e_4.14.167+2020-01-04-8a785679-1_mipsel_24kc.ipk
Size: 580785
SHA256sum: fb967ba9f8c06f3c0608197a04370456ee680075a094a442686c68fa0fdaaa8c
Description:  MediaTek MT7615 wireless driver

Package: kmod-mt76
Version: 4.14.167+2020-01-04-8a785679-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mt76-core, kmod-mt76x2, kmod-mt7603
Source: package/kernel/mt76
SourceName: kmod-mt76
License: GPLv2
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-mt76_4.14.167+2020-01-04-8a785679-1_mipsel_24kc.ipk
Size: 899
SHA256sum: fcd21007f7e18e05320528da45bff0a2c9539384e8a59f0f0e8c27c83f09f62a
Description:  MediaTek MT76x2/MT7603 wireless driver (metapackage)

Package: kmod-mt76x0-common
Version: 4.14.167+2020-01-04-8a785679-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-mt76x02-common
Source: package/kernel/mt76
SourceName: kmod-mt76x0-common
License: GPLv2
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 60220
Filename: kmod-mt76x0-common_4.14.167+2020-01-04-8a785679-1_mipsel_24kc.ipk
Size: 60925
SHA256sum: 97067c131bc78be39c2a2edae6b0573b7cd4539826b154d6be7336e682e61119
Description:  MediaTek MT76x0 wireless driver common code

Package: kmod-mt76x02-common
Version: 4.14.167+2020-01-04-8a785679-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-mt76-core
Source: package/kernel/mt76
SourceName: kmod-mt76x02-common
License: GPLv2
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 24440
Filename: kmod-mt76x02-common_4.14.167+2020-01-04-8a785679-1_mipsel_24kc.ipk
Size: 25156
SHA256sum: 2b3454584408e613cc611e33e8c4cc01fdfc698320a870bc37c09d512ed2eef4
Description:  MediaTek MT76x0/MT76x2 wireless driver common code

Package: kmod-mt76x02-usb
Version: 4.14.167+2020-01-04-8a785679-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-mt76-usb, kmod-mt76x02-common
Source: package/kernel/mt76
SourceName: kmod-mt76x02-usb
License: GPLv2
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 5046
Filename: kmod-mt76x02-usb_4.14.167+2020-01-04-8a785679-1_mipsel_24kc.ipk
Size: 5832
SHA256sum: 7258d41582f7e513e1f3702ed1c2ea5fd0041245bdadb3e17e933cfd4123c92e
Description:  MediaTek MT76x0/MT76x2 USB wireless driver common code

Package: kmod-mt76x0e
Version: 4.14.167+2020-01-04-8a785679-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-mt76x0-common
Source: package/kernel/mt76
SourceName: kmod-mt76x0e
License: GPLv2
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 3510
Filename: kmod-mt76x0e_4.14.167+2020-01-04-8a785679-1_mipsel_24kc.ipk
Size: 4298
SHA256sum: a73dd9035a58fa606f421b13c84d66047a5caec74dd664da338bfcade180a023
Description:  MediaTek MT76x0E wireless driver

Package: kmod-mt76x0u
Version: 4.14.167+2020-01-04-8a785679-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-mt76x0-common, kmod-mt76x02-usb
Source: package/kernel/mt76
SourceName: kmod-mt76x0u
License: GPLv2
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 3937
Filename: kmod-mt76x0u_4.14.167+2020-01-04-8a785679-1_mipsel_24kc.ipk
Size: 4734
SHA256sum: 2536aa7f9b617af2f65cb7ffb4dc807eb8e9aa69480e6258f0733db352dc87c2
Description:  MediaTek MT76x0U wireless driver

Package: kmod-mt76x2-common
Version: 4.14.167+2020-01-04-8a785679-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-mt76-core, kmod-mt76x02-common
Source: package/kernel/mt76
SourceName: kmod-mt76x2-common
License: GPLv2
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 78705
Filename: kmod-mt76x2-common_4.14.167+2020-01-04-8a785679-1_mipsel_24kc.ipk
Size: 79631
SHA256sum: ca8ec2029dd2c97c55d78df26b083f7cfdd97936e88664b0a0439ac5a290d41a
Description:  MediaTek MT76x2 wireless driver common code

Package: kmod-mt76x2
Version: 4.14.167+2020-01-04-8a785679-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-mt76x2-common
Source: package/kernel/mt76
SourceName: kmod-mt76x2
License: GPLv2
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 7618
Filename: kmod-mt76x2_4.14.167+2020-01-04-8a785679-1_mipsel_24kc.ipk
Size: 8426
SHA256sum: 1d2d6b3ed085f86d859e634ea200ad395d7485ea6a94626186b07e1d13d79372
Description:  MediaTek MT76x2 wireless driver

Package: kmod-mt76x2u
Version: 4.14.167+2020-01-04-8a785679-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-mt76x2-common, kmod-mt76x02-usb
Source: package/kernel/mt76
SourceName: kmod-mt76x2u
License: GPLv2
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 7619
Filename: kmod-mt76x2u_4.14.167+2020-01-04-8a785679-1_mipsel_24kc.ipk
Size: 8438
SHA256sum: 8537c6e83204e6b63446eacf46b738f9d629cde2cdc4eb890bde9423ebf38cef
Description:  MediaTek MT76x2U wireless driver

Package: kmod-mtd-rw
Version: 4.14.167+git-20160214-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: feeds/packages/kernel/mtd-rw
SourceName: kmod-mtd-rw
License: GPL-2.0
LicenseFiles: LICENSE
Section: kernel
Maintainer: Joseph C. Lehner <joseph.c.lehner@gmail.com>
Architecture: mipsel_24kc
Installed-Size: 1472
Filename: kmod-mtd-rw_4.14.167+git-20160214-1_mipsel_24kc.ipk
Size: 2307
SHA256sum: 9cc7b575ee97a6f7b1efa8db1db4db5f816d90ae97d4284fdf0698ae097a16b8
Description:  A kernel module that temporarily makes all MTD partitions writeable.

Package: kmod-mtdoops
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-mtdoops
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4534
Filename: kmod-mtdoops_4.14.167-1_mipsel_24kc.ipk
Size: 5248
SHA256sum: 6d600d9472348efcbd9d9af9b27a692d1ce896f73517f6bb712175d404b1f58e
Description:  Kernel modules for Log panic/oops to an MTD buffer

Package: kmod-mtdram
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-mtdram
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1826
Filename: kmod-mtdram_4.14.167-1_mipsel_24kc.ipk
Size: 2574
SHA256sum: da8e394a860c3c6c937368dc74127688115d75f2c80328f6ad44c896821f2d1d
Description:  Test MTD driver using RAM

Package: kmod-mtdtests
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-mtdtests
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 27955
Filename: kmod-mtdtests_4.14.167-1_mipsel_24kc.ipk
Size: 28597
SHA256sum: 23deadfeac16215a029a78526340823277ac124be908ad3b7dc354147d73e633
Description:  Kernel modules for MTD subsystem/driver testing

Package: kmod-mwifiex-pcie
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, mwifiex-pcie-firmware
Source: package/kernel/mac80211
SourceName: kmod-mwifiex-pcie
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 151292
Filename: kmod-mwifiex-pcie_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 148591
SHA256sum: 34ec6e0011e05d3e6f8b351ed80ccbef318b5942b834f2a1fa127d1ae20eb01b
Description:  Kernel modules for Marvell 802.11n/802.11ac PCIe Wireless cards

Package: kmod-mwifiex-sdio
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mmc, kmod-mac80211, mwifiex-sdio-firmware
Source: package/kernel/mac80211
SourceName: kmod-mwifiex-sdio
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 149586
Filename: kmod-mwifiex-sdio_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 146916
SHA256sum: a70397245b88ef2b898527c2f2e4dd199433c35db627a6e4ace4feb32cde4727
Description:  Kernel modules for Marvell 802.11n/802.11ac SDIO Wireless cards

Package: kmod-mwl8k
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, mwl8k-firmware
Source: package/kernel/mac80211
SourceName: kmod-mwl8k
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 26110
Filename: kmod-mwl8k_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 26773
SHA256sum: d9913dcebb6cdb33c323cb0bf81ce85a078f7f4d29ea26a43fb3ddec6daf92ed
Description:  Kernel modules for Marvell TOPDOG 802.11 Wireless cards

Package: kmod-nat46
Version: 4.14.167+2017-05-12-683fbd2b-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/nat46
SourceName: kmod-nat46
License: GPL-2.0
Section: kernel
Maintainer: Hans Dedecker <dedeckeh@gmail.com>
Architecture: mipsel_24kc
Installed-Size: 15588
Filename: kmod-nat46_4.14.167+2017-05-12-683fbd2b-1_mipsel_24kc.ipk
Size: 16330
SHA256sum: 951a4ac2911717e71198736803ca380a95094349428e1c048f8d86ce04b30f0f
Description:  Stateless NAT46 translation kernel module

Package: kmod-natsemi
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-natsemi
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 14015
Filename: kmod-natsemi_4.14.167-1_mipsel_24kc.ipk
Size: 14730
SHA256sum: ada20d4b2b3f84aabd87b561be6f38cc9bfe795494de4b74f429ae951e84240c
Description:  Kernel modules for National Semiconductor DP8381x series PCI Ethernet
 adapters.

Package: kmod-nbd
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-nbd
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 15997
Filename: kmod-nbd_4.14.167-1_mipsel_24kc.ipk
Size: 16685
SHA256sum: ab7ca7563f4d534b6e63ee490e86a776e2d4481255aa9e471dea29b80a30453d
Description:  Kernel module for network block device support

Package: kmod-ne2k-pci
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-ne2k-pci
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9708
Filename: kmod-ne2k-pci_4.14.167-1_mipsel_24kc.ipk
Size: 10468
SHA256sum: d584a7f8b83edcf40b0ea4610e73c93be86d111855f0d81437c8d130bf9c42c3
Description:  Kernel modules for NE2000 PCI Ethernet Adapter kernel

Package: kmod-net-prism54
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), prism54-firmware
Source: package/kernel/linux
SourceName: kmod-net-prism54
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-net-prism54_4.14.167-1_mipsel_24kc.ipk
Size: 848
SHA256sum: c21dbf91798e357998be38f21a50ed89a1c669b07110fdcc547d2587d6222fcd
Description:  Kernel modules for Intersil Prism54 support

Package: kmod-net-rtl8192su
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core, rtl8192su-firmware
Source: package/kernel/linux
SourceName: kmod-net-rtl8192su
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 75038
Filename: kmod-net-rtl8192su_4.14.167-1_mipsel_24kc.ipk
Size: 75614
SHA256sum: 3a67b2c428076691b318053e535d6ee45beb8b966362cefd5f07375f72e83df3
Description:  Kernel modules for RealTek RTL8712 and RTL81XXSU fullmac support.

Package: kmod-netatop
Version: 4.14.167+2.0-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: feeds/packages/admin/netatop
SourceName: kmod-netatop
License: GPL-2.0
Section: kernel
Maintainer: Toni Uhlig <matzeton@googlemail.com>
Architecture: mipsel_24kc
Installed-Size: 7644
Filename: kmod-netatop_4.14.167+2.0-1_mipsel_24kc.ipk
Size: 8693
SHA256sum: 866121045eae49df2ba5195de91703525336427ca43f8c60bb5424ab1c211212
Description:  The optional kernel module netatop can be loaded to gather statistics about
 the TCP and UDP packets that have been transmitted/received per process and
 per thread. As soon as atop discovers that this module is active, it shows
 the columns SNET and RNET in the generic screen for the number of transmitted
 and received packets per process. When the 'n' key is pressed, it shows
 detailed counters about the number packets transmitted/received via TCP and
 UDP, the average sizes of these packets, and the total bandwidth consumed
 for input and output per process/thread.

Package: kmod-netem
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sched
Source: package/kernel/linux
SourceName: kmod-netem
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6139
Filename: kmod-netem_4.14.167-1_mipsel_24kc.ipk
Size: 6883
SHA256sum: 0b70cac8e937e597ce9e7e2c8f5289ca05fc9d169100ecde1530fc6cc9b9eebb
Description:  Kernel modules for emulating the properties of wide area networks

Package: kmod-nf-conntrack-netlink
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nfnetlink, kmod-ipt-conntrack
Source: package/kernel/linux
SourceName: kmod-nf-conntrack-netlink
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 14439
Filename: kmod-nf-conntrack-netlink_4.14.167-1_mipsel_24kc.ipk
Size: 15210
SHA256sum: dfa1cf70fb1726d11ce0259e9900b2dc3ff1106a9ac7aec628fb5005ecd69889
Description:  Kernel modules support for a netlink-based connection tracking
 userspace interface

Package: kmod-nf-conntrack6
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nf-conntrack
Source: package/kernel/linux
SourceName: kmod-nf-conntrack6
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 8848
Filename: kmod-nf-conntrack6_4.14.167-1_mipsel_24kc.ipk
Size: 9609
SHA256sum: f35b8ccff0678049f5369e2a91372e765d9ade970a16c436918572c15fb66d1e
Description:  Netfilter IPv6 connection tracking

Package: kmod-nf-conntrack
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-nf-conntrack
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 46209
Filename: kmod-nf-conntrack_4.14.167-1_mipsel_24kc.ipk
Size: 46880
SHA256sum: e944ce35b0af64ebaef211972cf47cbe6ae2ca63e76f38b2e5376428d6ad729e
Description:  Netfilter connection tracking

Package: kmod-nf-flow
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nf-conntrack
Source: package/kernel/linux
SourceName: kmod-nf-flow
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10079
Filename: kmod-nf-flow_4.14.167-1_mipsel_24kc.ipk
Size: 10839
SHA256sum: e5d7fde6972160fe6808167ba27ef42e20d84b6fe29f756afc778c32c7b998e9
Description:  Netfilter flowtable support

Package: kmod-nf-ipt6
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nf-ipt
Source: package/kernel/linux
SourceName: kmod-nf-ipt6
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 8580
Filename: kmod-nf-ipt6_4.14.167-1_mipsel_24kc.ipk
Size: 9302
SHA256sum: ef8566acc927dde69644cf896ca6f375b84c7418b85c43c93b756b97b07d2168
Description:  Ip6tables core

Package: kmod-nf-ipt
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-nf-ipt
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 16685
Filename: kmod-nf-ipt_4.14.167-1_mipsel_24kc.ipk
Size: 17367
SHA256sum: 222422dd0439eaf0f66214b5e2e24b2451f71acf4a2b0aeb67f716e39fc883e6
Description:  Iptables core

Package: kmod-nf-ipvs-ftp
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nf-ipvs, kmod-nf-nat, kmod-nf-nathelper
Source: package/kernel/linux
SourceName: kmod-nf-ipvs-ftp
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2989
Filename: kmod-nf-ipvs-ftp_4.14.167-1_mipsel_24kc.ipk
Size: 3879
SHA256sum: 69eeb19971613a1cca871c789ecefb8f60bf420033f82569151111777aaf0a46
Description:  In the virtual server via Network Address Translation,
 the IP address and port number of real servers cannot be sent to
 clients in ftp connections directly, so FTP protocol helper is
 required for tracking the connection and mangling it back to that of
 virtual service.

Package: kmod-nf-ipvs-sip
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nf-ipvs, kmod-nf-nathelper-extra
Source: package/kernel/linux
SourceName: kmod-nf-ipvs-sip
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2268
Filename: kmod-nf-ipvs-sip_4.14.167-1_mipsel_24kc.ipk
Size: 3044
SHA256sum: 7a6a01e6261104f08d67c2a6e07991f1a74bf2e39f9247f59e92690765cb15c0
Description:  Allow persistence based on the SIP Call-ID

Package: kmod-nf-ipvs
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-crc32c, kmod-ipt-conntrack, kmod-nf-conntrack, kmod-nf-conntrack6, kmod-ipt-core, kmod-ipt-conntrack
Source: package/kernel/linux
SourceName: kmod-nf-ipvs
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 74488
Filename: kmod-nf-ipvs_4.14.167-1_mipsel_24kc.ipk
Size: 75139
SHA256sum: b54eab8d23f0d20d067eced1f4e17c9f254281fc9c9f0f9a9ba77690636f1fd0
Description:  IPVS (IP Virtual Server) implements transport-layer load balancing inside
 the Linux kernel so called Layer-4 switching.

Package: kmod-nf-nat6
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nf-conntrack6, kmod-nf-nat
Source: package/kernel/linux
SourceName: kmod-nf-nat6
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5673
Filename: kmod-nf-nat6_4.14.167-1_mipsel_24kc.ipk
Size: 6416
SHA256sum: dfbd780cdf7a6bd0aab3b9c34d1c09dff0b9813ea4bcd2df057d05d07ea39602
Description:  Netfilter IPV6-NAT

Package: kmod-nf-nat
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nf-conntrack
Source: package/kernel/linux
SourceName: kmod-nf-nat
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 13069
Filename: kmod-nf-nat_4.14.167-1_mipsel_24kc.ipk
Size: 13812
SHA256sum: 6a3fe93efbf10fadcef57106a3c65ce1535a5ef2b8bf7d917f8a43c2134e696d
Description:  Netfilter NAT

Package: kmod-nf-nathelper-extra
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nf-nat, kmod-lib-textsearch, kmod-ipt-raw
Source: package/kernel/linux
SourceName: kmod-nf-nathelper-extra
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 54114
Filename: kmod-nf-nathelper-extra_4.14.167-1_mipsel_24kc.ipk
Size: 54894
SHA256sum: 9ecff7811513ca137b4d48d57d836b820b3758d8d312bed9e09eed15dbddce1d
Description:  Extra Netfilter (IPv4) Conntrack and NAT helpers
 Includes:
 - amanda
 - h323
 - irc
 - mms
 - pptp
 - proto_gre
 - sip
 - snmp_basic
 - tftp
 - broadcast

Package: kmod-nf-nathelper
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nf-nat
Source: package/kernel/linux
SourceName: kmod-nf-nathelper
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5267
Filename: kmod-nf-nathelper_4.14.167-1_mipsel_24kc.ipk
Size: 6041
SHA256sum: 1165fc077426b5a6b583a4fd34a6c4acbfad838f748ad0128559ea115690f44e
Description:  Default Netfilter (IPv4) Conntrack and NAT helpers
 Includes:
 - ftp

Package: kmod-nf-reject6
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-nf-reject6
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2401
Filename: kmod-nf-reject6_4.14.167-1_mipsel_24kc.ipk
Size: 3165
SHA256sum: 9c709e9807e442e3cbe0541804bedb5f05fa7d15348cdbff24d87e8861e179d7
Description:  Netfilter IPv6 reject support

Package: kmod-nf-reject
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-nf-reject
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2078
Filename: kmod-nf-reject_4.14.167-1_mipsel_24kc.ipk
Size: 2833
SHA256sum: 43072e4faf31add12420d9a308bb3472c1e0b6203cc51ded16c3fee82a54d745
Description:  Netfilter IPv4 reject support

Package: kmod-nfnetlink-log
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nfnetlink
Source: package/kernel/linux
SourceName: kmod-nfnetlink-log
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6446
Filename: kmod-nfnetlink-log_4.14.167-1_mipsel_24kc.ipk
Size: 7257
SHA256sum: 828306907f2c0e38fa855b95fee8b13f1f9cb67ee8dc30b2036654058a46316e
Description:  Kernel modules support for logging packets via NFNETLINK
 Includes:
 - NFLOG

Package: kmod-nfnetlink-queue
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nfnetlink
Source: package/kernel/linux
SourceName: kmod-nfnetlink-queue
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7934
Filename: kmod-nfnetlink-queue_4.14.167-1_mipsel_24kc.ipk
Size: 8722
SHA256sum: 32b8277fba6a0f348e1f02fc61e5febdc18fe2cc2e386670fb90619712ddf839
Description:  Kernel modules support for queueing packets via NFNETLINK
 Includes:
 - NFQUEUE

Package: kmod-nfnetlink
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-nfnetlink
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4088
Filename: kmod-nfnetlink_4.14.167-1_mipsel_24kc.ipk
Size: 4811
SHA256sum: 52b9b6259bc1732444618fef69295ad636aca00716d8cf19bb72dc744dcc929a
Description:  Kernel modules support for a netlink-based userspace interface

Package: kmod-nft-arp
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nft-core
Source: package/kernel/linux
SourceName: kmod-nft-arp
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 850
Filename: kmod-nft-arp_4.14.167-1_mipsel_24kc.ipk
Size: 1610
SHA256sum: ae8b337b4d912416667be865a5ecb9dc5a893f1a2ff142ce7d27ded50fba9b8c
Description:  Netfilter nf_tables ARP table support

Package: kmod-nft-bridge
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nft-core
Source: package/kernel/linux
SourceName: kmod-nft-bridge
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4763
Filename: kmod-nft-bridge_4.14.167-1_mipsel_24kc.ipk
Size: 5523
SHA256sum: b75f7200738862294b0ce5fa2b3bfb0df0529e3f01a03a8cf913fae17449b963
Description:  Netfilter nf_tables bridge table support

Package: kmod-nft-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nfnetlink, kmod-nf-reject, kmod-nf-reject6, kmod-nf-conntrack6
Source: package/kernel/linux
SourceName: kmod-nft-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 67140
Filename: kmod-nft-core_4.14.167-1_mipsel_24kc.ipk
Size: 67903
SHA256sum: 26fcfa9980ea62feda485cd7640ef324dd50286d0fb1d6ccb2691e0470d796ac
Description:  Kernel module support for nftables

Package: kmod-nft-fib
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nft-core
Source: package/kernel/linux
SourceName: kmod-nft-fib
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5426
Filename: kmod-nft-fib_4.14.167-1_mipsel_24kc.ipk
Size: 6142
SHA256sum: f656f9e5493592b2d78b6540508ff4770c8a9fc3843dee84bc5f19f0cb80051e
Description:  Netfilter nf_tables fib support

Package: kmod-nft-nat6
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nft-nat, kmod-nf-nat6
Source: package/kernel/linux
SourceName: kmod-nft-nat6
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2211
Filename: kmod-nft-nat6_4.14.167-1_mipsel_24kc.ipk
Size: 2968
SHA256sum: c6f51c1c44e0f9966875a60fdb2f11284316f086c0cc3324544461debacc6c0e
Description:  Netfilter nf_tables IPv6-NAT support

Package: kmod-nft-nat
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nft-core, kmod-nf-nat
Source: package/kernel/linux
SourceName: kmod-nft-nat
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4085
Filename: kmod-nft-nat_4.14.167-1_mipsel_24kc.ipk
Size: 4814
SHA256sum: 1d6ff7af42421a15dee07da1362578b8d345d0e0d2861cb8b8a0058cd830692c
Description:  Netfilter nf_tables NAT support

Package: kmod-nft-netdev
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nft-core
Source: package/kernel/linux
SourceName: kmod-nft-netdev
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3064
Filename: kmod-nft-netdev_4.14.167-1_mipsel_24kc.ipk
Size: 3817
SHA256sum: 612ddcbe08db08c86c731f8d1c6d5b301a693dc2669b644b1ab81834891ca3d3
Description:  Netfilter nf_tables netdev support

Package: kmod-nft-offload
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nf-flow, kmod-nft-nat
Source: package/kernel/linux
SourceName: kmod-nft-offload
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2554
Filename: kmod-nft-offload_4.14.167-1_mipsel_24kc.ipk
Size: 3322
SHA256sum: 1766fce46f34b826806bd3ff6b6b96556448cf12447e5c52cc3111d5fc82c52d
Description:  Netfilter nf_tables routing/NAT offload support

Package: kmod-niu
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-niu
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 14261
Filename: kmod-niu_4.14.167-1_mipsel_24kc.ipk
Size: 14983
SHA256sum: efb8e4b628531933a9b2a55d2688be01bc56a7ea5e1e50ac7a62c97e1ebf42cb
Description:  This enables support for cards based upon Sun's Neptune chipset.

Package: kmod-nlmon
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-nlmon
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1267
Filename: kmod-nlmon_4.14.167-1_mipsel_24kc.ipk
Size: 2042
SHA256sum: e52189776177e04da3f5d523579a1d8a27b4241d7d390319dec49ccd4c3f0028
Description:  Kernel module which adds a monitoring device for netlink.

Package: kmod-nls-base
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-nls-base
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3086
Filename: kmod-nls-base_4.14.167-1_mipsel_24kc.ipk
Size: 3810
SHA256sum: 8a696f9761ea09c38e4133bb2ac612c42357e5fa7936ec135c140b9b90168476
Description:  Kernel module for NLS (Native Language Support)

Package: kmod-nls-cp1250
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-cp1250
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1978
Filename: kmod-nls-cp1250_4.14.167-1_mipsel_24kc.ipk
Size: 2731
SHA256sum: 55d4f4119c340be2d83a696b040700d4e155469e9fdea8e03bfa5695211d5b38
Description:  Kernel module for NLS Codepage 1250 (Eastern Europe)

Package: kmod-nls-cp1251
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-cp1251
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1894
Filename: kmod-nls-cp1251_4.14.167-1_mipsel_24kc.ipk
Size: 2639
SHA256sum: f475290f85f5c4ca24b77d7859c2b01542e5a2927fef9e2b8b20c5670fc98e09
Description:  Kernel module for NLS Codepage 1251 (Russian)

Package: kmod-nls-cp437
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-cp437
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2053
Filename: kmod-nls-cp437_4.14.167-1_mipsel_24kc.ipk
Size: 2809
SHA256sum: d789d07a18ce8c802869b64799ed8d62de4f1bf679830dea13f7c28c40d08100
Description:  Kernel module for NLS Codepage 437 (United States, Canada)

Package: kmod-nls-cp775
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-cp775
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2077
Filename: kmod-nls-cp775_4.14.167-1_mipsel_24kc.ipk
Size: 2825
SHA256sum: f890378304a47c6b1c2f4cc29d44ee30b5211331aef8915e5e7c3544381833bb
Description:  Kernel module for NLS Codepage 775 (Baltic Rim)

Package: kmod-nls-cp850
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-cp850
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2010
Filename: kmod-nls-cp850_4.14.167-1_mipsel_24kc.ipk
Size: 2760
SHA256sum: 4340ccca4dde4ccbddb3826680a048b16bb199c49581577ad042a893746eb07d
Description:  Kernel module for NLS Codepage 850 (Europe)

Package: kmod-nls-cp852
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-cp852
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2084
Filename: kmod-nls-cp852_4.14.167-1_mipsel_24kc.ipk
Size: 2828
SHA256sum: f47a83e7d42dd35f80309ec4cd1821926149a9999ea616bb39c153a6ecb013f0
Description:  Kernel module for NLS Codepage 852 (Europe)

Package: kmod-nls-cp862
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-cp862
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2019
Filename: kmod-nls-cp862_4.14.167-1_mipsel_24kc.ipk
Size: 2772
SHA256sum: ab2e1d911691cd9b3c53b43c445c7c89176c44372797d32c08c5a38754779262
Description:  Kernel module for NLS Codepage 862 (Hebrew)

Package: kmod-nls-cp864
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-cp864
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1994
Filename: kmod-nls-cp864_4.14.167-1_mipsel_24kc.ipk
Size: 2749
SHA256sum: 8d1130136af5fa8af6d27a418c56d7fbed888fb493cfbae5f1e9836c37ff7333
Description:  Kernel module for NLS Codepage 864 (Arabic)

Package: kmod-nls-cp866
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-cp866
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1902
Filename: kmod-nls-cp866_4.14.167-1_mipsel_24kc.ipk
Size: 2658
SHA256sum: de16ed58a32dc9369f782af9323625bceaecc6c29004b29c32c21f397e398542
Description:  Kernel module for NLS Codepage 866 (Cyrillic)

Package: kmod-nls-cp932
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-cp932
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 36397
Filename: kmod-nls-cp932_4.14.167-1_mipsel_24kc.ipk
Size: 37177
SHA256sum: 712765a1faed0bbf753f5354228e50a711f92fd4fbfc1127168961a2a32413b9
Description:  Kernel module for NLS Codepage 932 (Japanese)

Package: kmod-nls-cp936
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-cp936
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 85594
Filename: kmod-nls-cp936_4.14.167-1_mipsel_24kc.ipk
Size: 86161
SHA256sum: 2c46e1d56cb6d74a89cc828daaf10a4080f98315573698bd2275d42102de87bc
Description:  Kernel module for NLS Codepage 936 (Simplified Chinese)

Package: kmod-nls-cp950
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-cp950
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 61304
Filename: kmod-nls-cp950_4.14.167-1_mipsel_24kc.ipk
Size: 62060
SHA256sum: 0df08d4ef6d2926a46df03cbeb5dbd1366cfd92def0505bb3c35649f1ee6d6dd
Description:  Kernel module for NLS Codepage 950 (Traditional Chinese)

Package: kmod-nls-iso8859-13
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-iso8859-13
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1923
Filename: kmod-nls-iso8859-13_4.14.167-1_mipsel_24kc.ipk
Size: 2675
SHA256sum: f916a6cc7fbc9a9262b2a987ff60d2f00593b08de27f3b265909d1cf9ae6ad96
Description:  Kernel module for NLS ISO 8859-13 (Latin 7; Baltic)

Package: kmod-nls-iso8859-15
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-iso8859-15
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1795
Filename: kmod-nls-iso8859-15_4.14.167-1_mipsel_24kc.ipk
Size: 2543
SHA256sum: eff7d28f23185505c0248d9970b0794b7f29b48c184f7ce7f2b595c38a556d26
Description:  Kernel module for NLS ISO 8859-15 (Latin 9)

Package: kmod-nls-iso8859-1
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-iso8859-1
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1680
Filename: kmod-nls-iso8859-1_4.14.167-1_mipsel_24kc.ipk
Size: 2455
SHA256sum: 1173318c16b1d354746fa343a5c3363f542d55cc15410ecbb582d688964d5ab9
Description:  Kernel module for NLS ISO 8859-1 (Latin 1)

Package: kmod-nls-iso8859-2
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-iso8859-2
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1926
Filename: kmod-nls-iso8859-2_4.14.167-1_mipsel_24kc.ipk
Size: 2677
SHA256sum: 9472302407373ae244ce32af05e7b94dd2446297260000d576f7f51cc9946f23
Description:  Kernel module for NLS ISO 8859-2 (Latin 2)

Package: kmod-nls-iso8859-6
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-iso8859-6
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1583
Filename: kmod-nls-iso8859-6_4.14.167-1_mipsel_24kc.ipk
Size: 2359
SHA256sum: 77fd8e08dfaf8b446b17d36c5e2c9e5420b0feeb5e22111846d80432911203cc
Description:  Kernel module for NLS ISO 8859-6 (Arabic)

Package: kmod-nls-iso8859-8
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-iso8859-8
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1779
Filename: kmod-nls-iso8859-8_4.14.167-1_mipsel_24kc.ipk
Size: 2546
SHA256sum: f633dc7d3ba7f1cf4d5c47b7e15ab32bf542c7dc587d035ad79305151581e56e
Description:  Kernel module for Hebrew charsets (ISO-8859-8, CP1255)

Package: kmod-nls-koi8r
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-koi8r
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1934
Filename: kmod-nls-koi8r_4.14.167-1_mipsel_24kc.ipk
Size: 2688
SHA256sum: 4fe3fb78c2cd33a8e788535f8c1775f3a4b19e3815e8c47e5a98c379395b045e
Description:  Kernel module for NLS KOI8-R (Russian)

Package: kmod-nls-utf8
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-nls-utf8
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 956
Filename: kmod-nls-utf8_4.14.167-1_mipsel_24kc.ipk
Size: 1715
SHA256sum: 34062b9b2c60eaf0bb6caabace9987e5f45962f78fcedadacfd07db1842316fb
Description:  Kernel module for NLS UTF-8

Package: kmod-nvmem
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-nvmem
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6014
Filename: kmod-nvmem_4.14.167-1_mipsel_24kc.ipk
Size: 6797
SHA256sum: 21d4861988e220f7d84710653d6dcc8c324231370293d9f083836081b6c904ec
Description:  Support for NVMEM(Non Volatile Memory) devices like EEPROM, EFUSES, etc.

Package: kmod-of-mdio
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-libphy
Source: package/kernel/linux
SourceName: kmod-of-mdio
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 191
Filename: kmod-of-mdio_4.14.167-1_mipsel_24kc.ipk
Size: 940
SHA256sum: fb33a5bb5bfc7a003799d206cbc1fdf3b700800bed6336fa65fc07f0d765e859
Description:  Kernel driver for OpenFirmware MDIO support

Package: kmod-openvswitch-geneve-intree
Version: 4.14.167+2.11.1-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-openvswitch-intree, kmod-geneve
Provides: kmod-openvswitch-geneve
Source: feeds/packages/net/openvswitch
SourceName: kmod-openvswitch-geneve-intree
License: Apache-2.0
LicenseFiles: LICENSE
Section: kernel
Maintainer: Yousong Zhou <yszhou4tech@gmail.com>
Architecture: mipsel_24kc
Installed-Size: 1391
Filename: kmod-openvswitch-geneve-intree_4.14.167+2.11.1-2_mipsel_24kc.ipk
Size: 2253
SHA256sum: e1184dfd12b48691e426095623bff620e5a4ffe05e766c39cad9b0d42e89d86a
Description:  Open vSwitch Geneve tunneling support (in tree)

Package: kmod-openvswitch-geneve
Version: 4.14.167+2.11.1-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-openvswitch, kmod-geneve
Source: feeds/packages/net/openvswitch
SourceName: kmod-openvswitch-geneve
License: Apache-2.0
LicenseFiles: LICENSE
Section: kernel
Maintainer: Yousong Zhou <yszhou4tech@gmail.com>
Architecture: mipsel_24kc
Installed-Size: 1358
Filename: kmod-openvswitch-geneve_4.14.167+2.11.1-2_mipsel_24kc.ipk
Size: 2201
SHA256sum: 7c036ec23a945a40dfc70985c1fc11d01e6164840a5bb762c753039eab374308
Description:  Open vSwitch Geneve tunneling support (upstream)

Package: kmod-openvswitch-gre-intree
Version: 4.14.167+2.11.1-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-openvswitch-intree, kmod-gre
Provides: kmod-openvswitch-gre
Source: feeds/packages/net/openvswitch
SourceName: kmod-openvswitch-gre-intree
License: Apache-2.0
LicenseFiles: LICENSE
Section: kernel
Maintainer: Yousong Zhou <yszhou4tech@gmail.com>
Architecture: mipsel_24kc
Installed-Size: 1245
Filename: kmod-openvswitch-gre-intree_4.14.167+2.11.1-2_mipsel_24kc.ipk
Size: 2099
SHA256sum: 21555379ae7a65c6c3b47d77585cb711c66409de74c8fc51f1dc0af184f4710a
Description:  Open vSwitch GRE tunneling support (in tree)

Package: kmod-openvswitch-gre
Version: 4.14.167+2.11.1-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-openvswitch, kmod-gre
Source: feeds/packages/net/openvswitch
SourceName: kmod-openvswitch-gre
License: Apache-2.0
LicenseFiles: LICENSE
Section: kernel
Maintainer: Yousong Zhou <yszhou4tech@gmail.com>
Architecture: mipsel_24kc
Installed-Size: 1211
Filename: kmod-openvswitch-gre_4.14.167+2.11.1-2_mipsel_24kc.ipk
Size: 2059
SHA256sum: 519ba2e570e1bbc712abddef39cea98ae49e5f061e5e27d2528b29fa3ffe5284
Description:  Open vSwitch GRE tunneling support (upstream)

Package: kmod-openvswitch-intree
Version: 4.14.167+2.11.1-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-crc32c, kmod-mpls, kmod-nf-nat, kmod-nf-nat6, kmod-nf-conntrack, kmod-nf-conntrack6, kmod-gre, kmod-gre6
Provides: kmod-openvswitch
Source: feeds/packages/net/openvswitch
SourceName: kmod-openvswitch-intree
License: Apache-2.0
LicenseFiles: LICENSE
Section: kernel
Maintainer: Yousong Zhou <yszhou4tech@gmail.com>
Architecture: mipsel_24kc
Installed-Size: 128722
Filename: kmod-openvswitch-intree_4.14.167+2.11.1-2_mipsel_24kc.ipk
Size: 129180
SHA256sum: 39f215fd2ae8f275943682272856a25eca0bad6c0b0fe1cecdf361fe4d5ad88d
Description:  Open vSwitch kernel datapath (in tree)

Package: kmod-openvswitch-lisp-intree
Version: 4.14.167+2.11.1-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-openvswitch-intree
Provides: kmod-openvswitch-lisp
Source: feeds/packages/net/openvswitch
SourceName: kmod-openvswitch-lisp-intree
License: Apache-2.0
LicenseFiles: LICENSE
Section: kernel
Maintainer: Yousong Zhou <yszhou4tech@gmail.com>
Architecture: mipsel_24kc
Installed-Size: 1395
Filename: kmod-openvswitch-lisp-intree_4.14.167+2.11.1-2_mipsel_24kc.ipk
Size: 2247
SHA256sum: 2adf287156d34791d5f90f9fcce40430eea1ad0f66d574e2ae6ad154a3fd99ef
Description:  Open vSwitch LISP tunneling support (in tree)

Package: kmod-openvswitch-stt-intree
Version: 4.14.167+2.11.1-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-openvswitch-intree
Provides: kmod-openvswitch-stt
Source: feeds/packages/net/openvswitch
SourceName: kmod-openvswitch-stt-intree
License: Apache-2.0
LicenseFiles: LICENSE
Section: kernel
Maintainer: Yousong Zhou <yszhou4tech@gmail.com>
Architecture: mipsel_24kc
Installed-Size: 1392
Filename: kmod-openvswitch-stt-intree_4.14.167+2.11.1-2_mipsel_24kc.ipk
Size: 2244
SHA256sum: 2ac83c8951a1b3fa7ee286371becd53a23fb54f04fa619bd5c4df4f2deef4ccc
Description:  Open vSwitch STT tunneling support (in tree)

Package: kmod-openvswitch-vxlan-intree
Version: 4.14.167+2.11.1-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-openvswitch-intree, kmod-vxlan
Provides: kmod-openvswitch-vxlan
Source: feeds/packages/net/openvswitch
SourceName: kmod-openvswitch-vxlan-intree
License: Apache-2.0
LicenseFiles: LICENSE
Section: kernel
Maintainer: Yousong Zhou <yszhou4tech@gmail.com>
Architecture: mipsel_24kc
Installed-Size: 1801
Filename: kmod-openvswitch-vxlan-intree_4.14.167+2.11.1-2_mipsel_24kc.ipk
Size: 2661
SHA256sum: a86648e20738755cc227bef8f36a9fd781678f7a911b1368ce03f8143cbea305
Description:  Open vSwitch VXLAN tunneling support (in tree)

Package: kmod-openvswitch-vxlan
Version: 4.14.167+2.11.1-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-openvswitch, kmod-vxlan
Source: feeds/packages/net/openvswitch
SourceName: kmod-openvswitch-vxlan
License: Apache-2.0
LicenseFiles: LICENSE
Section: kernel
Maintainer: Yousong Zhou <yszhou4tech@gmail.com>
Architecture: mipsel_24kc
Installed-Size: 1717
Filename: kmod-openvswitch-vxlan_4.14.167+2.11.1-2_mipsel_24kc.ipk
Size: 2563
SHA256sum: 52f9db20f85f0603cda9996faea50b096f2e4180c94c2b8ee28e524271b668cf
Description:  Open vSwitch VXLAN tunneling support (upstream)

Package: kmod-openvswitch
Version: 4.14.167+2.11.1-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-crc32c, kmod-mpls, kmod-nf-nat, kmod-nf-nat6, kmod-nf-conntrack, kmod-nf-conntrack6
Source: feeds/packages/net/openvswitch
SourceName: kmod-openvswitch
License: Apache-2.0
LicenseFiles: LICENSE
Section: kernel
Maintainer: Yousong Zhou <yszhou4tech@gmail.com>
Architecture: mipsel_24kc
Installed-Size: 55324
Filename: kmod-openvswitch_4.14.167+2.11.1-2_mipsel_24kc.ipk
Size: 55980
SHA256sum: 4f6380b4fecb1acc63c24b7a38005efb163bda6bf0f66273ec9c099fa969c624
Description:  Open vSwitch kernel datapath (upstream)

Package: kmod-owl-loader
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-owl-loader
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2416
Filename: kmod-owl-loader_4.14.167-1_mipsel_24kc.ipk
Size: 3290
SHA256sum: 024c01278f3c5a355240e1f6218873f5c652f34f12d233bdac8420b22748c297
Description:  Kernel module that helps to initialize certain Qualcomm
 Atheros' PCI(e) Wifi chips, which have the init data
 (which contains the PCI device ID for example) stored
 together with the calibration data in the file system.
 
 This is necessary for devices like the Cisco Meraki Z1.

Package: kmod-p54-common
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-lib-crc-ccitt
Source: package/kernel/mac80211
SourceName: kmod-p54-common
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 18936
Filename: kmod-p54-common_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 19742
SHA256sum: c6ce48d7a4275442f69ed3df6d663f5f77b84fd1c79c4d1da4701384429b5f35
Description:  Prism54 Drivers (COMMON)

Package: kmod-p54-pci
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-p54-common, p54-pci-firmware
Source: package/kernel/mac80211
SourceName: kmod-p54-pci
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 5931
Filename: kmod-p54-pci_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 6694
SHA256sum: 6daa55121b42bad980f42b4877c7d90bc1034a2fbdb108810bbc3f97a563a710
Description:  Prism54 Drivers (PCI)

Package: kmod-p54-usb
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core, kmod-p54-common, p54-usb-firmware
Source: package/kernel/mac80211
SourceName: kmod-p54-usb
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 7114
Filename: kmod-p54-usb_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 7905
SHA256sum: d1ee855786a545a32705bd2dd1cdec92311e70bbda8100f289344779f65a8be2
Description:  Prism54 Drivers (USB)

Package: kmod-parport-pc
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ppdev
Source: package/kernel/linux
SourceName: kmod-parport-pc
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 17909
Filename: kmod-parport-pc_4.14.167-1_mipsel_24kc.ipk
Size: 18689
SHA256sum: 79c914188f84d52c608f21bec2af48c421421143e8a096a8fecd7b3a1c1fbde4
Description:  Parallel port interface (PC-style) support

Package: kmod-pcnet32
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mii
Source: package/kernel/linux
SourceName: kmod-pcnet32
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 19047
Filename: kmod-pcnet32_4.14.167-1_mipsel_24kc.ipk
Size: 19820
SHA256sum: 05b68299ad6cf80233ba54111361ef950910fccc72581a7017f415c045d14d98
Description:  Kernel modules for AMD PCnet32 Ethernet adapters

Package: kmod-pf-ring
Version: 4.14.167+7.2.0-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: feeds/packages/kernel/pfring
SourceName: kmod-pf-ring
License: GPL-2.0
Section: kernel
Maintainer: Banglang Huang <banglang.huang@foxmail.com>
Architecture: mipsel_24kc
Installed-Size: 61265
Filename: kmod-pf-ring_4.14.167+7.2.0-1_mipsel_24kc.ipk
Size: 61211
SHA256sum: e3f309116e8d4196069f8ee34fbf8c1dffdc5cf0e92895ac87f9b4d8e053c5f3
Description:  Kernel module for libpf-ring package

Package: kmod-phy-broadcom
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-libphy, kmod-phylib-broadcom
Source: package/kernel/linux
SourceName: kmod-phy-broadcom
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2991
Filename: kmod-phy-broadcom_4.14.167-1_mipsel_24kc.ipk
Size: 3771
SHA256sum: 4c5f2c98b51c331e2a758c909d217387f357ef7be881d36891f3a1d348a61bbd
Description:  Currently supports the BCM5411, BCM5421, BCM5461, BCM5464, BCM5481,
 BCM5482 and BCM57780 PHYs.

Package: kmod-phy-realtek
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-libphy
Source: package/kernel/linux
SourceName: kmod-phy-realtek
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1474
Filename: kmod-phy-realtek_4.14.167-1_mipsel_24kc.ipk
Size: 2225
SHA256sum: 4fb63c46e3edc61e8e83f2d57f3e9962a866d4161caf88626ba7ac0da395143c
Description:  Supports the Realtek 821x PHY.

Package: kmod-phylib-broadcom
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-libphy
Source: package/kernel/linux
SourceName: kmod-phylib-broadcom
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2599
Filename: kmod-phylib-broadcom_4.14.167-1_mipsel_24kc.ipk
Size: 3334
SHA256sum: de007bd577d29a45a0c5eea1316b2ec553ddef31aa24c6ddd00869782b4b2f60
Description:  Broadcom Ethernet PHY library

Package: kmod-pktgen
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-pktgen
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 25281
Filename: kmod-pktgen_4.14.167-1_mipsel_24kc.ipk
Size: 25895
SHA256sum: c97f826890141e4ab3ccb1c7c99297da8f451f25a49b820f5e7dfe9fdab338d8
Description:  Kernel modules for the Network Packet Generator

Package: kmod-pmbus-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-pmbus-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9419
Filename: kmod-pmbus-core_4.14.167-1_mipsel_24kc.ipk
Size: 10163
SHA256sum: 244bfb0e45201122089cb8f3234804f3f46fc6318b1007ccf5290e7d20dde8b2
Description:  Kernel modules for Power Management Bus

Package: kmod-pmbus-zl6100
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core, kmod-pmbus-core
Source: package/kernel/linux
SourceName: kmod-pmbus-zl6100
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3814
Filename: kmod-pmbus-zl6100_4.14.167-1_mipsel_24kc.ipk
Size: 4571
SHA256sum: 933753dc082dbd7daf300c0e90630bc047c78c7f31fb5172ba175f717119e843
Description:  Intersil / Zilker Labs ZL6100 hardware monitoring

Package: kmod-ppdev
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-ppdev
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 22865
Filename: kmod-ppdev_4.14.167-1_mipsel_24kc.ipk
Size: 23526
SHA256sum: ca55c27cc8ec3eb0a564e39f330c82e433ad2f90db1ccdc69edd5b395dfa74bb
Description:  Parallel port support

Package: kmod-ppp-synctty
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ppp
Source: package/kernel/linux
SourceName: kmod-ppp-synctty
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4355
Filename: kmod-ppp-synctty_4.14.167-1_mipsel_24kc.ipk
Size: 5078
SHA256sum: 326faf9577134b553a039b65cf3f100b4ebb97c3c98ba09353ea83e95573e0ad
Description:  Kernel modules for PPP sync tty support

Package: kmod-ppp
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-crc-ccitt, kmod-slhc
Source: package/kernel/linux
SourceName: kmod-ppp
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 21623
Filename: kmod-ppp_4.14.167-1_mipsel_24kc.ipk
Size: 22296
SHA256sum: 12839c9f47fef4fc97de8611053a8f17db2ab8a5fcdeb1c2307b8b78c2fa34f5
Description:  Kernel modules for PPP support

Package: kmod-pppoa
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ppp, kmod-atm
Source: package/kernel/linux
SourceName: kmod-pppoa
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2949
Filename: kmod-pppoa_4.14.167-1_mipsel_24kc.ipk
Size: 3683
SHA256sum: 163949f4b91af51c92ace63943c4269e608aedede04b2bd6090453eb182b0fa2
Description:  Kernel modules for PPPoA (PPP over ATM) support

Package: kmod-pppoe
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ppp, kmod-pppox
Source: package/kernel/linux
SourceName: kmod-pppoe
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7166
Filename: kmod-pppoe_4.14.167-1_mipsel_24kc.ipk
Size: 7935
SHA256sum: 917ecfbe3f7a85dfcbc622603b5ed3683cbe404bceef851d1fbcee40c28ab70a
Description:  Kernel module for PPPoE (PPP over Ethernet) support

Package: kmod-pppol2tp
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ppp, kmod-pppox, kmod-l2tp
Source: package/kernel/linux
SourceName: kmod-pppol2tp
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9970
Filename: kmod-pppol2tp_4.14.167-1_mipsel_24kc.ipk
Size: 10732
SHA256sum: c4569189d7d8187bdfba70be616676c1b694daffa5810b5b92c66f3c18f03d10
Description:  Kernel modules for PPPoL2TP (PPP over L2TP) support

Package: kmod-pppox
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ppp
Source: package/kernel/linux
SourceName: kmod-pppox
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1564
Filename: kmod-pppox_4.14.167-1_mipsel_24kc.ipk
Size: 2317
SHA256sum: aad24525b1c022511c0b4a8338d42551859bdc62f128da6a4f61dc016020a253
Description:  Kernel helper module for PPPoE and PPTP support

Package: kmod-pps-gpio
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-pps
Source: package/kernel/linux
SourceName: kmod-pps-gpio
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2188
Filename: kmod-pps-gpio_4.14.167-1_mipsel_24kc.ipk
Size: 2992
SHA256sum: bd19d5f1dca8049b30a11dd7836044f75eea670347d56e308ff070b3bf74ec37
Description:  Support for a PPS source using GPIO. To be useful you must
 also register a platform device specifying the GPIO pin and
 other options, usually in your board setup.

Package: kmod-pps-ldisc
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-pps
Source: package/kernel/linux
SourceName: kmod-pps-ldisc
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2034
Filename: kmod-pps-ldisc_4.14.167-1_mipsel_24kc.ipk
Size: 2795
SHA256sum: 7faf2db66fa0e3b4fdfb0d8a05806533ee2af655f0c84a364adf0f408d37148c
Description:  Support for a PPS source connected with the CD (Carrier
 Detect) pin of your serial port.

Package: kmod-pps
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-pps
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5111
Filename: kmod-pps_4.14.167-1_mipsel_24kc.ipk
Size: 5899
SHA256sum: fc5717e8729c692c2b5edf1423564d9f27f483fa9709215a9134c3d700f51479
Description:  PPS (Pulse Per Second) is a special pulse provided by some GPS
 antennae. Userland can use it to get a high-precision time
 reference.

Package: kmod-pptp
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ppp, kmod-gre, kmod-pppox
Source: package/kernel/linux
SourceName: kmod-pptp
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5150
Filename: kmod-pptp_4.14.167-1_mipsel_24kc.ipk
Size: 5866
SHA256sum: 5f6dcad2d3018bf220ce99bf1455921b29866a3a2681dd0564b976d0321179df
Description:  PPtP support

Package: kmod-ptp
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-pps
Source: package/kernel/linux
SourceName: kmod-ptp
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7936
Filename: kmod-ptp_4.14.167-1_mipsel_24kc.ipk
Size: 8739
SHA256sum: ab2ad9bee26c405451d8b6b9cb2950889a0da983faa623db35e168333f61b958
Description:  The IEEE 1588 standard defines a method to precisely
 synchronize distributed clocks over Ethernet networks.

Package: kmod-pwm-mediatek-ramips
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-pwm-mediatek-ramips
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1565
Filename: kmod-pwm-mediatek-ramips_4.14.167-1_mipsel_24kc.ipk
Size: 2314
SHA256sum: 1d7490a79ec773937ea16707b52f7e056e946c74134c037df82705fafcc2c920
Description:  MT7628 PWM

Package: kmod-r6040
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-libphy
Source: package/kernel/linux
SourceName: kmod-r6040
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6820
Filename: kmod-r6040_4.14.167-1_mipsel_24kc.ipk
Size: 7580
SHA256sum: 543b2de17820163876554dc5fc90604a0fefbb7431d3c2319ab99ca6f48fd29c
Description:  Kernel modules for RDC Fast-Ethernet adapters.

Package: kmod-r8169
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mii, r8169-firmware
Source: package/kernel/linux
SourceName: kmod-r8169
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 29800
Filename: kmod-r8169_4.14.167-1_mipsel_24kc.ipk
Size: 30514
SHA256sum: b665d04b0fc3a9d221313334fa2e329afabce918251ce822be8ec171b5edf2db
Description:  Kernel modules for RealTek RTL-8169 PCI Gigabit Ethernet adapters

Package: kmod-random-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-random-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-random-core_4.14.167-1_mipsel_24kc.ipk
Size: 853
SHA256sum: 1b4d563806e8740215fddc2cc677d83f465116005b1e673b1ed661a9c2dc5102
Description:  Kernel module for the HW random number generator core infrastructure

Package: kmod-random-tpm
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-random-core, kmod-tpm
Source: package/kernel/linux
SourceName: kmod-random-tpm
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 754
Filename: kmod-random-tpm_4.14.167-1_mipsel_24kc.ipk
Size: 1528
SHA256sum: 3fd747fa92ddcf0b1e68fe4c89101a0ccecedba4a9a106ca00a2fd02ca89668c
Description:  Kernel module for the Random Number Generator
 in the Trusted Platform Module.

Package: kmod-regmap-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-regmap-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-regmap-core_4.14.167-1_mipsel_24kc.ipk
Size: 831
SHA256sum: aaa13184312c0c37a894da9a480ad3dd08b4e10aae5a7a604205942e81e00af3
Description:  Generic register map support

Package: kmod-regmap-i2c
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-regmap-core, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-regmap-i2c
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1624
Filename: kmod-regmap-i2c_4.14.167-1_mipsel_24kc.ipk
Size: 2387
SHA256sum: 7cb33e4ddf421263397c9ad991743f8ac403dbcc2754423ef378388fbae3b064
Description:  I2C register map support

Package: kmod-regmap-spi
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-regmap-core
Source: package/kernel/linux
SourceName: kmod-regmap-spi
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1273
Filename: kmod-regmap-spi_4.14.167-1_mipsel_24kc.ipk
Size: 2024
SHA256sum: 0b4e165312f8a770aa75018d389c9fbd22c9d63e7e3e608d617637c190dd2d27
Description:  SPI register map support

Package: kmod-rsi91x-sdio
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, kmod-mmc, kmod-rsi91x, rs9113-firmware
Source: package/kernel/mac80211
SourceName: kmod-rsi91x-sdio
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 9683
Filename: kmod-rsi91x-sdio_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 10461
SHA256sum: 5087b8d1d31f5d8ab3a02ce68d393a160cc44440860a6b6a16c44d6d04eb5ce2
Description:  Redpine Signals SDIO bus support

Package: kmod-rsi91x-usb
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core, kmod-mac80211, kmod-rsi91x, rs9113-firmware
Source: package/kernel/mac80211
SourceName: kmod-rsi91x-usb
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 6105
Filename: kmod-rsi91x-usb_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 6892
SHA256sum: 048630eeece141ae24cb7b9106bb73f2d72955a654977113bd5041c4f785f47c
Description:  Redpine Signals USB bus support

Package: kmod-rsi91x
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211, rs9113-firmware
Source: package/kernel/mac80211
SourceName: kmod-rsi91x
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 29253
Filename: kmod-rsi91x_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 29966
SHA256sum: 6ca892af44e23e6898a89f2259c747d143117c9934942c6ec463d37439a92d25
Description:  Redpine Signals Inc 91x WLAN driver support

Package: kmod-rt2400-pci
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rt2x00-pci, kmod-eeprom-93cx6
Source: package/kernel/mac80211
SourceName: kmod-rt2400-pci
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 7233
Filename: kmod-rt2400-pci_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 8038
SHA256sum: e6df375c49794eb29d83fe9078a9aa9f3ddc064fa1a75b8edc1633dbd942df36
Description:  Ralink Drivers for RT2x00 cards (RT2400 PCI)

Package: kmod-rt2500-pci
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rt2x00-pci, kmod-eeprom-93cx6
Source: package/kernel/mac80211
SourceName: kmod-rt2500-pci
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 8262
Filename: kmod-rt2500-pci_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 9040
SHA256sum: 4ebf72e987a865ca188695b8d2863a7252ce49bcb92ae6bb8dac6e93c73949e9
Description:  Ralink Drivers for RT2x00 cards (RT2500 PCI)

Package: kmod-rt2500-usb
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rt2x00-usb
Source: package/kernel/mac80211
SourceName: kmod-rt2500-usb
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 8894
Filename: kmod-rt2500-usb_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 9674
SHA256sum: ed2402b2b3949da5da73d5985af74398ea3abfd06078f8313422d25bde99a7e9
Description:  Ralink Drivers for RT2x00 cards (RT2500 USB)

Package: kmod-rt2800-lib
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rt2x00-lib, kmod-lib-crc-ccitt
Source: package/kernel/mac80211
SourceName: kmod-rt2800-lib
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 53632
Filename: kmod-rt2800-lib_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 53347
SHA256sum: 376b2c8c0e6fea7f7e1960c0273967c5a018f1bf3e84b5c9e83a16fbd97d14fd
Description:  Ralink Drivers for RT2x00 cards (rt2800 LIB)

Package: kmod-rt2800-mmio
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rt2800-lib, kmod-rt2x00-mmio
Source: package/kernel/mac80211
SourceName: kmod-rt2800-mmio
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 4007
Filename: kmod-rt2800-mmio_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 4781
SHA256sum: 9287a88f136ce6bba324c210f9c2fbf341ed9da008c4bcc162519a6854c08d63
Description:  Ralink Drivers for RT2x00 cards (RT28xx/RT3xxx MMIO)

Package: kmod-rt2800-pci
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rt2x00-pci, kmod-rt2800-lib, kmod-rt2800-mmio, kmod-eeprom-93cx6, rt2800-pci-firmware
Source: package/kernel/mac80211
SourceName: kmod-rt2800-pci
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 3629
Filename: kmod-rt2800-pci_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 4433
SHA256sum: eedeee116c64fb2a257edc3362cbc676ff369492db7377fa6eb823ef60ff2843
Description:  Ralink Drivers for RT2x00 cards (RT2860 PCI)

Package: kmod-rt2800-usb
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rt2x00-usb, kmod-rt2800-lib, kmod-lib-crc-ccitt, rt2800-usb-firmware
Source: package/kernel/mac80211
SourceName: kmod-rt2800-usb
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 6636
Filename: kmod-rt2800-usb_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 7460
SHA256sum: 5c2f2884f9e55f81c39479b375339e94ce6a00c504ecd49c23a8b96ea081bb99
Description:  Ralink Drivers for RT2x00 cards (RT2870 USB)

Package: kmod-rt2x00-lib
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211
Source: package/kernel/mac80211
SourceName: kmod-rt2x00-lib
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 22884
Filename: kmod-rt2x00-lib_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 23551
SHA256sum: e2da0fd49f61c1e64c16a52a4924ddd5cb5f12703e8994770a6be739f69236d2
Description:  Ralink Drivers for RT2x00 cards (LIB)

Package: kmod-rt2x00-mmio
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rt2x00-lib
Source: package/kernel/mac80211
SourceName: kmod-rt2x00-mmio
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 2303
Filename: kmod-rt2x00-mmio_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 3102
SHA256sum: e2a133df17e313b19784b85175f6db146f56897d1a3fd1b15440ccb0ec157acf
Description:  Ralink Drivers for RT2x00 cards (MMIO)

Package: kmod-rt2x00-pci
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rt2x00-mmio, kmod-rt2x00-lib
Source: package/kernel/mac80211
SourceName: kmod-rt2x00-pci
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 1806
Filename: kmod-rt2x00-pci_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 2605
SHA256sum: 18e6c6e69af2881e76df3c5fb072255630b0fc30f83d1038bbf703521faddd41
Description:  Ralink Drivers for RT2x00 cards (PCI)

Package: kmod-rt2x00-usb
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rt2x00-lib, kmod-usb-core
Source: package/kernel/mac80211
SourceName: kmod-rt2x00-usb
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 6277
Filename: kmod-rt2x00-usb_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 7104
SHA256sum: d2f591b0bf8ccea243b991de23152eec0c8d2a0144a796a59aee3370d5566f34
Description:  Ralink Drivers for RT2x00 cards (USB)

Package: kmod-rt61-pci
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rt2x00-pci, kmod-eeprom-93cx6, kmod-lib-crc-itu-t, rt61-pci-firmware
Source: package/kernel/mac80211
SourceName: kmod-rt61-pci
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 11988
Filename: kmod-rt61-pci_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 12783
SHA256sum: 672d26c89806b4673d11f2c530e4f4b1a383c2ba0f62c11989cd3cb0a0899b55
Description:  Ralink Drivers for RT2x00 cards (RT2x61 PCI)

Package: kmod-rt73-usb
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rt2x00-usb, kmod-lib-crc-itu-t, rt73-usb-firmware
Source: package/kernel/mac80211
SourceName: kmod-rt73-usb
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 11789
Filename: kmod-rt73-usb_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 12579
SHA256sum: 52a07ba392c9902b8126575fee944102920cf930837eca4b4078af9834c87645
Description:  Ralink Drivers for RT2x00 cards (RT73 USB)

Package: kmod-rtl8180
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-eeprom-93cx6, kmod-mac80211
Source: package/kernel/mac80211
SourceName: kmod-rtl8180
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 21335
Filename: kmod-rtl8180_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 22056
SHA256sum: 96b20adbe46e3d1ba9b80317946c7245c7ecd463e166ab4137aba089aeafa45f
Description:  Realtek Drivers for RTL818x devices (RTL8180 PCI)

Package: kmod-rtl8187
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-eeprom-93cx6, kmod-mac80211, kmod-usb-core
Source: package/kernel/mac80211
SourceName: kmod-rtl8187
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 17136
Filename: kmod-rtl8187_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 17923
SHA256sum: c7464471063579add34872b07e966e591f95e83e2fcf41c5261521a82659ee92
Description:  Realtek Drivers for RTL818x devices (RTL8187 USB)

Package: kmod-rtl8192c-common
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rtlwifi
Source: package/kernel/mac80211
SourceName: kmod-rtl8192c-common
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 18062
Filename: kmod-rtl8192c-common_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 18818
SHA256sum: 83ec1990eda933ed8f73b33d9055e497b97873e256a6e902bcba5223e80d55bf
Description:  Realtek RTL8192CE/RTL8192CU common support module

Package: kmod-rtl8192ce
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rtlwifi-pci, kmod-rtl8192c-common, rtl8192ce-firmware
Source: package/kernel/mac80211
SourceName: kmod-rtl8192ce
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 24314
Filename: kmod-rtl8192ce_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 24997
SHA256sum: 7e11905d04214b0eed42e58aec47cd09437197ce10a7f17776de2b5c17f851ec
Description:  Realtek RTL8192CE/RTL8188CE support

Package: kmod-rtl8192cu
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rtlwifi-usb, kmod-rtl8192c-common, rtl8192cu-firmware
Source: package/kernel/mac80211
SourceName: kmod-rtl8192cu
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 26327
Filename: kmod-rtl8192cu_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 26946
SHA256sum: 688c56ce1b5e80e11e2de873e67bde5d269ccda6afbd23cc813af73492c4e53d
Description:  Realtek RTL8192CU/RTL8188CU support

Package: kmod-rtl8192de
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rtlwifi-pci, rtl8192de-firmware
Source: package/kernel/mac80211
SourceName: kmod-rtl8192de
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 46123
Filename: kmod-rtl8192de_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 46855
SHA256sum: 72c93e2c9152cdd97466114345bdebcf09a8fa0dc98c156087e870bc2db79b28
Description:  Realtek RTL8192DE/RTL8188DE support

Package: kmod-rtl8192se
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rtlwifi-pci, rtl8192se-firmware
Source: package/kernel/mac80211
SourceName: kmod-rtl8192se
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 29591
Filename: kmod-rtl8192se_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 30340
SHA256sum: 95a38b607477909b682bfbc0172f2d8117651da42af7e76eae321f58e2f421cb
Description:  Realtek RTL8192SE/RTL8191SE support

Package: kmod-rtl8812au-ct
Version: 4.14.167+2018-11-16-661268fd-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-cfg80211, kmod-usb-core
Provides: kmod-rtl8812au
Source: package/kernel/rtl8812au-ct
SourceName: kmod-rtl8812au-ct
License: GPLv2
Section: kernel
Maintainer: Ben Greear <greearb@candelatech.com>
Architecture: mipsel_24kc
Installed-Size: 546720
Filename: kmod-rtl8812au-ct_4.14.167+2018-11-16-661268fd-1_mipsel_24kc.ipk
Size: 499420
SHA256sum: 10bcd499b0ff04bf8eda23b79b0a810638d523c7172ce8d211f1c74087d3cda4
Description:  Driver for Realtek 8812 AU devices comfast 912-ac, etc

Package: kmod-rtl8821ae
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rtlwifi-btcoexist, kmod-rtlwifi-pci, rtl8821ae-firmware
Source: package/kernel/mac80211
SourceName: kmod-rtl8821ae
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 73505
Filename: kmod-rtl8821ae_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 63362
SHA256sum: cf5c0670fb5a4ae8abe1980fd84474862e9acfec09f90420acfe19e990f8e685
Description:  Realtek RTL8821AE support

Package: kmod-rtl8xxxu
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core, kmod-mac80211
Source: package/kernel/mac80211
SourceName: kmod-rtl8xxxu
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 41327
Filename: kmod-rtl8xxxu_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 42580
SHA256sum: cb84e1a0643852b982a76b5edb5bbbcbcc7e4d80b49aee1059b532d02f153706
Description:  This is an alternative driver for various Realtek RTL8XXX
 parts written to utilize the Linux mac80211 stack.
 The driver is known to work with a number of RTL8723AU,
 RL8188CU, RTL8188RU, RTL8191CU, and RTL8192CU devices
 
 This driver is under development and has a limited feature
 set. In particular it does not yet support 40MHz channels
 and power management. However it should have a smaller
 memory footprint than the vendor drivers and benetifs
 from the in kernel mac80211 stack.
 
 It can coexist with drivers from drivers/staging/rtl8723au,
 drivers/staging/rtl8192u, and drivers/net/wireless/rtlwifi,
 but you will need to control which module you wish to load.
 
 RTL8XXXU_UNTESTED is enabled
 This option enables detection of Realtek 8723/8188/8191/8192 WiFi
 USB devices which have not been tested directly by the driver
 author or reported to be working by third parties.
 
 Please report your results!

Package: kmod-rtlwifi-btcoexist
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rtlwifi
Source: package/kernel/mac80211
SourceName: kmod-rtlwifi-btcoexist
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 56488
Filename: kmod-rtlwifi-btcoexist_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 56430
SHA256sum: 2395f600460179ef5e08267b7d54fe8ff28950779b42e1bd77c1cb0d538ceb08
Description:  Realtek BT coexist support

Package: kmod-rtlwifi-pci
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-rtlwifi
Source: package/kernel/mac80211
SourceName: kmod-rtlwifi-pci
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 12952
Filename: kmod-rtlwifi-pci_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 13702
SHA256sum: 80d358d1e9075ccee46f51613897f9084c628d6520c8533e789317b0262e5981
Description:  Realtek common driver part (PCI support)

Package: kmod-rtlwifi-usb
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core, kmod-rtlwifi
Source: package/kernel/mac80211
SourceName: kmod-rtlwifi-usb
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 7287
Filename: kmod-rtlwifi-usb_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 8117
SHA256sum: d7b2ce070727cb3b69395ada13e28b7ef0c0f10be9abfd5c7391a861d1d1043d
Description:  Realtek common driver part (USB support)

Package: kmod-rtlwifi
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mac80211
Source: package/kernel/mac80211
SourceName: kmod-rtlwifi
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 32915
Filename: kmod-rtlwifi_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 33617
SHA256sum: 4a0fa3d5699f4510db9f3734730905cbf54df09891411c4fd2731712243362d2
Description:  Realtek common driver part

Package: kmod-sched-act-vlan
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sched-core
Source: package/kernel/linux
SourceName: kmod-sched-act-vlan
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2805
Filename: kmod-sched-act-vlan_4.14.167-1_mipsel_24kc.ipk
Size: 3542
SHA256sum: 4d4b3149fa2ab753674bb13a8dae52d35c22c290469d1673fdbf6578286b9b20
Description:  Allows to configure rules to push or pop vlan headers.

Package: kmod-sched-bpf
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-sched-bpf
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6698
Filename: kmod-sched-bpf_4.14.167-1_mipsel_24kc.ipk
Size: 7483
SHA256sum: 11ad687e2490ee09abb3651d91f2a358207d29f0c687ba9dd327b69d25c717bf
Description:  Traffic shaper support for Berkeley Packet Filter

Package: kmod-sched-cake
Version: 4.14.167+2019-03-12-057c7388-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ipt-conntrack
Source: package/kernel/kmod-sched-cake
SourceName: kmod-sched-cake
Section: kernel
Maintainer: Kevin Darbyshire-Bryant <ldir@darbyshire-bryant.me.uk>
Architecture: mipsel_24kc
Installed-Size: 17734
Filename: kmod-sched-cake_4.14.167+2019-03-12-057c7388-1_mipsel_24kc.ipk
Size: 18566
SHA256sum: 8036bb57b2dd1fe9e39db20c1df4f9c4c9139610e1919f3ef9458e6085f77cf0
Description:  Common Applications Kept Enhanced fq_codel/blue derived shaper

Package: kmod-sched-connmark
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sched-core, kmod-ipt-core, kmod-ipt-conntrack-extra
Source: package/kernel/linux
SourceName: kmod-sched-connmark
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2512
Filename: kmod-sched-connmark_4.14.167-1_mipsel_24kc.ipk
Size: 3249
SHA256sum: 95f9bb9b3b9337e06ab7b92944b0351cf7590a770143a47c2b81800c7c41dc2e
Description:  Traffic shaper conntrack mark support

Package: kmod-sched-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-sched-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 49204
Filename: kmod-sched-core_4.14.167-1_mipsel_24kc.ipk
Size: 49985
SHA256sum: c04360c82f1ccd0530d654e488800ca5eb2754c8f78c6de04fd008ddb906f4af
Description:  Core kernel scheduler support for IP traffic

Package: kmod-sched-ctinfo
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sched-core, kmod-ipt-core, kmod-ipt-conntrack-extra
Source: package/kernel/linux
SourceName: kmod-sched-ctinfo
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3470
Filename: kmod-sched-ctinfo_4.14.167-1_mipsel_24kc.ipk
Size: 4210
SHA256sum: fe92065b7d53edba1d3b05a58ded9737373d06ba9fc5b976c04e6c408e3cfbfa
Description:  Traffic shaper ctinfo support

Package: kmod-sched-flower
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sched-core
Source: package/kernel/linux
SourceName: kmod-sched-flower
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 8736
Filename: kmod-sched-flower_4.14.167-1_mipsel_24kc.ipk
Size: 9520
SHA256sum: 64ecfa1724fb621c14f918c83ad68b851c4d8378fef272c9f59f05217ffe1ac9
Description:  Allows to classify packets based on a configurable combination of packet keys and masks.

Package: kmod-sched-ipset
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sched-core, kmod-ipt-ipset
Source: package/kernel/linux
SourceName: kmod-sched-ipset
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1470
Filename: kmod-sched-ipset_4.14.167-1_mipsel_24kc.ipk
Size: 2237
SHA256sum: 3095dbd30b1eb942a57d0ab41bc2bc6edc924f31350ca7ecb73f7e988df7dd18
Description:  Traffic shaper ipset support

Package: kmod-sched-mqprio
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sched-core
Source: package/kernel/linux
SourceName: kmod-sched-mqprio
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3764
Filename: kmod-sched-mqprio_4.14.167-1_mipsel_24kc.ipk
Size: 4530
SHA256sum: beba8e95d1c1013dddeb00642f68953976cbb75240e684ff044592788d061c76
Description:  This scheduler allows QOS to be offloaded on NICs that have support for offloading QOS schedulers.

Package: kmod-sched
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sched-core, kmod-ipt-core, kmod-lib-crc32c
Source: package/kernel/linux
SourceName: kmod-sched
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 51523
Filename: kmod-sched_4.14.167-1_mipsel_24kc.ipk
Size: 52236
SHA256sum: bdf9fbea2c6b5f582925435547099fafb24fb27d425bd0f56b671fdd4d6ef1df
Description:  Extra kernel schedulers modules for IP traffic

Package: kmod-scsi-cdrom
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-scsi-core
Source: package/kernel/linux
SourceName: kmod-scsi-cdrom
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 25888
Filename: kmod-scsi-cdrom_4.14.167-1_mipsel_24kc.ipk
Size: 26486
SHA256sum: 22885e8376129254d220ab910abbbfdb22644a2e6d5e01814bfc3f45f679b2d3
Description:  Kernel support for CD / DVD drives

Package: kmod-scsi-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-scsi-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 79819
Filename: kmod-scsi-core_4.14.167-1_mipsel_24kc.ipk
Size: 80070
SHA256sum: 2dcc5d58a2c5ac8435f3905dc6484f0ea28cd14a3abf2566554afbf12c25c477
Description:  SCSI device support

Package: kmod-scsi-generic
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-scsi-core
Source: package/kernel/linux
SourceName: kmod-scsi-generic
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 16269
Filename: kmod-scsi-generic_4.14.167-1_mipsel_24kc.ipk
Size: 16975
SHA256sum: a7819235589284acfac4b63a53c4d383ffc5c97d157f0bedf7948f961d314cec
Description:  Kernel support for SCSI generic

Package: kmod-scsi-tape
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-scsi-core
Source: package/kernel/linux
SourceName: kmod-scsi-tape
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 29994
Filename: kmod-scsi-tape_4.14.167-1_mipsel_24kc.ipk
Size: 30618
SHA256sum: 2cc27f1ea72a0fae7d0cab752752812a7d2449fd33f4b685a15c26aeee5d75a5
Description:  Kernel support for scsi tape drives

Package: kmod-sctp
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-crc32c, kmod-crypto-md5, kmod-crypto-hmac
Source: package/kernel/linux
SourceName: kmod-sctp
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 117123
Filename: kmod-sctp_4.14.167-1_mipsel_24kc.ipk
Size: 117141
SHA256sum: ee2738c42f5056664a2882b22b38e84392627956218d7dc13250d75fba4d2f07
Description:  Kernel modules for SCTP protocol support

Package: kmod-sdhci-mt7620
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mmc
Source: package/kernel/linux
SourceName: kmod-sdhci-mt7620
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9641
Filename: kmod-sdhci-mt7620_4.14.167-1_mipsel_24kc.ipk
Size: 10379
SHA256sum: 5f016fa75c1045ce3422f4ac2505b1f516e543cc161e9e5f1ab7f3078cd07fe3
Description:  MT7620 SDCI

Package: kmod-sdhci
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mmc
Source: package/kernel/linux
SourceName: kmod-sdhci
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 20253
Filename: kmod-sdhci_4.14.167-1_mipsel_24kc.ipk
Size: 20919
SHA256sum: 6e5791a721e0f369a0602d87904dac97dadb39c83e17f58ab301d3884c7f81ba
Description:  Kernel support for SDHCI Hosts

Package: kmod-serial-8250-exar
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-serial-8250
Source: package/kernel/linux
SourceName: kmod-serial-8250-exar
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2736
Filename: kmod-serial-8250-exar_4.14.167-1_mipsel_24kc.ipk
Size: 3468
SHA256sum: 63b7049f8c3490aa69ea7409869fc2a5239a0893ea3f33ada59abd08a73fab36
Description:  Kernel module for Exar serial ports

Package: kmod-serial-8250
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-serial-8250
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 11627
Filename: kmod-serial-8250_4.14.167-1_mipsel_24kc.ipk
Size: 12368
SHA256sum: 6994b7d5cbe9a2c15bed9825b453f730d0784419c1e4068edeb8290805665f15
Description:  Kernel module for 8250 UART based serial ports

Package: kmod-siit
Version: 4.14.167+1.2-3
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: feeds/packages/net/siit
SourceName: kmod-siit
License: GPL-2.0-or-later
Section: kernel
Maintainer: Vladimir Ulrich <admin@evl.su>
Architecture: mipsel_24kc
Installed-Size: 5192
Filename: kmod-siit_4.14.167+1.2-3_mipsel_24kc.ipk
Size: 5976
SHA256sum: f8c3e1d50990218f3fb491dc73c303fca471e42aedd8530883c4da51b4cdeab2
Description:  Stateless IP ICMP Translation Algorithm

Package: kmod-sis190
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mii
Source: package/kernel/linux
SourceName: kmod-sis190
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10173
Filename: kmod-sis190_4.14.167-1_mipsel_24kc.ipk
Size: 10935
SHA256sum: d0fc385bd953503ba095ecc78e650c802129356062913f8f8209a2c3465cdf82
Description:  SiS 190 Fast/Gigabit Ethernet support

Package: kmod-sis900
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mii
Source: package/kernel/linux
SourceName: kmod-sis900
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 12065
Filename: kmod-sis900_4.14.167-1_mipsel_24kc.ipk
Size: 12799
SHA256sum: 537d8c93945f469d6797d1605dce230cf6e53b45922ba6bf99708ae2db1c4d39
Description:  Kernel modules for Sis 900 Ethernet adapters.

Package: kmod-sit
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-iptunnel, kmod-iptunnel4
Source: package/kernel/linux
SourceName: kmod-sit
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10943
Filename: kmod-sit_4.14.167-1_mipsel_24kc.ipk
Size: 11713
SHA256sum: 199e304b53275501c76f733a68ace39b1089408318f41046dac5668a893078e7
Description:  Kernel modules for IPv6-in-IPv4 tunnelling

Package: kmod-skge
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-skge
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 17440
Filename: kmod-skge_4.14.167-1_mipsel_24kc.ipk
Size: 18149
SHA256sum: 5ee31d0d806c5250d8ff278e3dc9200b95ff33f7319bbc2b14fd80da41fbe00c
Description:  SysKonnect Yukon support

Package: kmod-sky2
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-sky2
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 26536
Filename: kmod-sky2_4.14.167-1_mipsel_24kc.ipk
Size: 27241
SHA256sum: 601789c96e43cf53b6b0589ab86e33f77f429660f7e67a6503d4344032820db9
Description:  This driver supports Gigabit Ethernet adapters based on the
 Marvell Yukon 2 chipset:
 Marvell 88E8021/88E8022/88E8035/88E8036/88E8038/88E8050/88E8052/
 88E8053/88E8055/88E8061/88E8062, SysKonnect SK-9E21D/SK-9S21
 
 There is companion driver for the older Marvell Yukon and
 Genesis based adapters: skge.

Package: kmod-slhc
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-crc-ccitt
Source: package/kernel/linux
SourceName: kmod-slhc
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3887
Filename: kmod-slhc_4.14.167-1_mipsel_24kc.ipk
Size: 4604
SHA256sum: 67e808d37aeeacac306c098d867d7f16ebc11dbd40bc5c100a6c56f1801323ed
Description:  Serial Line Header Compression

Package: kmod-slip
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-slhc
Source: package/kernel/linux
SourceName: kmod-slip
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7682
Filename: kmod-slip_4.14.167-1_mipsel_24kc.ipk
Size: 8440
SHA256sum: 6537518ff6b9db09e1222b77379ddfe20ab2e10876ed05d8effc0baf7ebf5145
Description:  Kernel modules for SLIP support

Package: kmod-softdog
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-softdog
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1898
Filename: kmod-softdog_4.14.167-1_mipsel_24kc.ipk
Size: 2615
SHA256sum: db365726a1dd9e8380a979d30eae6d00ea611f824d4848d90e9df0d16d55d091
Description:  Software watchdog driver

Package: kmod-solos-pci
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-atm
Source: package/kernel/linux
SourceName: kmod-solos-pci
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 12582
Filename: kmod-solos-pci_4.14.167-1_mipsel_24kc.ipk
Size: 13325
SHA256sum: ad0626784bee411586c235fa935da01f881058495afaa010a3f4e43e8d0355bf
Description:  Kernel module for Traverse Technologies' Solos PCI cards
 and Geos ADSL2+ x86 motherboard

Package: kmod-sound-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-input-core
Source: package/kernel/linux
SourceName: kmod-sound-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 134858
Filename: kmod-sound-core_4.14.167-1_mipsel_24kc.ipk
Size: 135315
SHA256sum: d6aa35989a730cf2d2017ee4d2f044a83d1371bd33d5db135e4da9176cd186f1
Description:  Kernel modules for sound support

Package: kmod-sound-dummy
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core
Source: package/kernel/linux
SourceName: kmod-sound-dummy
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6255
Filename: kmod-sound-dummy_4.14.167-1_mipsel_24kc.ipk
Size: 7057
SHA256sum: 4879641b7f2dc08fe89291b00241bc6c8cc5f2ffde429b330d13168c8eb568fb
Description:  Null sound output driver (sink)

Package: kmod-sound-ens1371
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ac97, kmod-sound-core
Source: package/kernel/linux
SourceName: kmod-sound-ens1371
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9001
Filename: kmod-sound-ens1371_4.14.167-1_mipsel_24kc.ipk
Size: 9785
SHA256sum: 4631000b7fab365e4dcef5fe972223c86f77a8a295af67ac968fb485578be85f
Description:  support for (Creative) Ensoniq AudioPCI 1371 chips

Package: kmod-sound-hda-codec-analog
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core, kmod-sound-hda-core
Source: package/kernel/linux
SourceName: kmod-sound-hda-codec-analog
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4542
Filename: kmod-sound-hda-codec-analog_4.14.167-1_mipsel_24kc.ipk
Size: 5304
SHA256sum: 8a776379d71e7899c8aa9f0b63fa298a1c18e88cfc11e0752a85911eea9459c9
Description:  Kernel modules for HD Audio Analog Devices codec support

Package: kmod-sound-hda-codec-ca0110
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core, kmod-sound-hda-core
Source: package/kernel/linux
SourceName: kmod-sound-hda-codec-ca0110
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1312
Filename: kmod-sound-hda-codec-ca0110_4.14.167-1_mipsel_24kc.ipk
Size: 2107
SHA256sum: 44b09e62a10449ba28ede5e50281ed88ed7ce48f6069846a79236e449331a9db
Description:  Kernel modules for HD Audio Creative CA0110 codec support

Package: kmod-sound-hda-codec-ca0132
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core, kmod-sound-hda-core
Source: package/kernel/linux
SourceName: kmod-sound-hda-codec-ca0132
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9746
Filename: kmod-sound-hda-codec-ca0132_4.14.167-1_mipsel_24kc.ipk
Size: 10557
SHA256sum: 66f35e955d663fe1736473a1c77561f9f6cd706e797a2594ea7efdb35ced6031
Description:  Kernel modules for HD Audio Creative CA0132 codec support

Package: kmod-sound-hda-codec-cirrus
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core, kmod-sound-hda-core
Source: package/kernel/linux
SourceName: kmod-sound-hda-codec-cirrus
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4852
Filename: kmod-sound-hda-codec-cirrus_4.14.167-1_mipsel_24kc.ipk
Size: 5602
SHA256sum: de98adaf0f11bbd87a022cdad6bca53b322d185bd223328a68386d031b872663
Description:  Kernel modules for HD Audio Cirrus Logic codec support

Package: kmod-sound-hda-codec-cmedia
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core, kmod-sound-hda-core
Source: package/kernel/linux
SourceName: kmod-sound-hda-codec-cmedia
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1641
Filename: kmod-sound-hda-codec-cmedia_4.14.167-1_mipsel_24kc.ipk
Size: 2428
SHA256sum: cf7efb6b820bc1ccd1d80c2d7a9a1a19ca8d08ac00b0d04b4b5578b64b827ffa
Description:  Kernel modules for HD Audio C-Media codec support

Package: kmod-sound-hda-codec-conexant
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core, kmod-sound-hda-core
Source: package/kernel/linux
SourceName: kmod-sound-hda-codec-conexant
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5572
Filename: kmod-sound-hda-codec-conexant_4.14.167-1_mipsel_24kc.ipk
Size: 6340
SHA256sum: 7058ac64a678f116979d7206097acdfc4b87613906debaba45efbeb2ea019e97
Description:  Kernel modules for HD Audio Conexant codec support

Package: kmod-sound-hda-codec-hdmi
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core, kmod-sound-hda-core
Source: package/kernel/linux
SourceName: kmod-sound-hda-codec-hdmi
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 20800
Filename: kmod-sound-hda-codec-hdmi_4.14.167-1_mipsel_24kc.ipk
Size: 21433
SHA256sum: 113a3a11b757cbc4af062d86d3762c0f9619a9b2f7c7aa1f3824b841bd040722
Description:  Kernel modules for HD Audio HDMI codec support

Package: kmod-sound-hda-codec-idt
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core, kmod-sound-hda-core
Source: package/kernel/linux
SourceName: kmod-sound-hda-codec-idt
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 14861
Filename: kmod-sound-hda-codec-idt_4.14.167-1_mipsel_24kc.ipk
Size: 15557
SHA256sum: dd72020386babc8728e371229fa769f9690ca9384fbff528b72f6302e9bf939e
Description:  Kernel modules for HD Audio Sigmatel IDT codec support

Package: kmod-sound-hda-codec-realtek
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core, kmod-sound-hda-core
Source: package/kernel/linux
SourceName: kmod-sound-hda-codec-realtek
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 25292
Filename: kmod-sound-hda-codec-realtek_4.14.167-1_mipsel_24kc.ipk
Size: 25958
SHA256sum: 13d2e9ec9b49e28e52c83c5604b5b2b16d93712f1d0fa75cfce4c9455f8267d1
Description:  Kernel modules for Intel HDA Realtek codec support

Package: kmod-sound-hda-codec-si3054
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core, kmod-sound-hda-core
Source: package/kernel/linux
SourceName: kmod-sound-hda-codec-si3054
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2411
Filename: kmod-sound-hda-codec-si3054_4.14.167-1_mipsel_24kc.ipk
Size: 3169
SHA256sum: 1a8576a5bec069b65fd3f9caa7c14a23f188587a5d049e0da0d7c336872e4ece
Description:  Kernel modules for HD Audio Silicon Labs 3054 codec support

Package: kmod-sound-hda-codec-via
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core, kmod-sound-hda-core
Source: package/kernel/linux
SourceName: kmod-sound-hda-codec-via
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5465
Filename: kmod-sound-hda-codec-via_4.14.167-1_mipsel_24kc.ipk
Size: 6224
SHA256sum: 1b8cf1f948b3c0b617a99b85b94096359de97643b33cb2609a39ebdc1e9a85cd
Description:  Kernel modules for HD Audio VIA codec support

Package: kmod-sound-hda-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core, kmod-regmap-core
Source: package/kernel/linux
SourceName: kmod-sound-hda-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 88958
Filename: kmod-sound-hda-core_4.14.167-1_mipsel_24kc.ipk
Size: 89630
SHA256sum: 4cea657390cfa579c3288b1f2f8b11eebc4bf3f64edde54af7ff0cd63f6233ce
Description:  Kernel modules for HD Audio sound support

Package: kmod-sound-hda-intel
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core, kmod-sound-hda-core
Source: package/kernel/linux
SourceName: kmod-sound-hda-intel
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9205
Filename: kmod-sound-hda-intel_4.14.167-1_mipsel_24kc.ipk
Size: 9978
SHA256sum: 435e51b90fe4431c6cb79a1aaa8b38b47f9f04397fbaeb6be3464a2f248305a0
Description:  Kernel modules for HD Audio Intel driver support

Package: kmod-sound-i8x0
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ac97, kmod-sound-core
Source: package/kernel/linux
SourceName: kmod-sound-i8x0
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 14237
Filename: kmod-sound-i8x0_4.14.167-1_mipsel_24kc.ipk
Size: 15055
SHA256sum: 68732af91d4ae9ab090764183a6068368ce2ad796f24a0e0fc3a4c86225b7ba8
Description:  support for the integrated AC97 sound device on motherboards
 with Intel/SiS/nVidia/AMD chipsets, or ALi chipsets using
 the M5455 Audio Controller.

Package: kmod-sound-mpu401
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core
Source: package/kernel/linux
SourceName: kmod-sound-mpu401
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3449
Filename: kmod-sound-mpu401_4.14.167-1_mipsel_24kc.ipk
Size: 4214
SHA256sum: 5596df804ab9a0b416a809adf8f80cb347b70aa27e65284e63fb67016854febb
Description:  support for MIDI ports compatible with the Roland MPU-401
 interface in UART mode.

Package: kmod-sound-mt7620
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-soc-core, kmod-regmap-i2c, kmod-dma-ralink, kmod-sound-core
Source: package/kernel/linux
SourceName: kmod-sound-mt7620
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 18535
Filename: kmod-sound-mt7620_4.14.167-1_mipsel_24kc.ipk
Size: 19276
SHA256sum: 99554e192acfb5362b187408c23c326d3e5e3d0d5f91507c03c32d60029ee86a
Description:  Alsa modules for ralink i2s controller.

Package: kmod-sound-seq
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-sound-core
Source: package/kernel/linux
SourceName: kmod-sound-seq
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 31443
Filename: kmod-sound-seq_4.14.167-1_mipsel_24kc.ipk
Size: 32147
SHA256sum: 11641c9e8707301ce6c3b3376a51f4a0675243f8cbe6f632e8d2c4794d12ed09
Description:  Kernel modules for sequencer support

Package: kmod-sound-soc-ac97
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ac97, kmod-sound-soc-core, kmod-sound-core
Source: package/kernel/linux
SourceName: kmod-sound-soc-ac97
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1271
Filename: kmod-sound-soc-ac97_4.14.167-1_mipsel_24kc.ipk
Size: 2039
SHA256sum: 7c760b329000862821a511e949e25a960b2977e606030529122caa337934f3b7
Description:  AC97 Codec support

Package: kmod-sound-soc-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-regmap-core, kmod-ac97, kmod-sound-core
Source: package/kernel/linux
SourceName: kmod-sound-soc-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 63620
Filename: kmod-sound-soc-core_4.14.167-1_mipsel_24kc.ipk
Size: 64010
SHA256sum: af1bf9207ef1d831f4bc4ba711cb6f6c625bf3177e36924c823589b700036df3
Description:  SoC sound support

Package: kmod-sound-via82xx
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-ac97, kmod-sound-mpu401, kmod-sound-core
Source: package/kernel/linux
SourceName: kmod-sound-via82xx
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 11211
Filename: kmod-sound-via82xx_4.14.167-1_mipsel_24kc.ipk
Size: 12030
SHA256sum: 5dfd55f15ae4d4791ea4dc43cad7074eb627dfb898df5be9214b61d90db3b202
Description:  support for the integrated AC97 sound device on motherboards
 with VIA chipsets.

Package: kmod-spi-bitbang
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-spi-bitbang
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2053
Filename: kmod-spi-bitbang_4.14.167-1_mipsel_24kc.ipk
Size: 2816
SHA256sum: c7a3511fd66b9365af20304a072f23f1739a15e237bd12098b8d93fdfe955b46
Description:  This package contains the SPI bitbanging library

Package: kmod-spi-dev
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-spi-dev
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4594
Filename: kmod-spi-dev_4.14.167-1_mipsel_24kc.ipk
Size: 5308
SHA256sum: 7a19517e1a2b2904cda0f808b15385d908c33c5e8318f8684cfafc61f3cdd8f9
Description:  This package contains the user mode SPI device driver

Package: kmod-spi-gpio-custom
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-spi-bitbang, kmod-spi-gpio, kmod-spi-dev
Source: package/kernel/spi-gpio-custom
SourceName: kmod-spi-gpio-custom
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2522
Filename: kmod-spi-gpio-custom_4.14.167-1_mipsel_24kc.ipk
Size: 3298
SHA256sum: 84d6a9e01785db652fb630a1a0db961d29748cf6af39d932e61450ee736adc7c
Description:  Kernel module for register a custom spi-gpio platform device.

Package: kmod-spi-gpio
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-spi-bitbang
Source: package/kernel/linux
SourceName: kmod-spi-gpio
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3393
Filename: kmod-spi-gpio_4.14.167-1_mipsel_24kc.ipk
Size: 4139
SHA256sum: 1642e194b37f3a158e30377dbd200e905472a95e789b06c8068cf69af6a74fcc
Description:  This package contains the GPIO-based bitbanging SPI Master

Package: kmod-spi-ks8995
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-spi-ks8995
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2843
Filename: kmod-spi-ks8995_4.14.167-1_mipsel_24kc.ipk
Size: 3582
SHA256sum: 2a7817b61402876fbf00520da695f5a7253bf436e2c373d94277aae7653330ac
Description:  Kernel module for Micrel/Kendin KS8995 ethernet switch

Package: kmod-ssb
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-ssb
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 19778
Filename: kmod-ssb_4.14.167-1_mipsel_24kc.ipk
Size: 20533
SHA256sum: c8d9a6fa2bb32cf8b0969e408496dc5e27c82b836d3ad8eef790875e5b0692f0
Description:  Silicon Sonics Backplane glue code.

Package: kmod-swconfig
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-libphy
Source: package/kernel/linux
SourceName: kmod-swconfig
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 189
Filename: kmod-swconfig_4.14.167-1_mipsel_24kc.ipk
Size: 920
SHA256sum: 46ce86f264ea2f6777c353c512f4b577d95f12bb685177ca2ab85d3cc3949cd8
Description:  Switch configuration API module

Package: kmod-switch-ip17xx
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-swconfig
Source: package/kernel/linux
SourceName: kmod-switch-ip17xx
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6019
Filename: kmod-switch-ip17xx_4.14.167-1_mipsel_24kc.ipk
Size: 6766
SHA256sum: b0ffbf0c24800fcd044363647002b25d57fcf43d85d51069d745da4c846a7413
Description:  IC+ IP175C/IP178C switch support

Package: kmod-switch-mvsw61xx
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-swconfig
Source: package/kernel/linux
SourceName: kmod-switch-mvsw61xx
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5165
Filename: kmod-switch-mvsw61xx_4.14.167-1_mipsel_24kc.ipk
Size: 5919
SHA256sum: df9d9fd8ca18e0af96069668b98c29eae424af344b144cb803389af92101e972
Description:  Marvell 88E61xx switch support

Package: kmod-switch-rtl8306
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-swconfig
Source: package/kernel/linux
SourceName: kmod-switch-rtl8306
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6348
Filename: kmod-switch-rtl8306_4.14.167-1_mipsel_24kc.ipk
Size: 7076
SHA256sum: 3d13cda9fdd235966aaa88fc9b4df0a307dc2bbaa1252dd3e7fb72aa7ce35e57
Description:  Realtek RTL8306S switch support

Package: kmod-switch-rtl8366-smi
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-swconfig
Source: package/kernel/linux
SourceName: kmod-switch-rtl8366-smi
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7064
Filename: kmod-switch-rtl8366-smi_4.14.167-1_mipsel_24kc.ipk
Size: 7820
SHA256sum: 84a37f0711626c07ce522c2f96d37b98f99002e70f031b055846b3064fd342c5
Description:  Realtek RTL8366 SMI switch interface support

Package: kmod-switch-rtl8366rb
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-switch-rtl8366-smi
Source: package/kernel/linux
SourceName: kmod-switch-rtl8366rb
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5860
Filename: kmod-switch-rtl8366rb_4.14.167-1_mipsel_24kc.ipk
Size: 6613
SHA256sum: 0c26d5a75913dabc26edc336e455fa33ad3454add38ac5e59b40dbb1cddb7e47
Description:  Realtek RTL8366RB switch support

Package: kmod-switch-rtl8366s
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-switch-rtl8366-smi
Source: package/kernel/linux
SourceName: kmod-switch-rtl8366s
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5608
Filename: kmod-switch-rtl8366s_4.14.167-1_mipsel_24kc.ipk
Size: 6368
SHA256sum: 83d98f217cdba4edf07ad5d11629fa331a1866d8c639221be318ab16a3c6eb01
Description:  Realtek RTL8366S switch support

Package: kmod-switch-rtl8367b
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-switch-rtl8366-smi
Source: package/kernel/linux
SourceName: kmod-switch-rtl8367b
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 8158
Filename: kmod-switch-rtl8367b_4.14.167-1_mipsel_24kc.ipk
Size: 8914
SHA256sum: a8a951bf3a33b63137b969f365f957b57ae7787e723273f633a95cd27753f3fa
Description:  Realtek RTL8367R/B switch support

Package: kmod-tcp-bbr
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-tcp-bbr
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4728
Filename: kmod-tcp-bbr_4.14.167-1_mipsel_24kc.ipk
Size: 5564
SHA256sum: 819f2ef3e8fe096b8583466dfd318f65c9968e043d2ebfff8761d9eb571f24cc
Description:  Kernel module for BBR (Bottleneck Bandwidth and RTT) TCP congestion
 control. It requires the fq ("Fair Queue") pacing packet scheduler.
 For kernel 4.13+, TCP internal pacing is implemented as fallback.

Package: kmod-tg3
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-libphy, kmod-ptp
Source: package/kernel/linux
SourceName: kmod-tg3
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 76730
Filename: kmod-tg3_4.14.167-1_mipsel_24kc.ipk
Size: 77358
SHA256sum: ce30a4f2a52ec4698870eceba9bf77fcf3438d055b4f724f4d5e4c0622054707
Description:  Kernel modules for Broadcom Tigon3 Gigabit Ethernet adapters

Package: kmod-tpm-i2c-atmel
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-tpm, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-tpm-i2c-atmel
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1585
Filename: kmod-tpm-i2c-atmel_4.14.167-1_mipsel_24kc.ipk
Size: 2347
SHA256sum: 984b4c4f9c47e793981f3e0feb9429b8db529b765d2f75a336c0ade774b1e224
Description:  This enables the TPM Interface Specification 1.2 Interface (I2C - Atmel)

Package: kmod-tpm-i2c-infineon
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-tpm, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-tpm-i2c-infineon
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3997
Filename: kmod-tpm-i2c-infineon_4.14.167-1_mipsel_24kc.ipk
Size: 4760
SHA256sum: eae1afcb80322591ecd59e0eac68a0ab750d8a189e8576601dcdbbc54f79e011
Description:  This enables the TPM Interface Specification 1.2 Interface (I2C - Infineon)

Package: kmod-tpm
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-tpm
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 23995
Filename: kmod-tpm_4.14.167-1_mipsel_24kc.ipk
Size: 24647
SHA256sum: ed331999b32afe40a75c5bf8feb9783e4bf60345f9e17de10df544928f8a879b
Description:  This enables TPM Hardware Support.

Package: kmod-trelay
Version: 4.14.167+0.1-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/trelay
SourceName: kmod-trelay
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3024
Filename: kmod-trelay_4.14.167+0.1-2_mipsel_24kc.ipk
Size: 3945
SHA256sum: f06b12ed1e7d1fbc9bf3d81c5ecd68ec1c5262479e740caad971c9d8ce8785ac
Description:  trelay relays ethernet packets between two devices (similar to a bridge), but
 without any MAC address checks. This makes it possible to bridge client mode
 or ad-hoc mode wifi devices to ethernet VLANs, assuming the remote end uses
 the same source MAC address as the device that packets are supposed to exit
 from.

Package: kmod-tulip
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mii
Source: package/kernel/linux
SourceName: kmod-tulip
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 66584
Filename: kmod-tulip_4.14.167-1_mipsel_24kc.ipk
Size: 67358
SHA256sum: e1459330446f0fc67f71a6fde787071a5c1e6dc314b0a9cff0fc79cbe9d42719
Description:  Kernel modules for the Tulip family of network cards,
 including DECchip Tulip, DIGITAL EtherWORKS, Winbond W89c840,
 Davicom DM910x/DM980x and ULi M526x controller support.

Package: kmod-tun
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-tun
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 15694
Filename: kmod-tun_4.14.167-1_mipsel_24kc.ipk
Size: 16426
SHA256sum: 56a37baba189442c44ac3a93f8f28253865fd9b766fd2e6d2afc2a7cf47245b8
Description:  Kernel support for the TUN/TAP tunneling device

Package: kmod-udptunnel4
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-udptunnel4
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2232
Filename: kmod-udptunnel4_4.14.167-1_mipsel_24kc.ipk
Size: 2985
SHA256sum: b678b1931985fe77ea0252741109850e3836ed58f5979efdcec1ed2c6ec039c3
Description:  IPv4 UDP tunneling support

Package: kmod-udptunnel6
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-udptunnel6
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1695
Filename: kmod-udptunnel6_4.14.167-1_mipsel_24kc.ipk
Size: 2448
SHA256sum: 60e4162807e7afc4f921c90562e189faed1cc516a2dd4452651b87bb629b38da
Description:  IPv6 UDP tunneling support

Package: kmod-usb-acm
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-acm
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9894
Filename: kmod-usb-acm_4.14.167-1_mipsel_24kc.ipk
Size: 10669
SHA256sum: d671e1cf4d92b06c63f5b224128388ea72d2b7a0bf397f5e7a4797e54653c8eb
Description:  Kernel support for USB ACM devices (modems/isdn controllers)

Package: kmod-usb-atm-cxacru
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-atm
Source: package/kernel/linux
SourceName: kmod-usb-atm-cxacru
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10474
Filename: kmod-usb-atm-cxacru_4.14.167-1_mipsel_24kc.ipk
Size: 11169
SHA256sum: 0648d28ba938980f6d835bd3bce319c4dab6f299760b4c381d333e4245d9af6a
Description:  Kernel support for cxacru based USB ADSL modems

Package: kmod-usb-atm-speedtouch
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-atm
Source: package/kernel/linux
SourceName: kmod-usb-atm-speedtouch
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6665
Filename: kmod-usb-atm-speedtouch_4.14.167-1_mipsel_24kc.ipk
Size: 7415
SHA256sum: dbc7b11aad1f8d6d1012cabc951c419003af1b0d75eb61c312ae66857ddc8ff6
Description:  Kernel support for SpeedTouch USB ADSL modems

Package: kmod-usb-atm-ueagle
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-atm
Source: package/kernel/linux
SourceName: kmod-usb-atm-ueagle
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 13780
Filename: kmod-usb-atm-ueagle_4.14.167-1_mipsel_24kc.ipk
Size: 14495
SHA256sum: 421fb045e1a5b3cb9176d3f56dfde00c70c8e5250cf6a196e1b395a25c39b089
Description:  Kernel support for Eagle 8051 based USB ADSL modems

Package: kmod-usb-atm
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-atm, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-atm
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7795
Filename: kmod-usb-atm_4.14.167-1_mipsel_24kc.ipk
Size: 8543
SHA256sum: 21411477513a090cd55da57b84823fa23e656de33be290c30e30fa00f67823da
Description:  Kernel support for USB DSL modems

Package: kmod-usb-audio
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core, kmod-sound-core
Source: package/kernel/linux
SourceName: kmod-usb-audio
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 76860
Filename: kmod-usb-audio_4.14.167-1_mipsel_24kc.ipk
Size: 77116
SHA256sum: aaf7a5f26378e674703e40f954494a74de3786a7861aa49312ee012c2ee672e1
Description:  Kernel support for USB audio devices

Package: kmod-usb-cm109
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-input-evdev, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-cm109
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5938
Filename: kmod-usb-cm109_4.14.167-1_mipsel_24kc.ipk
Size: 6583
SHA256sum: 4c92de95733a089b8ad048c51f2703e15fa059100264ab8d4fd7da4508957f84
Description:  Kernel support for CM109 VOIP phone

Package: kmod-usb-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nls-base
Source: package/kernel/linux
SourceName: kmod-usb-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 82489
Filename: kmod-usb-core_4.14.167-1_mipsel_24kc.ipk
Size: 83005
SHA256sum: 0a7ca4fd6210eae690640262a54f2985df873c094b1702d685992a3f0e43481f
Description:  Kernel support for USB

Package: kmod-usb-dwc2
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-dwc2
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 43823
Filename: kmod-usb-dwc2_4.14.167-1_mipsel_24kc.ipk
Size: 43936
SHA256sum: b435a854d1fbae07227feeb74ccae51c1d01fc3cd26446a9488d053986bf14f5
Description:  This driver provides USB Device Controller support for the
 Synopsys DesignWare USB OTG Core

Package: kmod-usb-dwc3
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-dwc3
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10484
Filename: kmod-usb-dwc3_4.14.167-1_mipsel_24kc.ipk
Size: 10829
SHA256sum: 1935817e49f26ce25021a3c9619e521590b04f306341b840e83dc5d4795a69ec
Description:  This driver provides support for the Dual Role SuperSpeed
 USB Controller based on the Synopsys DesignWare USB3 IP Core

Package: kmod-usb-ehci
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-ehci
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 23195
Filename: kmod-usb-ehci_4.14.167-1_mipsel_24kc.ipk
Size: 23925
SHA256sum: 30483991430507d463447fe3e58aab485af368a05f6b99e55ce993cc03e9eefd
Description:  EHCI controller support

Package: kmod-usb-hid
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hid, kmod-hid-generic, kmod-input-evdev, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-hid
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 16520
Filename: kmod-usb-hid_4.14.167-1_mipsel_24kc.ipk
Size: 17332
SHA256sum: 323cecc382c22e9dfded354a2bfdc326924d460e12f1cf15ee459c98e5ae6ce4
Description:  Kernel support for USB HID devices such as keyboards and mice

Package: kmod-usb-ledtrig-usbport
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-ledtrig-usbport
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2829
Filename: kmod-usb-ledtrig-usbport_4.14.167-1_mipsel_24kc.ipk
Size: 3683
SHA256sum: f048dbe8f4b9a0399186303018df19a9d6135809d9871550405113adcc4b7bac
Description:  This driver allows LEDs to be controlled by USB events. Enabling this
 trigger allows specifying list of USB ports that should turn on LED
 when some USB device gets connected.
 If possible it should be prefered over similar ledtrig-usbdev.

Package: kmod-usb-net-asix-ax88179
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-libphy, kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-asix-ax88179
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7874
Filename: kmod-usb-net-asix-ax88179_4.14.167-1_mipsel_24kc.ipk
Size: 8685
SHA256sum: 09040171c3a0e77272bc38c9525e9d8578e73594e3606f740d12a3dd18f179d7
Description:  Kernel module for USB-to-Ethernet ASIX AX88179 based USB 3.0/2.0
 to Gigabit Ethernet adapters.

Package: kmod-usb-net-asix
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-libphy, kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-asix
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 11829
Filename: kmod-usb-net-asix_4.14.167-1_mipsel_24kc.ipk
Size: 12588
SHA256sum: 8bd523c6a7efc6bf1d20545f92d1e24f4c29171fec920145087200c685b8e5a9
Description:  Kernel module for USB-to-Ethernet Asix convertors

Package: kmod-usb-net-cdc-eem
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-cdc-eem
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2279
Filename: kmod-usb-net-cdc-eem_4.14.167-1_mipsel_24kc.ipk
Size: 3047
SHA256sum: b140929aa4080449da68d8e3cf3b77fbcb356426b69306070843d16329503496
Description:  Kernel support for USB CDC EEM

Package: kmod-usb-net-cdc-ether
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-cdc-ether
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3529
Filename: kmod-usb-net-cdc-ether_4.14.167-1_mipsel_24kc.ipk
Size: 4271
SHA256sum: 6b2c76ecc998be4cd194138904a8bedf63b2fa1752149c82089eacc92c792009
Description:  Kernel support for USB CDC Ethernet devices

Package: kmod-usb-net-cdc-mbim
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net, kmod-usb-wdm, kmod-usb-net-cdc-ncm
Source: package/kernel/linux
SourceName: kmod-usb-net-cdc-mbim
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3653
Filename: kmod-usb-net-cdc-mbim_4.14.167-1_mipsel_24kc.ipk
Size: 4409
SHA256sum: 87ee9b22726f5ff48c4b7976b00c260cda6c4c622baf350e1aab8605b8d379ae
Description:  Kernel module for Option USB High Speed Mobile Devices

Package: kmod-usb-net-cdc-ncm
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-cdc-ncm
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9899
Filename: kmod-usb-net-cdc-ncm_4.14.167-1_mipsel_24kc.ipk
Size: 10661
SHA256sum: 56982251bb33a8e64734c0374e477e3895ee2aa75a5525d230cfaacf6b059b4b
Description:  Kernel support for CDC NCM connections

Package: kmod-usb-net-cdc-subset
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-cdc-subset
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1293
Filename: kmod-usb-net-cdc-subset_4.14.167-1_mipsel_24kc.ipk
Size: 2085
SHA256sum: e1ca447af9cfd65491d64e043ed7714c00cbfc04835ff2284d217978d6c59bee
Description:  Kernel support for Simple USB Network Links (CDC Ethernet subset)

Package: kmod-usb-net-dm9601-ether
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-dm9601-ether
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4077
Filename: kmod-usb-net-dm9601-ether_4.14.167-1_mipsel_24kc.ipk
Size: 4822
SHA256sum: b7ed746f634d7101406428bad4010d3e732bf724a6b27b780e084a5f448fe4dc
Description:  Kernel support for USB DM9601 devices

Package: kmod-usb-net-hso
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-hso
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 16724
Filename: kmod-usb-net-hso_4.14.167-1_mipsel_24kc.ipk
Size: 17426
SHA256sum: 82a07adbb6deabd944adea96ee3c2192ffb14037442598e88d791036635ba46f
Description:  Kernel module for Option USB High Speed Mobile Devices

Package: kmod-usb-net-huawei-cdc-ncm
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net, kmod-usb-net-cdc-ncm, kmod-usb-wdm
Source: package/kernel/linux
SourceName: kmod-usb-net-huawei-cdc-ncm
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1542
Filename: kmod-usb-net-huawei-cdc-ncm_4.14.167-1_mipsel_24kc.ipk
Size: 2326
SHA256sum: ebe45106caa6472a54a80767f0dde33bf6aceaee9f3fe21a960121916777651d
Description:  Kernel support for Huawei CDC NCM connections

Package: kmod-usb-net-ipheth
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-ipheth
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4135
Filename: kmod-usb-net-ipheth_4.14.167-1_mipsel_24kc.ipk
Size: 4884
SHA256sum: d1e9c59dd8de04a66e7a718083ea03d5f704ccf26f87844c83733b41c9f0ba29
Description:  Kernel support for Apple iPhone USB Ethernet driver

Package: kmod-usb-net-kalmia
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-kalmia
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2576
Filename: kmod-usb-net-kalmia_4.14.167-1_mipsel_24kc.ipk
Size: 3321
SHA256sum: 7a8b6021561561cee6fa7af3b9a309eb8d3248a4e9357c02e6375b93b9f28f89
Description:  Kernel support for Samsung Kalmia based LTE USB modem

Package: kmod-usb-net-kaweth
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-kaweth
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6448
Filename: kmod-usb-net-kaweth_4.14.167-1_mipsel_24kc.ipk
Size: 7249
SHA256sum: 87b7f9aa052ca78f2b305fce313c65a7749dae3b001bf29ad540a207beb58b17
Description:  Kernel module for USB-to-Ethernet Kaweth convertors

Package: kmod-usb-net-mcs7830
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-mcs7830
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3430
Filename: kmod-usb-net-mcs7830_4.14.167-1_mipsel_24kc.ipk
Size: 4171
SHA256sum: 90ad622ec18af23248ab27a6ad86b453acfed69bb22a8b5277ac12457351000d
Description:  Kernel module for USB-to-Ethernet MCS7830 convertors

Package: kmod-usb-net-pegasus
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-pegasus
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 9590
Filename: kmod-usb-net-pegasus_4.14.167-1_mipsel_24kc.ipk
Size: 10364
SHA256sum: ba647fcd8650392b81e97ffec2a002ac0b5b6866603dde1f0d647fa6bb4e2e46
Description:  Kernel module for USB-to-Ethernet Pegasus convertors

Package: kmod-usb-net-pl
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-pl
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1026
Filename: kmod-usb-net-pl_4.14.167-1_mipsel_24kc.ipk
Size: 1799
SHA256sum: 01e04a1cd73583bf9b3ba48f734b6457734cb314ca7aa25982ef3a5f7afbaa6f
Description:  Kernel support for Prolific PL-2301/2302/25A1 based cables

Package: kmod-usb-net-qmi-wwan
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net, kmod-usb-wdm
Source: package/kernel/linux
SourceName: kmod-usb-net-qmi-wwan
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7235
Filename: kmod-usb-net-qmi-wwan_4.14.167-1_mipsel_24kc.ipk
Size: 7834
SHA256sum: 7dcee236552a85a7ca3a711395a9bfc19d8326c0c5afd114ddbc6f67fccbf06e
Description:  QMI WWAN driver for Qualcomm MSM based 3G and LTE modems

Package: kmod-usb-net-rndis
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net, kmod-usb-net-cdc-ether
Source: package/kernel/linux
SourceName: kmod-usb-net-rndis
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4297
Filename: kmod-usb-net-rndis_4.14.167-1_mipsel_24kc.ipk
Size: 5039
SHA256sum: eeb69fecdb72c97d94f45a1fc06de63918a94860aaf9faa911e8eb5ed275d90d
Description:  Kernel support for RNDIS connections

Package: kmod-usb-net-rtl8150
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-rtl8150
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5643
Filename: kmod-usb-net-rtl8150_4.14.167-1_mipsel_24kc.ipk
Size: 6404
SHA256sum: f1f52bae16381aca7e783a59c9c3c18538b1a14a0204cef60820a960425a6434
Description:  Kernel module for USB-to-Ethernet Realtek 8150 convertors

Package: kmod-usb-net-rtl8152
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-rtl8152
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 20870
Filename: kmod-usb-net-rtl8152_4.14.167-1_mipsel_24kc.ipk
Size: 21624
SHA256sum: 4246a3d20759e2f2608a3043c7d0a1d6e54a53d098ff4ff5d158d3571f641da6
Description:  Kernel module for USB-to-Ethernet Realtek 8152 USB2.0/3.0 convertors

Package: kmod-usb-net-sierrawireless
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-sierrawireless
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5195
Filename: kmod-usb-net-sierrawireless_4.14.167-1_mipsel_24kc.ipk
Size: 5936
SHA256sum: 01d3d2f1001149205a347dc2b120ae2d7412151e35c98971c7500922c21a45f7
Description:  Kernel support for Sierra Wireless devices

Package: kmod-usb-net-smsc95xx
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net, kmod-lib-crc16
Source: package/kernel/linux
SourceName: kmod-usb-net-smsc95xx
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10771
Filename: kmod-usb-net-smsc95xx_4.14.167-1_mipsel_24kc.ipk
Size: 11536
SHA256sum: 389bfbf254f0717a1e44e863e6a0f3c6058e6c7032acf883147124bff737c90d
Description:  Kernel module for SMSC LAN95XX based devices

Package: kmod-usb-net-sr9700
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-net
Source: package/kernel/linux
SourceName: kmod-usb-net-sr9700
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3783
Filename: kmod-usb-net-sr9700_4.14.167-1_mipsel_24kc.ipk
Size: 4549
SHA256sum: 1dcfe9c1d031f5a9cef8ced7a2b5661052f97502302c7ce1268a141858f45883
Description:  Kernel module for CoreChip-sz SR9700 based USB 1.1 10/100 ethernet devices

Package: kmod-usb-net
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mii, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-net
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 12202
Filename: kmod-usb-net_4.14.167-1_mipsel_24kc.ipk
Size: 12955
SHA256sum: b645691bfde528d268fc575249549b44a6c59b8b41ea72a305bcf56c003f4d65
Description:  Kernel modules for USB-to-Ethernet convertors

Package: kmod-usb-ohci-pci
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-ohci, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-ohci-pci
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2015
Filename: kmod-usb-ohci-pci_4.14.167-1_mipsel_24kc.ipk
Size: 2754
SHA256sum: 417b734303956b4ab417cde2943830e763ea1d3bb917951ca0ee922ae0174745
Description:  Kernel support for PCI OHCI controllers

Package: kmod-usb-ohci
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-ohci
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 20303
Filename: kmod-usb-ohci_4.14.167-1_mipsel_24kc.ipk
Size: 21042
SHA256sum: 8ec219b8bc8eb699e778a8d3e0f23d4a4cb41c82d6d2c96fbed6c556a2de13c0
Description:  Kernel support for USB OHCI controllers

Package: kmod-usb-printer
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-printer
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6947
Filename: kmod-usb-printer_4.14.167-1_mipsel_24kc.ipk
Size: 7736
SHA256sum: 94766b85690dadaa1c6826d65cf06423b5245a52d4c04494a8b3c4eb126df286
Description:  Kernel support for USB printers

Package: kmod-usb-serial-ark3116
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-ark3116
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3997
Filename: kmod-usb-serial-ark3116_4.14.167-1_mipsel_24kc.ipk
Size: 4748
SHA256sum: 5c835652d852245849451f717df9de43619558dc208d6b88f34b960b9345acd6
Description:  Kernel support for ArkMicroChips ARK3116 USB-to-Serial converters

Package: kmod-usb-serial-belkin
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-belkin
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3331
Filename: kmod-usb-serial-belkin_4.14.167-1_mipsel_24kc.ipk
Size: 4072
SHA256sum: 0a7bcb93303575c5fa5e145b6eb26b8bcf6495022c266718ab258653be9a38a1
Description:  Kernel support for Belkin USB-to-Serial converters

Package: kmod-usb-serial-ch341
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-ch341
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3443
Filename: kmod-usb-serial-ch341_4.14.167-1_mipsel_24kc.ipk
Size: 4204
SHA256sum: edbefc9d3f3c03a0dd2b976f8ce250da1400cb74d07888302c45f4e4f2f2de5e
Description:  Kernel support for Winchiphead CH341 USB-to-Serial converters

Package: kmod-usb-serial-cp210x
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-cp210x
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5428
Filename: kmod-usb-serial-cp210x_4.14.167-1_mipsel_24kc.ipk
Size: 6196
SHA256sum: a0d35647dd2f09c25cec6a38dc3945f2054af0edfcd773750c52d17594a47c36
Description:  Kernel support for Silicon Labs cp210x USB-to-Serial converters

Package: kmod-usb-serial-cypress-m8
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-cypress-m8
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5800
Filename: kmod-usb-serial-cypress-m8_4.14.167-1_mipsel_24kc.ipk
Size: 6645
SHA256sum: 73a2256b26d1b64b2fdeece9ccd0cf41d44fa63f4e33422ac4f5dbde7ac89695
Description:  Kernel support for devices with Cypress M8 USB to Serial chip
 (for example, the Delorme Earthmate LT-20 GPS)
 Supported microcontrollers in the CY4601 family are:
 CY7C63741 CY7C63742 CY7C63743 CY7C64013

Package: kmod-usb-serial-dmx_usb_module
Version: 4.14.167+0.1.20130818-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: feeds/packages/libs/dmx_usb_module
SourceName: kmod-usb-serial-dmx_usb_module
License: GPL-2.0
Section: kernel
Maintainer: Martijn Zilverschoon <martijn@friedzombie.com>
Architecture: mipsel_24kc
Installed-Size: 4722
Filename: kmod-usb-serial-dmx_usb_module_4.14.167+0.1.20130818-2_mipsel_24kc.ipk
Size: 5657
SHA256sum: 6f8eda55c0991beab52fb63d8ebc22d32959edf8ac169a29e43f1d0c8cab7acb
Description:  Open DMX USB is an open USB to DMX dongle hardware design developed by Enttec.
 The Open in Open DMX USB refers to the fact that everybody is free to use the
 design and produce its own USB DMX Dongle without paying any licenses.

Package: kmod-usb-serial-edgeport
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial, edgeport-firmware
Source: package/kernel/linux
SourceName: kmod-usb-serial-edgeport
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10972
Filename: kmod-usb-serial-edgeport_4.14.167-1_mipsel_24kc.ipk
Size: 11824
SHA256sum: 65ee3dc0080a268fc04a1c528d296d16f441501f034bdc077d8a27664fe2be1e
Description:  Kernel support for Inside Out Networks (Digi)
 Edgeport/4
 Rapidport/4
 Edgeport/4t
 Edgeport/2
 Edgeport/4i
 Edgeport/2i
 Edgeport/421
 Edgeport/21
 Edgeport/8
 Edgeport/8 Dual
 Edgeport/2D8
 Edgeport/4D8
 Edgeport/8i
 Edgeport/2 DIN
 Edgeport/4 DIN
 Edgeport/16 Dual

Package: kmod-usb-serial-ftdi
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-ftdi
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10830
Filename: kmod-usb-serial-ftdi_4.14.167-1_mipsel_24kc.ipk
Size: 11463
SHA256sum: 18084707c3d113f327167e24c629ef0f5c32accf873e73732b719ca44deacd84
Description:  Kernel support for FTDI USB-to-Serial converters

Package: kmod-usb-serial-garmin
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-garmin
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5153
Filename: kmod-usb-serial-garmin_4.14.167-1_mipsel_24kc.ipk
Size: 5908
SHA256sum: 1c828227a5afb6052a574b3debb66128183784e82f5fe4ec84db2d0a932aacda
Description:  Should work with most Garmin GPS devices which have a native USB port.

Package: kmod-usb-serial-ipw
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial, kmod-usb-serial-wwan
Source: package/kernel/linux
SourceName: kmod-usb-serial-ipw
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2116
Filename: kmod-usb-serial-ipw_4.14.167-1_mipsel_24kc.ipk
Size: 2861
SHA256sum: 5917515c9accbdd54ee5426becdde32d833cf9a0cbe64cd60ac00da6513939cb
Description:  Support for IPWireless 3G devices

Package: kmod-usb-serial-keyspan
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-keyspan
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10417
Filename: kmod-usb-serial-keyspan_4.14.167-1_mipsel_24kc.ipk
Size: 11160
SHA256sum: 5dd4d6eded49c53154c15920de9e82dd801202171483c33e34937e8deeffcc5c
Description:  Kernel support for Keyspan USB-to-Serial devices

Package: kmod-usb-serial-mct
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-mct
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3702
Filename: kmod-usb-serial-mct_4.14.167-1_mipsel_24kc.ipk
Size: 4460
SHA256sum: c346a0961b90bde4795759abaa449d5ff7f8c57e0249b205e4f8d68a57fca533
Description:  Kernel support for Magic Control Technology USB-to-Serial converters

Package: kmod-usb-serial-mos7720
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-mos7720
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4992
Filename: kmod-usb-serial-mos7720_4.14.167-1_mipsel_24kc.ipk
Size: 5738
SHA256sum: c8d3dad37f62374b5def832ad6c7c07a49a8d2db90751fe7414782ead57b4200
Description:  Kernel support for Moschip MOS7720 USB-to-Serial converters

Package: kmod-usb-serial-mos7840
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-mos7840
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7589
Filename: kmod-usb-serial-mos7840_4.14.167-1_mipsel_24kc.ipk
Size: 8370
SHA256sum: 23b008e95c24a8e39b2788c1361633712f8fccfd74b5be4fe9a72031d05f1491
Description:  Kernel support for Moschip MOS7840 USB-to-Serial converters

Package: kmod-usb-serial-option
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial, kmod-usb-serial-wwan
Source: package/kernel/linux
SourceName: kmod-usb-serial-option
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5561
Filename: kmod-usb-serial-option_4.14.167-1_mipsel_24kc.ipk
Size: 5460
SHA256sum: 4f3dcab3e40615f7df72093bf8b8d2c2bbf9e2beb6a203281d0b4a710a55f1b8
Description:  Kernel support for Option HSDPA modems

Package: kmod-usb-serial-oti6858
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-oti6858
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4237
Filename: kmod-usb-serial-oti6858_4.14.167-1_mipsel_24kc.ipk
Size: 5003
SHA256sum: 831563d6bd41afd9b01e26e3073c2c2843f316fe466631a2507016576249601e
Description:  Kernel support for Ours Technology OTI6858 USB-to-Serial converters

Package: kmod-usb-serial-pl2303
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-pl2303
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5052
Filename: kmod-usb-serial-pl2303_4.14.167-1_mipsel_24kc.ipk
Size: 5805
SHA256sum: 69cdfe9497a206c0d3d9e86c9430be68e244ed737f913d5d6f0988758dfe18b0
Description:  Kernel support for Prolific PL2303 USB-to-Serial converters

Package: kmod-usb-serial-qualcomm
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial, kmod-usb-serial-wwan
Source: package/kernel/linux
SourceName: kmod-usb-serial-qualcomm
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2369
Filename: kmod-usb-serial-qualcomm_4.14.167-1_mipsel_24kc.ipk
Size: 3127
SHA256sum: 0ba7e95b5ab1d75e6fcf6c01a0b5bdbd595d4da665fb92e425a3c7c79c94565a
Description:  Kernel support for Qualcomm USB Serial devices (Gobi)

Package: kmod-usb-serial-sierrawireless
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-sierrawireless
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4313
Filename: kmod-usb-serial-sierrawireless_4.14.167-1_mipsel_24kc.ipk
Size: 5063
SHA256sum: 73f6c461b5e0ab17b91b78aa386baffae8b56b3ee5525c5a61d1926f90b8b078
Description:  Kernel support for Sierra Wireless devices

Package: kmod-usb-serial-simple
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-simple
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1494
Filename: kmod-usb-serial-simple_4.14.167-1_mipsel_24kc.ipk
Size: 2453
SHA256sum: d659e46baf120944a4dc72233cee50db988121b6baaf80d7a14c5050d67d48ae
Description:  Kernel support for "very simple devices".
 
 Specifically, it supports:
 - Suunto ANT+ USB device.
 - Medtronic CareLink USB device (3.18)
 - Fundamental Software dongle.
 - Google USB serial devices (3.19)
 - HP4x calculators
 - a number of Motorola phones
 - Novatel Wireless GPS receivers (3.18)
 - Siemens USB/MPI adapter.
 - ViVOtech ViVOpay USB device.
 - Infineon Modem Flashloader USB interface
 - ZIO Motherboard USB serial interface

Package: kmod-usb-serial-ti-usb
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-ti-usb
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7698
Filename: kmod-usb-serial-ti-usb_4.14.167-1_mipsel_24kc.ipk
Size: 8433
SHA256sum: 031da34801c6674e44aecc35beee3084f05485be0a193765b2c384b7291f254f
Description:  Kernel support for TI USB 3410/5052 devices

Package: kmod-usb-serial-visor
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-visor
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3587
Filename: kmod-usb-serial-visor_4.14.167-1_mipsel_24kc.ipk
Size: 4314
SHA256sum: 75df9160a38fe8d3d5565eded1148844fd8c8e741468ee00e1068b95dff22f20
Description:  Kernel support for Handspring Visor PDAs

Package: kmod-usb-serial-wwan
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: package/kernel/linux
SourceName: kmod-usb-serial-wwan
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3865
Filename: kmod-usb-serial-wwan_4.14.167-1_mipsel_24kc.ipk
Size: 4610
SHA256sum: 065b38c37bad59b534ec0851943fe9627258fe9bd105c00d5c6d266556ff5385
Description:  Kernel support for USB GSM and CDMA modems

Package: kmod-usb-serial-xr_usb_serial_common
Version: 4.14.167+1a-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-serial
Source: feeds/packages/libs/xr_usb_serial_common
SourceName: kmod-usb-serial-xr_usb_serial_common
License: GPLv2
Section: kernel
Maintainer: Daniel Golle <daniel@makrotopia.org>
Architecture: mipsel_24kc
Installed-Size: 14897
Filename: kmod-usb-serial-xr_usb_serial_common_4.14.167+1a-1_mipsel_24kc.ipk
Size: 15659
SHA256sum: 4491a5a9742e901df2946019519f9cd225eab63b64e39dc0791861a271370861
Description:  Support for Exar USB to RS-485/RS-422

Package: kmod-usb-serial
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-serial
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 12870
Filename: kmod-usb-serial_4.14.167-1_mipsel_24kc.ipk
Size: 13617
SHA256sum: a7f1164dcd4c2dd0b08d60f6b27d56bed66c4eb8e9695761524b2af6f0ea57f5
Description:  Kernel support for USB-to-Serial converters

Package: kmod-usb-storage-extras
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-storage
Source: package/kernel/linux
SourceName: kmod-usb-storage-extras
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 32551
Filename: kmod-usb-storage-extras_4.14.167-1_mipsel_24kc.ipk
Size: 33319
SHA256sum: 840b96ce79c136e4aaf9e3a2bc8aadd365c00445813e43a6e1a6148c12b5efe0
Description:  Say Y here if you want to have some more drivers,
 such as for SmartMedia card readers

Package: kmod-usb-storage-uas
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-storage
Source: package/kernel/linux
SourceName: kmod-usb-storage-uas
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 8730
Filename: kmod-usb-storage-uas_4.14.167-1_mipsel_24kc.ipk
Size: 9553
SHA256sum: 3f2ebe3145126b27c6e9e29b254a725b36f42ae409b5275065db79afcd928b78
Description:  Say Y here if you want to include support for
 USB Attached SCSI (UAS/UASP), a higher
 performance protocol available on many
 newer USB 3.0 storage devices

Package: kmod-usb-storage
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-scsi-core, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-storage
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 23420
Filename: kmod-usb-storage_4.14.167-1_mipsel_24kc.ipk
Size: 23639
SHA256sum: 39580399c7dc32a11e309fcc9f2cdc34bf735f31fe393db97f4a1d4a47b2b853
Description:  Kernel support for USB Mass Storage devices

Package: kmod-usb-test
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-test
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 16236
Filename: kmod-usb-test_4.14.167-1_mipsel_24kc.ipk
Size: 16942
SHA256sum: e00fa899b360bf4f431b62214b1a83c68358d0574291f531c4c9f84b95f97181
Description:  Kernel support for testing USB Host Controller software

Package: kmod-usb-uhci
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-uhci
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 13806
Filename: kmod-usb-uhci_4.14.167-1_mipsel_24kc.ipk
Size: 14526
SHA256sum: 4d652be60eba3101ef9153a6a9dff80aebcc97e54bdcaa4475f2fb56831b7d67
Description:  Kernel support for USB UHCI controllers

Package: kmod-usb-wdm
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-wdm
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5933
Filename: kmod-usb-wdm_4.14.167-1_mipsel_24kc.ipk
Size: 6687
SHA256sum: a236d259cd0fceea4b0755ff9b4096c515002717535c32126c599563bd34c862
Description:  USB Wireless Device Management support

Package: kmod-usb-yealink
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-input-evdev, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb-yealink
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5881
Filename: kmod-usb-yealink_4.14.167-1_mipsel_24kc.ipk
Size: 6651
SHA256sum: 5b2d2f86a920360bc5d95983d5ff701810f83e9a370e138dbbb844057a3d67e9
Description:  Kernel support for Yealink VOIP phone

Package: kmod-usb2-pci
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb2, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb2-pci
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2968
Filename: kmod-usb2-pci_4.14.167-1_mipsel_24kc.ipk
Size: 3712
SHA256sum: 63942cb8c4983a0c10e12bbdf8d141face48cba15028bd912fe0613a2f0e7317
Description:  Kernel support for PCI USB2 (EHCI) controllers

Package: kmod-usb2
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-ehci, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb2
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3553
Filename: kmod-usb2_4.14.167-1_mipsel_24kc.ipk
Size: 4292
SHA256sum: 495d58eaee70227b257b00fc631f10e714dc5461896b764df8950eb435d12de9
Description:  Kernel support for USB2 (EHCI) controllers

Package: kmod-usb3
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usb3
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 60682
Filename: kmod-usb3_4.14.167-1_mipsel_24kc.ipk
Size: 61111
SHA256sum: 61b75d6eeb7d6fba7910fdf5323dbec47af412d93be7f7e300bfd2b9a5c2d3b1
Description:  Kernel support for USB3 (XHCI) controllers

Package: kmod-usbip-client
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usbip, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usbip-client
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 12504
Filename: kmod-usbip-client_4.14.167-1_mipsel_24kc.ipk
Size: 13212
SHA256sum: e7c4b42c332760719f28469b22089643039a9a5275ff3828beae599afa175f87
Description:  USB-over-IP client driver

Package: kmod-usbip-server
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usbip, kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usbip-server
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 10127
Filename: kmod-usbip-server_4.14.167-1_mipsel_24kc.ipk
Size: 10875
SHA256sum: 31f66f6d3ddadedc2fd14b14b8374736dddd4e72e4af3cf5a276a5fb4f30830f
Description:  USB-over-IP host driver

Package: kmod-usbip
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usbip
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4341
Filename: kmod-usbip_4.14.167-1_mipsel_24kc.ipk
Size: 5055
SHA256sum: 6b6b5c8841ed9f3dfb47fe6bd6b769facc8280b8d18e2d434d9bd46e6dff3ed6
Description:  USB-over-IP kernel support

Package: kmod-usbmon
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core
Source: package/kernel/linux
SourceName: kmod-usbmon
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 12250
Filename: kmod-usbmon_4.14.167-1_mipsel_24kc.ipk
Size: 12991
SHA256sum: c7d3f8f6337bb0a26dc696259ccbb8700d57e8a3b657290c0ce4d15faa4e32ec
Description:  Kernel support for USB traffic monitoring

Package: kmod-veth
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-veth
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2962
Filename: kmod-veth_4.14.167-1_mipsel_24kc.ipk
Size: 3739
SHA256sum: d13d4b0157b3c0d0fe5a249a3183a0d02ff87a0dd3cacffc1651d2ea83584371
Description:  This device is a local ethernet tunnel. Devices are created in pairs.
 When one end receives the packet it appears on its pair and vice
 versa.

Package: kmod-via-rhine
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mii
Source: package/kernel/linux
SourceName: kmod-via-rhine
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 12845
Filename: kmod-via-rhine_4.14.167-1_mipsel_24kc.ipk
Size: 13588
SHA256sum: 8efe14eefae42fb10556c2dd9507ef74baf121f78f97b85ab5426266d268ec3f
Description:  Kernel modules for Via Rhine Ethernet chipsets

Package: kmod-via-velocity
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-crc-ccitt
Source: package/kernel/linux
SourceName: kmod-via-velocity
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 15051
Filename: kmod-via-velocity_4.14.167-1_mipsel_24kc.ipk
Size: 15807
SHA256sum: f49cddde36213f3851a043a88a912904b97856ef8f80fc9f7e53e41f9d12495e
Description:  Kernel modules for VIA Velocity Gigabit Ethernet chipsets

Package: kmod-video-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-video-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 63936
Filename: kmod-video-core_4.14.167-1_mipsel_24kc.ipk
Size: 63917
SHA256sum: 84b1ca4d507a0905202fd99560663b9b53b3276a15fa780a785f4bb98a0bc3f7
Description:  Kernel modules for Video4Linux support

Package: kmod-video-cpia2
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core, kmod-video-core
Source: package/kernel/linux
SourceName: kmod-video-cpia2
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 18396
Filename: kmod-video-cpia2_4.14.167-1_mipsel_24kc.ipk
Size: 19150
SHA256sum: db07cf54092484fc89efec7d061fe6091871b4be008397407f401ef8815e0fa5
Description:  Kernel modules for supporting CPIA2 USB based cameras

Package: kmod-video-gspca-conex
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-conex
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5819
Filename: kmod-video-gspca-conex_4.14.167-1_mipsel_24kc.ipk
Size: 6584
SHA256sum: 7c449f0231bf0cd00d9452e83408524f7803a579a9628b27f32f09b42bf74209
Description:  The Conexant Camera Driver (conex) kernel module

Package: kmod-video-gspca-core
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core, kmod-input-core, kmod-video-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-core
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 14441
Filename: kmod-video-gspca-core_4.14.167-1_mipsel_24kc.ipk
Size: 15212
SHA256sum: f0dc335c2a18b885cc5df177da2ec24be48e7b25a50cc2dbf1d9b09f7e71a04f
Description:  Kernel modules for supporting GSPCA based webcam devices. Note this is just
 the core of the driver, please select a submodule that supports your webcam.

Package: kmod-video-gspca-etoms
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-etoms
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4813
Filename: kmod-video-gspca-etoms_4.14.167-1_mipsel_24kc.ipk
Size: 5558
SHA256sum: 72057cfac768faa95ace21695cdb8fa51839a469885e30cae6bd7125d17d3bfe
Description:  The Etoms USB Camera Driver (etoms) kernel module

Package: kmod-video-gspca-finepix
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-finepix
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2240
Filename: kmod-video-gspca-finepix_4.14.167-1_mipsel_24kc.ipk
Size: 3001
SHA256sum: 46ab2f6aa5d4bac1244621d270caf2740b0428f71d3b77ea8e7e7a754c8c13ca
Description:  The Fujifilm FinePix USB V4L2 driver (finepix) kernel module

Package: kmod-video-gspca-gl860
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-gl860
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 15125
Filename: kmod-video-gspca-gl860_4.14.167-1_mipsel_24kc.ipk
Size: 15816
SHA256sum: a2f5f3664a7923acbf03f691af789799b6d45797759a8788a02d5316ceccbc39
Description:  The GL860 USB Camera Driver (gl860) kernel module

Package: kmod-video-gspca-jeilinj
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-jeilinj
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4255
Filename: kmod-video-gspca-jeilinj_4.14.167-1_mipsel_24kc.ipk
Size: 5007
SHA256sum: 9135192055ff4146f3b1877f33696a574d529ac80f7ea188e8f14e24e05c8e6b
Description:  The JEILINJ USB Camera Driver (jeilinj) kernel module

Package: kmod-video-gspca-konica
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-konica
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3620
Filename: kmod-video-gspca-konica_4.14.167-1_mipsel_24kc.ipk
Size: 4362
SHA256sum: 29bfd96a6c2f5f15585af64f42e9e05e176838ab80a0b79e86c7d9cc5e1db853
Description:  The Konica USB Camera Driver (konica) kernel module

Package: kmod-video-gspca-m5602
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-m5602
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 16219
Filename: kmod-video-gspca-m5602_4.14.167-1_mipsel_24kc.ipk
Size: 16880
SHA256sum: 6764bf81534fd595c10d833ef746370043293a9efb9590e7a06e57fc6061de20
Description:  The ALi USB m5602 Camera Driver (m5602) kernel module

Package: kmod-video-gspca-mars
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-mars
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3585
Filename: kmod-video-gspca-mars_4.14.167-1_mipsel_24kc.ipk
Size: 4331
SHA256sum: 85b66dc33b7d8c1ca961b6d8633eb652aaa09f42f54132caf664937bf862b0ae
Description:  The Mars USB Camera Driver (mars) kernel module

Package: kmod-video-gspca-mr97310a
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-mr97310a
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5650
Filename: kmod-video-gspca-mr97310a_4.14.167-1_mipsel_24kc.ipk
Size: 6408
SHA256sum: a8aa30a780beb74fcad5bb1aac7f16c7fb5745d6afac7deea9f0509fb84dcf4c
Description:  The Mars-Semi MR97310A USB Camera Driver (mr97310a) kernel module

Package: kmod-video-gspca-ov519
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-ov519
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 20993
Filename: kmod-video-gspca-ov519_4.14.167-1_mipsel_24kc.ipk
Size: 21723
SHA256sum: 9b180977faa2e8cdac0a43df9d8be3f30246000ab79be43ffaa6683d4cfd93a1
Description:  The OV519 USB Camera Driver (ov519) kernel module

Package: kmod-video-gspca-ov534-9
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-ov534-9
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6476
Filename: kmod-video-gspca-ov534-9_4.14.167-1_mipsel_24kc.ipk
Size: 7247
SHA256sum: 3a1714325c377cd3b3069c182fbea431ab756a418e76df4cb952fd667b1feaf0
Description:  The OV534-9 USB Camera Driver (ov534_9) kernel module

Package: kmod-video-gspca-ov534
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-ov534
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 7566
Filename: kmod-video-gspca-ov534_4.14.167-1_mipsel_24kc.ipk
Size: 8336
SHA256sum: 27ba5bdda224f6ece789b92df371408a0248bd41c82bce036490db2c4fb943b8
Description:  The OV534 USB Camera Driver (ov534) kernel module

Package: kmod-video-gspca-pac207
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-pac207
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3972
Filename: kmod-video-gspca-pac207_4.14.167-1_mipsel_24kc.ipk
Size: 4726
SHA256sum: 01567d178dea7e6a4c64c47613ce0605754b4b7f8d140732399ba5523daf7465
Description:  The Pixart PAC207 USB Camera Driver (pac207) kernel module

Package: kmod-video-gspca-pac7311
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-pac7311
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4433
Filename: kmod-video-gspca-pac7311_4.14.167-1_mipsel_24kc.ipk
Size: 5199
SHA256sum: bf9596a8c3fa9096775f0e4b282e637f32fbb1aa67eaf51b004993a5a089cb19
Description:  The Pixart PAC7311 USB Camera Driver (pac7311) kernel module

Package: kmod-video-gspca-se401
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-se401
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4721
Filename: kmod-video-gspca-se401_4.14.167-1_mipsel_24kc.ipk
Size: 5456
SHA256sum: 04e8a6e82e76a9690fc57610484df128adf031c8d9cf41315a2cca3b90371036
Description:  The SE401 USB Camera Driver kernel module

Package: kmod-video-gspca-sn9c20x
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-sn9c20x
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 13831
Filename: kmod-video-gspca-sn9c20x_4.14.167-1_mipsel_24kc.ipk
Size: 14555
SHA256sum: 6876c902c4636685ab5bea113d087a05e4e8606dec4a8dc3648de0002c8cda4e
Description:  The SN9C20X USB Camera Driver (sn9c20x) kernel module

Package: kmod-video-gspca-sonixb
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-sonixb
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6823
Filename: kmod-video-gspca-sonixb_4.14.167-1_mipsel_24kc.ipk
Size: 7625
SHA256sum: a4c3cbf7a11c20971c6e434f671e56b499a888186993f43765c70ccfb53eac74
Description:  The SONIX Bayer USB Camera Driver (sonixb) kernel module

Package: kmod-video-gspca-sonixj
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-sonixj
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 13873
Filename: kmod-video-gspca-sonixj_4.14.167-1_mipsel_24kc.ipk
Size: 14607
SHA256sum: 01b648c5477d2919ba24f1fea038cfdd1ba35ba9d79524048eca554fae0dac91
Description:  The SONIX JPEG USB Camera Driver (sonixj) kernel module

Package: kmod-video-gspca-spca500
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-spca500
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5876
Filename: kmod-video-gspca-spca500_4.14.167-1_mipsel_24kc.ipk
Size: 6636
SHA256sum: 205085e5bb892ec42b810b7624ee66ccf94ddf0c213f978125aa4d3c81efe52b
Description:  The SPCA500 USB Camera Driver (spca500) kernel module

Package: kmod-video-gspca-spca501
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-spca501
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4178
Filename: kmod-video-gspca-spca501_4.14.167-1_mipsel_24kc.ipk
Size: 4921
SHA256sum: 31fafa6bb0ba207ca1af14397f4fd6e0988c769e9686a42b2ebe5e6877a764ed
Description:  The SPCA501 USB Camera Driver (spca501) kernel module

Package: kmod-video-gspca-spca505
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-spca505
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3088
Filename: kmod-video-gspca-spca505_4.14.167-1_mipsel_24kc.ipk
Size: 3836
SHA256sum: 8e6feead33c439a37ff2d8f7b48566935ca31605d48686e19cd54e8735cfcec1
Description:  The SPCA505 USB Camera Driver (spca505) kernel module

Package: kmod-video-gspca-spca506
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-spca506
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3869
Filename: kmod-video-gspca-spca506_4.14.167-1_mipsel_24kc.ipk
Size: 4617
SHA256sum: 98d0dae3993194b96449de28fc0592c7cefde60a3a134079773a584932071ff9
Description:  The SPCA506 USB Camera Driver (spca506) kernel module

Package: kmod-video-gspca-spca508
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-spca508
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3889
Filename: kmod-video-gspca-spca508_4.14.167-1_mipsel_24kc.ipk
Size: 4637
SHA256sum: 3d99e9e112d546c033579b7ef8c0939bdfc8517e8ccd374fa4457c88114314c1
Description:  The SPCA508 USB Camera Driver (spca508) kernel module

Package: kmod-video-gspca-spca561
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-spca561
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5046
Filename: kmod-video-gspca-spca561_4.14.167-1_mipsel_24kc.ipk
Size: 5787
SHA256sum: 1b64031dad0967bdc6c7af96655cb64776f2fad247d192297c1a76b168eb07c0
Description:  The SPCA561 USB Camera Driver (spca561) kernel module

Package: kmod-video-gspca-sq905
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-sq905
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3065
Filename: kmod-video-gspca-sq905_4.14.167-1_mipsel_24kc.ipk
Size: 3824
SHA256sum: 009c87601b600ee92fc997d91e4f2438ed0ae75d1bc930ee9d8a16597e31963f
Description:  The SQ Technologies SQ905 based USB Camera Driver (sq905) kernel module

Package: kmod-video-gspca-sq905c
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-sq905c
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2802
Filename: kmod-video-gspca-sq905c_4.14.167-1_mipsel_24kc.ipk
Size: 3570
SHA256sum: 373ddbc2619f6e0996b7fe1fcd56937ef3067dc6158974cd0615f21e0bc39593
Description:  The SQ Technologies SQ905C based USB Camera Driver (sq905c) kernel module

Package: kmod-video-gspca-stk014
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-stk014
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 3751
Filename: kmod-video-gspca-stk014_4.14.167-1_mipsel_24kc.ipk
Size: 4507
SHA256sum: d7229b82bb2cecb93072295f868cc670fbb64a5ff890268386bf0a9566b5f7bb
Description:  The Syntek DV4000 (STK014) USB Camera Driver (stk014) kernel module

Package: kmod-video-gspca-stv06xx
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-stv06xx
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 11506
Filename: kmod-video-gspca-stv06xx_4.14.167-1_mipsel_24kc.ipk
Size: 12267
SHA256sum: aec54d41b3a94d2b3588dfd1a5c23fdaf0ec00825b29452666ce31ab9930e35b
Description:  The STV06XX USB Camera Driver (stv06xx) kernel module

Package: kmod-video-gspca-sunplus
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-sunplus
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6136
Filename: kmod-video-gspca-sunplus_4.14.167-1_mipsel_24kc.ipk
Size: 6905
SHA256sum: 964fdd71095566da0594f6fe34acf1f1794d63b9654b7041a83c843c8b138ba7
Description:  The SUNPLUS USB Camera Driver (sunplus) kernel module

Package: kmod-video-gspca-t613
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-t613
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 6351
Filename: kmod-video-gspca-t613_4.14.167-1_mipsel_24kc.ipk
Size: 7170
SHA256sum: 8a1ffd5423667c53a140d2508115c2b91fc468ac79cd767d9956befffa45bb62
Description:  The T613 (JPEG Compliance) USB Camera Driver (t613) kernel module

Package: kmod-video-gspca-tv8532
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-tv8532
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2315
Filename: kmod-video-gspca-tv8532_4.14.167-1_mipsel_24kc.ipk
Size: 3058
SHA256sum: d4d32ea7e7d9eb404f5d1fece5670d69bb2c9a682f83acf6e6e655f44ce9b59f
Description:  The TV8532 USB Camera Driver (tv8532) kernel module

Package: kmod-video-gspca-vc032x
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-vc032x
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 11697
Filename: kmod-video-gspca-vc032x_4.14.167-1_mipsel_24kc.ipk
Size: 12465
SHA256sum: 75bf59c1f6ed0ac5fdc00988ee92509170b4b55c71596c7d0343e5d0922a6ef8
Description:  The VC032X USB Camera Driver (vc032x) kernel module

Package: kmod-video-gspca-zc3xx
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-video-gspca-core
Source: package/kernel/linux
SourceName: kmod-video-gspca-zc3xx
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 16288
Filename: kmod-video-gspca-zc3xx_4.14.167-1_mipsel_24kc.ipk
Size: 16947
SHA256sum: f57ccf1e92a0ef7680bd4a7c57c330c6656819348adff1986b359eb319aaa9ec
Description:  The ZC3XX USB Camera Driver (zc3xx) kernel module

Package: kmod-video-pwc
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core, kmod-video-videobuf2, kmod-video-core
Source: package/kernel/linux
SourceName: kmod-video-pwc
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 23187
Filename: kmod-video-pwc_4.14.167-1_mipsel_24kc.ipk
Size: 23920
SHA256sum: 57bfbe632d223e3d2c3eee072767a6e1ce1fb6a987a4c1aaee781a3e1a241932
Description:  Kernel modules for supporting Philips USB based cameras

Package: kmod-video-uvc
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core, kmod-video-videobuf2, kmod-input-core, kmod-video-core
Source: package/kernel/linux
SourceName: kmod-video-uvc
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 40919
Filename: kmod-video-uvc_4.14.167-1_mipsel_24kc.ipk
Size: 41724
SHA256sum: 1e88297b16beb1aa2dd47315059254f94394acf5ea074867a791db1fbf9511c5
Description:  Kernel modules for supporting USB Video Class (UVC) devices

Package: kmod-video-videobuf2
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-dma-buf, kmod-video-core
Source: package/kernel/linux
SourceName: kmod-video-videobuf2
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 23702
Filename: kmod-video-videobuf2_4.14.167-1_mipsel_24kc.ipk
Size: 24399
SHA256sum: 9e0e780de0a1e87599227b1b822cdfa616bc38917a10464245747167f10b49c5
Description:  Kernel modules that implements three basic types of media buffers.

Package: kmod-vmxnet3
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-vmxnet3
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 20703
Filename: kmod-vmxnet3_4.14.167-1_mipsel_24kc.ipk
Size: 21436
SHA256sum: 4a8605f88cebf909b7f5731583d4ea7920f6f509ad5acf9087f7a5ec490460cb
Description:  Kernel modules for VMware VMXNET3 ethernet adapters.

Package: kmod-vxlan
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-iptunnel, kmod-udptunnel4, kmod-udptunnel6
Source: package/kernel/linux
SourceName: kmod-vxlan
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 23419
Filename: kmod-vxlan_4.14.167-1_mipsel_24kc.ipk
Size: 24177
SHA256sum: 28dc1276fae21a0229e0da863f3fcd31369c6c82b130665e522e9e0d73329c88
Description:  Kernel module for supporting VXLAN in the Kernel.
 Requires Kernel 3.12 or newer.

Package: kmod-w1-gpio-custom
Version: 4.14.167-4
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-w1, kmod-w1-master-gpio
Source: package/kernel/w1-gpio-custom
SourceName: kmod-w1-gpio-custom
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1599
Filename: kmod-w1-gpio-custom_4.14.167-4_mipsel_24kc.ipk
Size: 2363
SHA256sum: c109b36aaf2456bc94464d1b2c9b89840e5aa04e680e9cd610bada7d466adce3
Description:  Kernel module to register a custom w1-gpio platform device.

Package: kmod-w1-master-ds2482
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-w1, kmod-i2c-core
Source: package/kernel/linux
SourceName: kmod-w1-master-ds2482
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2743
Filename: kmod-w1-master-ds2482_4.14.167-1_mipsel_24kc.ipk
Size: 3557
SHA256sum: d5849786521b7ab22768f233a7bc064bac7faf50c100855c5b77ecfc58bc9c24
Description:  Kernel module for the DS2482 i2c 1-wire bus master driver
 NOTE: Init with: echo ds2482 0x18 > /sys/bus/i2c/devices/i2c-0/new_device
 or use owfs

Package: kmod-w1-master-ds2490
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core, kmod-w1
Source: package/kernel/linux
SourceName: kmod-w1-master-ds2490
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 5428
Filename: kmod-w1-master-ds2490_4.14.167-1_mipsel_24kc.ipk
Size: 6196
SHA256sum: 6068e8b3fdb5ff1fe8bd9ccd46d70a30ce8d6d0a67d7abe96f00a1a4d29fb5f7
Description:  Kernel module for the DS2490 usb 1-wire bus master driver

Package: kmod-w1-master-gpio
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-w1
Source: package/kernel/linux
SourceName: kmod-w1-master-gpio
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2063
Filename: kmod-w1-master-gpio_4.14.167-1_mipsel_24kc.ipk
Size: 2801
SHA256sum: 6f066bd6df9592c94b898b76d91db5d14c92d4d7328339e7bf1a69367854fae5
Description:  Kernel module for the GPIO 1-wire bus master driver

Package: kmod-w1-slave-ds2413
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-w1
Source: package/kernel/linux
SourceName: kmod-w1-slave-ds2413
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1324
Filename: kmod-w1-slave-ds2413_4.14.167-1_mipsel_24kc.ipk
Size: 2112
SHA256sum: 27087e2f6e3ca80534ddb65fe5e4b6522c0cfbcea4f2504a2c9879f854cb9562
Description:  Kernel module for 1-wire DS2413 Dual Channel Addressable Switch support

Package: kmod-w1-slave-ds2431
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-w1
Source: package/kernel/linux
SourceName: kmod-w1-slave-ds2431
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 2243
Filename: kmod-w1-slave-ds2431_4.14.167-1_mipsel_24kc.ipk
Size: 3007
SHA256sum: 560b592d6f23a79879ba43a9344309208a45711a1cf4e4cf877a7ca4d827153f
Description:  Kernel module for 1-wire 1kb EEPROM (DS2431)

Package: kmod-w1-slave-ds2433
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-w1
Source: package/kernel/linux
SourceName: kmod-w1-slave-ds2433
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1643
Filename: kmod-w1-slave-ds2433_4.14.167-1_mipsel_24kc.ipk
Size: 2420
SHA256sum: 772ecf5d8f67727900588de2a0692a8d4bfae80c195d03292cfc677033c023cd
Description:  Kernel module for 1-wire 4kb EEPROM (DS2433)

Package: kmod-w1-slave-ds2760
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-w1
Source: package/kernel/linux
SourceName: kmod-w1-slave-ds2760
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 1599
Filename: kmod-w1-slave-ds2760_4.14.167-1_mipsel_24kc.ipk
Size: 2380
SHA256sum: 67e33f92aedb36b2b6056c1162b1f0681b9464abf84c3a976f0632ab288797ac
Description:  Kernel module for 1-wire DS2760 battery monitor chip support

Package: kmod-w1-slave-smem
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-w1
Source: package/kernel/linux
SourceName: kmod-w1-slave-smem
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 819
Filename: kmod-w1-slave-smem_4.14.167-1_mipsel_24kc.ipk
Size: 1595
SHA256sum: 4c09777317e80fa4f4d902d33f590b2f7d58486171633eb9ac0c0ba3ac269a1e
Description:  Kernel module for 1-wire simple 64bit memory rom(ds2401/ds2411/ds1990*)

Package: kmod-w1-slave-therm
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-w1
Source: package/kernel/linux
SourceName: kmod-w1-slave-therm
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 4324
Filename: kmod-w1-slave-therm_4.14.167-1_mipsel_24kc.ipk
Size: 5051
SHA256sum: 1cf3357926c1b50ba2af4d83d12f1de17ddbb6ada47da9655b015faf9e654e0b
Description:  Kernel module for 1-wire thermal sensors

Package: kmod-w1
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-hwmon-core
Source: package/kernel/linux
SourceName: kmod-w1
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 11616
Filename: kmod-w1_4.14.167-1_mipsel_24kc.ipk
Size: 12393
SHA256sum: 0d7decc0bb049e6ecc2f2a41a7d9713842088b928e342aa6c7d27bfe25f53525
Description:  Kernel module for Dallas's 1-wire support

Package: kmod-w83627hf-wdt
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c)
Source: package/kernel/linux
SourceName: kmod-w83627hf-wdt
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 105
Filename: kmod-w83627hf-wdt_4.14.167-1_mipsel_24kc.ipk
Size: 852
SHA256sum: eb6d1f3c85e28cb29349bc48eebc3a24246675c49137305ee631991df99fa5e5
Description:  Kernel module for Winbond 83627HF Watchdog Timer

Package: kmod-wifidog-ng
Version: 4.14.167+2.0.0-2
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-nf-nat, kmod-ipt-ipset
Source: feeds/packages/net/wifidog-ng
SourceName: kmod-wifidog-ng
License: LGPL-2.1
LicenseFiles: LICENSE
Section: kernel
Maintainer: Jianhui Zhao <jianhuizhao329@gmail.com>
Architecture: mipsel_24kc
Installed-Size: 3838
Filename: kmod-wifidog-ng_4.14.167+2.0.0-2_mipsel_24kc.ipk
Size: 4618
SHA256sum: d10fd4cd7b7b0aff1bfd7484b4d2655ac05ea9062bafc7977b757eff1912e77b
Description:  Kernel module for wifidog-ng

Package: kmod-wireguard
Version: 4.14.167+0.0.20190702-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-udptunnel6, kmod-udptunnel4
Source: package/network/services/wireguard
SourceName: kmod-wireguard
License: GPL-2.0 Apache-2.0
LicenseFiles: COPYING
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 55167
Filename: kmod-wireguard_4.14.167+0.0.20190702-1_mipsel_24kc.ipk
Size: 56198
SHA256sum: eb3f1241d0653c8b4f08c4dac6769dab68ab1348914b01d19814ffcecb1b29a1
Description:  WireGuard is a novel VPN that runs inside the Linux Kernel and utilizes
 state-of-the-art cryptography. It aims to be faster, simpler, leaner, and
 more useful than IPSec, while avoiding the massive headache. It intends to
 be considerably more performant than OpenVPN.  WireGuard is designed as a
 general purpose VPN for running on embedded interfaces and super computers
 alike, fit for many different circumstances. It uses UDP.
 
 This package provides the kernel module for WireGuard.

Package: kmod-wl12xx
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-wlcore, wl12xx-firmware
Source: package/kernel/mac80211
SourceName: kmod-wl12xx
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 19865
Filename: kmod-wl12xx_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 20411
SHA256sum: e8c508136c018b888b2f9c6214e5e21b1113772c5af3a17a71fa4e423e346181
Description:  Kernel modules for TI WL12xx

Package: kmod-wl18xx
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-wlcore, wl18xx-firmware
Source: package/kernel/mac80211
SourceName: kmod-wl18xx
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 27634
Filename: kmod-wl18xx_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 27680
SHA256sum: 0f2b088bb5d463f457fc0b54501684928fb6a9c2b2b2b38607c5494f6d44fb61
Description:  Kernel modules for TI WL18xx

Package: kmod-wlcore
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-mmc, kmod-mac80211
Source: package/kernel/mac80211
SourceName: kmod-wlcore
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 84033
Filename: kmod-wlcore_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 84187
SHA256sum: f43b0ec4671cc6c938007ecc3953fc0852c748e5ecbc7466f68a9c7072d0da40
Description:  This module contains some common parts needed by TI Wireless drivers.

Package: kmod-zd1211rw
Version: 4.14.167+4.19.98-1-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-usb-core, kmod-mac80211
Source: package/kernel/mac80211
SourceName: kmod-zd1211rw
Section: kernel
Maintainer: Felix Fietkau <nbd@nbd.name>
Architecture: mipsel_24kc
Installed-Size: 37690
Filename: kmod-zd1211rw_4.14.167+4.19.98-1-1_mipsel_24kc.ipk
Size: 38326
SHA256sum: 857312526046ccfd560f3bada209a19c291424e6f4b30bc4abf8be602a261c7b
Description:  Zydas ZD1211 support

Package: kmod-zram
Version: 4.14.167-1
Depends: kernel (=4.14.167-1-d92769dc5268e102503ae83fe968a56c), kmod-lib-lzo, kmod-lib-lz4
Source: package/kernel/linux
SourceName: kmod-zram
License: GPL-2.0
Section: kernel
Architecture: mipsel_24kc
Installed-Size: 16566
Filename: kmod-zram_4.14.167-1_mipsel_24kc.ipk
Size: 17309
SHA256sum: f1595f7ef4129f5aa8d28c9b0db2bb57df32b0a16cca8b985c29e3598b57bb8c
Description:  Compressed RAM block device support

