// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "netgear,ex6150", "mediatek,mt7621-soc";
	model = "Netgear EX6150";

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_amber;
		led-running = &power_green;
		led-upgrade = &power_amber;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x4000000>;
	};

	chosen {
		bootargs = "console=ttyS0,57600";
	};

	leds {
		compatible = "gpio-leds";

		power_amber: power_amber {
			label = "ex6150:amber:power";
			gpios = <&gpio0 15 GPIO_ACTIVE_LOW>;
		};

		power_green: power_green {
			label = "ex6150:green:power";
			gpios = <&gpio0 13 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "ex6150:green:wps";
			gpios = <&gpio0 16 GPIO_ACTIVE_LOW>;
		};

		rightarrow {
			label = "ex6150:blue:rightarrow";
			gpios = <&gpio0 28 GPIO_ACTIVE_LOW>;
		};

		leftarrow {
			label = "ex6150:blue:leftarrow";
			gpios = <&gpio0 31 GPIO_ACTIVE_LOW>;
		};

		router_green {
			label = "ex6150:green:router";
			gpios = <&gpio0 29 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		router_red {
			label = "ex6150:red:router";
			gpios = <&gpio0 30 GPIO_ACTIVE_LOW>;
		};

		client_green {
			label = "ex6150:green:client";
			gpios = <&gpio1 1 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		client_red {
			label = "ex6150:red:client";
			gpios = <&gpio1 0 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		wps {
			label = "wps";
			gpios = <&gpio1 15 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		reset {
			label = "reset";
			gpios = <&gpio1 14 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		toggle {
			label = "AP/Extender toggle";
			gpios = <&gpio1 16 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			/* Active when switch is set to "Access Point" */
		};
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "config";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0xe80000>;
			};

			partition@ed0000 {
				label = "ML1";
				reg = <0xed0000 0x10000>;
				read-only;
			};

			partition@ef0000 {
				label = "ML2";
				reg = <0xef0000 0x20000>;
				read-only;
			};

			partition@f10000 {
				label = "ML3";
				reg = <0xf10000 0x20000>;
				read-only;
			};

			partition@f30000 {
				label = "ML4";
				reg = <0xf30000 0x20000>;
				read-only;
			};

			partition@f50000 {
				label = "ML5";
				reg = <0xf50000 0x20000>;
				read-only;
			};

			partition@f70000 {
				label = "ML6";
				reg = <0xf70000 0x20000>;
				read-only;
			};

			partition@f90000 {
				label = "ML7";
				reg = <0xf90000 0x20000>;
				read-only;
			};

			partition@fb0000 {
				label = "T_Meter1";
				reg = <0xfb0000 0x10000>;
				read-only;
			};

			partition@fc0000 {
				label = "T_Meter2";
				reg = <0xfc0000 0x10000>;
				read-only;
			};

			partition@fd0000 {
				label = "POT";
				reg = <0xfd0000 0x10000>;
				read-only;
			};

			partition@fe0000 {
				label = "board_data";
				reg = <0xfe0000 0x10000>;
				read-only;
			};

			partition@ff0000 {
				label = "nvram";
				reg = <0xff0000 0x10000>;
				read-only;
			};
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x8000>;
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&pcie1 {
	wifi@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x0000>;
		ieee80211-freq-limit = <2400000 2500000>;
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x00000004>;
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "sdhci", "rgmii2", "jtag";
			ralink,function = "gpio";
		};
	};
};
