// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "qca956x.dtsi"

/ {
	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	keys {
		compatible = "gpio-keys";

		wifi_button {
			label = "WiFi button";
			linux,code = <KEY_RFKILL>;
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};

		reset_button {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "tp-link:green:power";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wlan2g {
			label = "tp-link:green:wlan2g";
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		wlan5g {
			label = "tp-link:green:wlan5g";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wan_green {
			label = "tp-link:green:wan";
			gpios = <&gpio 20 GPIO_ACTIVE_LOW>;
		};

		wan_amber {
			label = "tp-link:amber:wan";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};

		lan {
			label = "tp-link:green:lan";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "tp-link:green:wps";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
		};
	};
};

&uart {
	status = "okay";
};

&pcie {
	status = "okay";
};

&eth0 {
	status = "okay";

	phy-mode = "mii";
	phy-handle = <&swphy4>;

	mtd-mac-address = <&mac 0x8>;
};

&eth1 {
	status = "okay";

	mtd-mac-address = <&mac 0x8>;
	mtd-mac-address-increment = <1>;
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
	mtd-mac-address = <&mac 0x8>;
};
