#!/bin/sh
#
# Copyright (C) 2018 OpenWrt.org
#

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
comfast,cf-e5)
	ucidef_add_gpio_switch "lte_power" "LTE Power" "14" "1"
	ucidef_add_gpio_switch "lte_wakeup" "LTE Wakeup" "11" "1"
	ucidef_add_gpio_switch "lte_poweroff" "LTE Poweroff" "1" "1"
	ucidef_add_gpio_switch "lte_reset" "LTE Reset" "12" "1"
	;;
dlink,dir-825-c1|\
dlink,dir-835-a1)
	ucidef_add_gpio_switch "wan_led_auto" "WAN LED Auto" "20" "0"
	;;
librerouter,librerouter-v1)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "1" "0"
	;;
tplink,archer-c25-v1)
	ucidef_add_gpio_switch "led_control" "LED control" "21" "0"
	ucidef_add_gpio_switch "led_reset" "LED reset" "19" "1"
	;;
tplink,cpe220-v3)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "20"
	;;
ubnt,nanostation-ac)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "3"
	;;
ubnt,nanostation-m)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "8"
	;;
ubnt,nanostation-m-xw)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "2"
	;;
ubnt,acb-isp)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "11"
	;;
zbtlink,zbt-wd323)
	ucidef_add_gpio_switch "io0" "IO#0" "0"
	ucidef_add_gpio_switch "io1" "IO#1" "1"
	ucidef_add_gpio_switch "io2" "IO#2" "2"
	ucidef_add_gpio_switch "io14" "IO#14" "14"
	;;
esac

board_config_flush

exit 0
