/dts-v1/;

#include "rt3883.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "sitecom,wlr-6000", "ralink,rt3883-soc";
	model = "Sitecom WLR-6000";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio1 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "wlr-6000:red:power";
			gpios = <&gpio0 1 GPIO_ACTIVE_LOW>;
		};

		ops {
			label = "wlr-6000:white:ops";
			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
		};
	};

	gpio_export {
		compatible = "gpio-export";
		#size-cells = <0>;

		usb {
			gpio-export,name = "usb";
			gpio-export,output = <1>;
			gpios = <&gpio0 9 GPIO_ACTIVE_HIGH>;
		};
	};
};

&gpio1 {
	status = "okay";
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "i2c", "jtag", "uartf";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	status = "okay";
	mtd-mac-address = <&factory 0x8004>;
	mtd-mac-address-increment = <1>;

	port@0 {
		phy-handle = <&phy0>;
		phy-mode = "rgmii";
	};

	mdio-bus {
		status = "okay";

		phy0: ethernet-phy@0 {
			reg = <0>;
			phy-mode = "rgmii";

			qca,ar8327-initvals = <
				0x04 0x07600000 /* PORT0 PAD MODE CTRL */
				0x0c 0x07600000 /* PORT6 PAD MODE CTRL */
				0x10 0x40000000 /* Power-on Strapping: 176-pin interface configuration */
				0x50 0xc437c437 /* LED Control Register 0 */
				0x54 0xc337c337 /* LED Control Register 1 */
				0x58 0x00000000 /* LED Control Register 2 */
				0x5c 0x03ffff00 /* LED Control Register 3 */
				0x7c 0x0000007e /* PORT0_STATUS */
				0x94 0x0000007e /* PORT6 STATUS */
			>;
		};
	};
};

&spi0 {
	status = "okay";

	m25p80@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <8600000>;
		m25p,fast-read;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x713000>;
			};

			partition@763000 {
				label = "manufacture";
				reg = <0x763000 0x7D000>;
				read-only;
			};

			partition@7E0000 {
				label = "backup";
				reg = <0x7E0000 0x10000>;
				read-only;
			};

			partition@7F0000 {
				label = "storage";
				reg = <0x7F0000 0x10000>;
				read-only;
			};
		};
	};
};

&pci {
	status = "okay";
};

&pci1 {
	status = "okay";

	wifi@0,0 {
		compatible = "pci1814,3091";
		reg = <0x10000 0 0 0 0>;
		ralink,mtd-eeprom = <&factory 0x8000>;
	};
};

&wmac {
	status = "okay";
	ralink,2ghz = <0>;
	ralink,mtd-eeprom = <&factory 0x0>;
};

&ehci {
	status = "okay";
};

&ohci {
	status = "okay";
};
