#!/bin/sh
#
# Copyright (C) 2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
traverse,ls1043v)
	ucidef_set_led_netdev "wan" "WAN LED" "ls1043v:yellow:wan" "eth4"
	;;
traverse,ls1043s)
	ucidef_set_led_netdev "wan" "WAN LED" "ls1043s:yellow:wan" "eth4"
	ucidef_set_led_netdev "xgact" "10G Activity" "ls1043s:yellow:10gact" "eth6"
	ucidef_set_led_netdev "xglink" "10G Link" "ls1043s:green:10glink" "eth6"
	;;
esac

board_config_flush

exit 0
