#!/bin/sh

[ -e /lib/firmware/$FIRMWARE ] && exit 0

. /lib/functions.sh
. /lib/functions/system.sh

ath9k_eeprom_die() {
	echo "ath9k eeprom: " "$*"
	exit 1
}

ath9k_eeprom_extract() {
	local part=$1
	local offset=$2
	local count=$3
	local mtd

	mtd=$(find_mtd_chardev $part)
	[ -n "$mtd" ] || \
		ath9k_eeprom_die "no mtd device found for partition $part"

	dd if=$mtd of=/lib/firmware/$FIRMWARE iflag=skip_bytes bs=$count skip=$offset count=1 2>/dev/null || \
		ath9k_eeprom_die "failed to extract from $mtd"
}

ath9k_eeprom_extract_reverse() {
	local part=$1
	local offset=$2
	local count=$3
	local mtd
	local reversed
	local caldata

	mtd=$(find_mtd_chardev "$part")
	reversed=$(hexdump -v -s $offset -n $count -e '/1 "%02x "' $mtd)

	for byte in $reversed; do
		caldata="\x${byte}${caldata}"
	done

	printf "%b" "$caldata" > /lib/firmware/$FIRMWARE
}

xor() {
	local val
	local ret="0x$1"
	local retlen=${#1}

	shift
	while [ -n "$1" ]; do
		val="0x$1"
		ret=$((ret ^ val))
		shift
	done

	printf "%0${retlen}x" "$ret"
}

ath9k_patch_fw_mac() {
	local mac=$1
	local mac_offset=$2
	local chksum_offset=$3
	local xor_mac
	local xor_fw_mac
	local xor_fw_chksum

	[ -z "$mac" -o -z "$mac_offset" ] && return

	[ -n "$chksum_offset" ] && {
		xor_mac=${mac//:/}
		xor_mac="${xor_mac:0:4} ${xor_mac:4:4} ${xor_mac:8:4}"

		xor_fw_mac=$(hexdump -v -n 6 -s $mac_offset -e '/1 "%02x"' /lib/firmware/$FIRMWARE)
		xor_fw_mac="${xor_fw_mac:0:4} ${xor_fw_mac:4:4} ${xor_fw_mac:8:4}"

		xor_fw_chksum=$(hexdump -v -n 2 -s $chksum_offset -e '/1 "%02x"' /lib/firmware/$FIRMWARE)
		xor_fw_chksum=$(xor $xor_fw_chksum $xor_fw_mac $xor_mac)

		printf "%b" "\x${xor_fw_chksum:0:2}\x${xor_fw_chksum:2:2}" | \
			dd of=/lib/firmware/$FIRMWARE conv=notrunc bs=1 seek=$chksum_offset count=2
	}

	macaddr_2bin $mac | dd of=/lib/firmware/$FIRMWARE conv=notrunc oflag=seek_bytes bs=6 seek=$mac_offset count=1
}

ath9k_patch_fw_mac_crc() {
	local mac=$1
	local mac_offset=$2
	local chksum_offset=$((mac_offset - 10))

	ath9k_patch_fw_mac "${mac}" "${mac_offset}" "${chksum_offset}"
}

board=$(board_name)

case "$FIRMWARE" in
"ath9k-eeprom-ahb-18100000.wmac.bin")
	case $board in
	avm,fritz4020)
		ath9k_eeprom_extract_reverse "urlader" 5441 1088
		;;
	dlink,dir-825-c1|\
	dlink,dir-835-a1)
		ath9k_eeprom_extract "art" 4096 1088
		ath9k_patch_fw_mac $(mtd_get_mac_text "mac" 4) 2
		;;
	dlink,dir-859-a1|\
	nec,wg1200cr|\
	wd,mynet-n750)
		ath9k_eeprom_extract "art" 4096 1088
		ath9k_patch_fw_mac $(mtd_get_mac_ascii devdata "wlan24mac") 2
		;;
	engenius,ecb1750)
		ath9k_eeprom_extract "art" 4096 1088
		ath9k_patch_fw_mac $(macaddr_add $(mtd_get_mac_ascii u-boot-env "athaddr") +1) 2
		;;
	engenius,epg5000|\
	iodata,wn-ac1167dgr|\
	iodata,wn-ac1600dgr|\
	iodata,wn-ac1600dgr2|\
	iodata,wn-ag300dgr)
		ath9k_eeprom_extract "art" 4096 1088
		ath9k_patch_fw_mac $(mtd_get_mac_ascii u-boot-env ethaddr) 2
		;;
	nec,wg800hp)
		ath9k_eeprom_extract "art" 4096 1088
		ath9k_patch_fw_mac $(mtd_get_mac_text board_data 1664) 2
		;;
	*)
		ath9k_eeprom_die "board $board is not supported yet"
		;;
	esac
	;;
"ath9k-eeprom-pci-0000:00:00.0.bin")
	case $board in
	avm,fritz300e)
		ath9k_eeprom_extract_reverse "urloader" 5441 1088
		;;
	buffalo,whr-g301n|\
	buffalo,wzr-hp-g302h-a1a0|\
	tplink,tl-wr841-v5|\
	tplink,tl-wr941-v4)
		ath9k_eeprom_extract "art" 4096 3768
		;;
	buffalo,wzr-hp-g450h)
		ath9k_eeprom_extract "art" 4096 1088
		;;
	dlink,dir-825-c1|\
	dlink,dir-835-a1)
		ath9k_eeprom_extract "art" 20480 1088
		ath9k_patch_fw_mac $(macaddr_add $(mtd_get_mac_text "mac" 24) 1) 2
		;;
	ocedo,raccoon|\
	tplink,tl-wdr3600-v1|\
	tplink,tl-wdr4300-v1|\
	tplink,tl-wdr4300-v1-il|\
	tplink,tl-wdr4900-v2|\
	winchannel,wb2000)
		ath9k_eeprom_extract "art" 20480 1088
		;;
	netgear,wnr612-v2|\
	on,n150r|\
	pcs,cap324|\
	tplink,tl-mr3220-v1|\
	tplink,tl-mr3420-v1|\
	tplink,tl-wr2543-v1|\
	tplink,tl-wr740n-v1|\
	tplink,tl-wr740n-v3|\
	tplink,tl-wr741-v1|\
	tplink,tl-wr743nd-v1|\
	tplink,tl-wr841-v7|\
	tplink,tl-wr842n-v1|\
	ubnt,airrouter|\
	ubnt,bullet-m|\
	ubnt,nanostation-m|\
	ubnt,rocket-m)
		ath9k_eeprom_extract "art" 4096 4096
		;;
	pqi,air-pen)
		ath9k_eeprom_extract "art" 4096 2002
		;;
	ubnt,unifi)
		ath9k_eeprom_extract "art" 4096 2048
		;;
	wd,mynet-n750)
		ath9k_eeprom_extract "art" 20480 1088
		ath9k_patch_fw_mac $(mtd_get_mac_ascii devdata "wlan5mac") 2
		;;
	wd,mynet-wifi-rangeextender)
		ath9k_eeprom_extract "art" 4096 4096
		ath9k_patch_fw_mac $(nvram get wl0_hwaddr) 2
		;;
	*)
		ath9k_eeprom_die "board $board is not supported yet"
		;;
	esac
	;;
"ath9k-eeprom-pci-0000:00:11.0.bin")
	case $board in
	buffalo,wzr-hp-ag300h|\
	netgear,wndr3700|\
	netgear,wndr3700v2|\
	netgear,wndr3800)
		ath9k_eeprom_extract "art" 4096 3768
		;;
	dlink,dir-825-b1)
		ath9k_eeprom_extract "caldata" 4096 3768
		ath9k_patch_fw_mac_crc $(mtd_get_mac_text "caldata" 65440) 524
		;;
	*)
		ath9k_eeprom_die "board $board is not supported yet"
		;;
	esac
	;;
"ath9k-eeprom-pci-0000:00:12.0.bin")
	case $board in
	buffalo,wzr-hp-ag300h|\
	netgear,wndr3700|\
	netgear,wndr3700v2|\
	netgear,wndr3800)
		ath9k_eeprom_extract "art" 20480 3768
		;;
	dlink,dir-825-b1)
		ath9k_eeprom_extract "caldata" 20480 3768
		ath9k_patch_fw_mac_crc $(macaddr_add $(mtd_get_mac_text "caldata" 65460) 1) 524
		;;
	*)
		ath9k_eeprom_die "board $board is not supported yet"
		;;
	esac
	;;
esac
