// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "qca956x.dtsi"

/ {
	compatible = "tplink,archer-c5x", "qca,qca9560";

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	led_spi {
		compatible = "spi-gpio";
		#address-cells = <1>;
		#size-cells = <0>;

		gpio-sck = <&gpio 18 GPIO_ACTIVE_HIGH>;
		gpio-mosi = <&gpio 17 GPIO_ACTIVE_HIGH>;
		cs-gpios = <&gpio 20 GPIO_ACTIVE_HIGH>;
		num-chipselects = <1>;

		led_gpio: led_gpio@0 {
			compatible = "fairchild,74hc595";
			reg = <0>;
			gpio-controller;
			#gpio-cells = <2>;
			registers-number = <1>;
			spi-max-frequency = <10000000>;
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		wps_button {
			label = "WPS button";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};

		wifi_button {
			label = "WiFi button";
			linux,code = <KEY_RFKILL>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};

		reset_button {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
		};
	};

	gpio-export {
		compatible = "gpio-export";

		gpio_shift_register_oe {
			gpio-export,name = "tp-link:oe:sr";
			gpio-export,output = <0>;
			gpios = <&gpio 16 GPIO_ACTIVE_HIGH>;
		};

		gpio_shift_register_reset {
			gpio-export,name = "tp-link:reset:sr";
			gpio-export,output = <1>;
			gpios = <&gpio 19 GPIO_ACTIVE_HIGH>;
		};

	};
};

&uart {
	status = "okay";
};

&gpio {
	status = "okay";
};

&pcie {
	status = "okay";
};

&eth0 {
	phy-mode = "mii";
	phy-handle = <&swphy0>;

	gmac-config {
		device = <&gmac>;

		switch-phy-addr-swap = <1>;
		switch-phy-swap = <1>;
	};
};
