/dts-v1/;

#include "mt7620n.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "dlink,dwr-116-a1", "ralink,mt7620n-soc";
	model = "D-Link DWR-116 A1/A2";

	aliases {
		led-boot = &led_status;
		led-failsafe = &led_status;
		led-running = &led_status;
		led-upgrade = &led_status;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		wps {
			label = "wps";
			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		reset {
			label = "reset";
			gpios = <&gpio0 1 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_status: status {
			label = "dwr-116-a1:green:status";
			gpios = <&gpio0 0 GPIO_ACTIVE_HIGH>;
		};

		wifi {
			label = "dwr-116-a1:green:wifi";
			gpios = <&gpio3 0 GPIO_ACTIVE_LOW>;
		};
	};
};

&gpio1 {
	status = "okay";
};

&gpio3 {
	status = "okay";
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "jboot";
				reg = <0x0 0x10000>;
				read-only;
			};

			partition@10000 {
				compatible = "amit,jimage";
				label = "firmware";
				reg = <0x10000 0x7e0000>;
			};

			config: partition@7f0000 {
				label = "config";
				reg = <0x7f0000 0x10000>;
				read-only;
			};
		};
	};
};

&ehci {
	status = "okay";
};

&ohci {
	status = "okay";
};

&pinctrl {
	state_default: pinctrl0 {
		default {
			ralink,group = "i2c", "wled";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	mediatek,portmap = "llllw";
	pinctrl-names = "default";
	pinctrl-0 = <&ephy_pins>;
};
