#!/bin/sh
#
# Copyright (C) 2012-2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
"cloudengines,pogoe02")
	ucidef_set_led_default "health" "health" "pogo_e02:green:health" "1"
	ucidef_set_led_default "fault" "fault" "pogo_e02:orange:fault" "1"
	;;
"iom,ix2-200")
	ucidef_set_led_timer "health" "health" "status:white:rebuild_led" "200" "800"
	;;
"linksys,audi")
	ucidef_set_led_default "power" "power" "audi:green:power" "1"
	;;
"linksys,viper")
	ucidef_set_led_default "health" "health" "viper:white:health" "1"
	ucidef_set_led_default "pulse" "pulse" "viper:white:pulse" "1"
	;;
"raidsonic,ib-nas62x0")
	ucidef_set_led_default "health" "health" "ib62x0:green:os" "1"
	ucidef_set_led_default "fault" "fault" "ib62x0:red:os" "1"
	;;
"seagate,dockstar")
	ucidef_set_led_default "health" "health" "status:green:health" "1"
	ucidef_set_led_default "fault" "fault" "status:orange:fault" "1"
	;;
"seagate,goflexhome"|\
"seagate,goflexnet")
	ucidef_set_led_default "health" "health" "status:green:health" "1"
	ucidef_set_led_default "fault" "fault" "status:orange:fault" "0"
	;;
"zyxel,nsa310b")
	ucidef_set_led_default "health" "health" "nsa310:green:sys" "1"
	ucidef_set_led_usbhost "usb" "USB" "nsa310:green:usb"
	ucidef_set_led_ataport "hdd" "HDD" "nsa310:green:hdd" "1"
	ucidef_set_led_ataport "esata" "eSata" "nsa310:green:esata" "2"
	;;
"zyxel,nsa325")
	ucidef_set_led_default "health" "health" "nsa325:green:sys" "1"
	ucidef_set_led_usbhost "usb" "USB" "nsa325:green:usb"
	ucidef_set_led_ataport "hdd1" "HDD1" "nsa325:green:hdd1" "1"
	ucidef_set_led_ataport "hdd2" "HDD2" "nsa325:green:hdd2" "2"
	;;
esac

board_config_flush

exit 0
