// SPDX-License-Identifier: GPL-2.0
/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "ar9132.dtsi"

/ {
	compatible = "tplink,tl-wr941-v2", "qca,ar9132";
	model = "TP-Link TL-WR941N/ND v2/v3";

	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
	};

	keys {
		compatible = "gpio-keys";

		button0 {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		button1 {
			label = "qss";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_system: system {
			label = "tp-link:green:system";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};

		qss_r {
			label = "tp-link:red:qss";
			gpios = <&gpio 4 GPIO_ACTIVE_HIGH>;
		};

		qss_g {
			label = "tp-link:green:qss";
			gpios = <&gpio 5 GPIO_ACTIVE_HIGH>;
		};

		wlan {
			label = "tp-link:green:wlan";
			gpios = <&gpio 9 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};

	dsa {
		compatible = "marvell,dsa";
		#address-cells = <1>;
		#size-cells = <0>;

		dsa,mii-bus = <&mdio0>;
		dsa,ethernet = <&eth0>;

		switch@0 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0>;

			port@0 {
				reg = <0>;
				label = "wan";
			};

			port@1 {
				reg = <1>;
				label = "lan1";
			};

			port@2 {
				reg = <2>;
				label = "lan2";
			};

			port@3 {
				reg = <3>;
				label = "lan3";
			};

			port@4 {
				reg = <4>;
				label = "lan4";
			};

			port@5 {
				reg = <5>;
				label = "cpu";
			};
		};
	};
};

&uart {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				label = "u-boot";
				reg = <0x000000 0x20000>;
				read-only;
			};

			partition@20000 {
				compatible = "tplink,firmware";
				label = "firmware";
				reg = <0x020000 0x3d0000>;
			};

			art: partition@3f0000 {
				label = "art";
				reg = <0x3f0000 0x10000>;
				read-only;
			};
		};
	};
};

&mdio0 {
	status = "okay";
};

&eth0 {
	status = "okay";

	phy-mode = "rmii";
	mtd-mac-address = <&uboot 0x1fc00>;

	fixed-link {
		speed = <100>;
		full-duplex;
	};
};

&wmac {
	status = "okay";
	mtd-cal-data = <&art 0x1000>;
	mtd-mac-address = <&uboot 0x1fc00>;
};
