/dts-v1/;

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "buffalo,wsr-600dhp", "mediatek,mt7621-soc";
	model = "Buffalo WSR-600DHP";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x4000000>;
	};

	chosen {
		bootargs = "console=ttyS0,57600";
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "wsr-600:green:power";
			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
		};

		wifi_o {
			label = "wsr-600:orange:wifi";
			gpios = <&gpio1 9 GPIO_ACTIVE_LOW>;
		};

		diag {
			label = "wsr-600:orange:diag";
			gpios = <&gpio1 10 GPIO_ACTIVE_LOW>;
		};

		wifi_g {
			label = "wsr-600:green:wifi";
			gpios = <&gpio1 12 GPIO_ACTIVE_LOW>;
		};

		router_o {
			label = "wsr-600:orange:router";
			gpios = <&gpio1 13 GPIO_ACTIVE_LOW>;
		};

		router_g {
			label = "wsr-600:green:router";
			gpios = <&gpio1 14 GPIO_ACTIVE_LOW>;
		};

		internet_o {
			label = "wsr-600:orange:internet";
			gpios = <&gpio1 15 GPIO_ACTIVE_LOW>;
		};

		internet_g {
			label = "wsr-600:green:internet";
			gpios = <&gpio1 16 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		power {
			label = "power";
			gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_POWER>;
		};

		reset {
			label = "reset";
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		aoss {
			label = "aoss";
			gpios = <&gpio0 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		auto {
			label = "mode";
			gpios = <&gpio0 7 GPIO_ACTIVE_HIGH>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
		};

		ap {
			label = "ap";
			gpios = <&gpio0 6 GPIO_ACTIVE_HIGH>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
		};

		router {
			label = "router";
			gpios = <&gpio0 10 GPIO_ACTIVE_HIGH>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
		};
	};

	gpio_poweroff {
		compatible = "gpio-poweroff";
		gpios = <&gpio1 11 GPIO_ACTIVE_LOW>;
	};
};

&spi0 {
	status = "okay";

	m25p80@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0xfb0000>;
			};
		};
	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "i2c", "uart2", "uart3", "rgmii2", "sdhci";
			ralink,function = "gpio";
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	rt5592@0,0 {
		reg = <0x0000 0 0 0 0>;
		ralink,mtd-eeprom = <&factory 0x8000>;
	};
};

&pcie1 {
	mt76@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x0000>;
	};
};

&xhci {
	status = "disabled";
};
