// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "qca956x.dtsi"

/ {
	compatible = "tplink,re450-v2", "qca,qca9563";
	model = "TP-Link RE450 v2";

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	aliases {
		led-boot = &system;
		led-failsafe = &system;
		led-running = &system;
		led-upgrade = &system;
		mdio-gpio0 = &mdio2;
	};

	leds {
		compatible = "gpio-leds";

		system: power {
			label = "tp-link:blue:power";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};

		wlan2g {
			label = "tp-link:blue:wlan2g";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		wlan5g {
			label = "tp-link:blue:wlan5g";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		lan_link {
			label = "tp-link:green:lan_link";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};

		lan_data {
			label = "tp-link:green:lan_data";
			gpios = <&gpio 9 GPIO_ACTIVE_LOW>;
		};

		wps_blue {
			label = "tp-link:blue:wps";
			gpios = <&gpio 17 GPIO_ACTIVE_HIGH>;
		};

		wps_red {
			label = "tp-link:red:wps";
			gpios = <&gpio 20 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		power {
			label = "Power button";
			linux,code = <KEY_POWER>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		leds {
			label = "LED control button";
			linux,code = <BTN_0>;
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		wps {
			label = "WPS button";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	mdio2: mdio {
		compatible = "virtual,mdio-gpio";

		gpios = <&gpio 3 GPIO_ACTIVE_HIGH>, /* MDC */
			<&gpio 4 GPIO_ACTIVE_HIGH>; /* MDIO */
		#address-cells = <1>;
		#size-cells = <0>;

		phy0: ethernet-phy@4 {
			reg = <4>;
			device_type = "ethernet-phy";
			reset-gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};
	};
};

&pcie {
	status = "okay";
};

&uart {
	status = "okay";
};

&gpio {
	status = "okay";
};

&spi {
	status = "okay";
	num-cs = <1>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x020000>;
				read-only;
			};

			partition@20000 {
				compatible = "tplink,firmware";
				label = "firmware";
				reg = <0x020000 0x5e0000>;
			};

			partition@600000 {
				label = "partition-table";
				reg = <0x600000 0x010000>;
				read-only;
			};

			info: partition@610000 {
				label = "info";
				reg = <0x610000 0x020000>;
				read-only;
			};

			partition@630000 {
				label = "config";
				reg = <0x630000 0x020000>;
				read-only;
			};

			art: partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x010000>;
				read-only;
			};
		};
	};
};

&eth0 {
	status = "okay";
	mtd-mac-address = <&info 0x8>;
	phy-handle = <&phy0>;
};

&wmac {
	status = "okay";
	mtd-cal-data = <&art 0x1000>;
	mtd-mac-address = <&info 0x8>;
};
