#!/bin/sh
#
# Copyright (C) 2013 OpenWrt.org
#

. /lib/ramips.sh

ramips_set_preinit_iface() {
	RT3X5X=`cat /proc/cpuinfo | egrep "(RT3.5|RT5350|MT7628|MT7688|MT7620|MT7621)"`

	if [ -n "${RT3X5X}" ]; then
		# The ethernet switch driver enables VLAN by default, but
		# failsafe uses eth0, making the device unreachable:
		# https://dev.openwrt.org/ticket/18768
		case "${RT3X5X}" in
		*MT7620*)
			ralink_switchdev=mt7620
			;;
		*MT7621*)
			ralink_switchdev=mt7530
			;;
		*)
			ralink_switchdev=rt305x
			;;
		esac
		swconfig dev $ralink_switchdev set reset 1
		swconfig dev $ralink_switchdev set enable_vlan 0
		swconfig dev $ralink_switchdev set apply 1
	fi

	ifname=eth0
}

boot_hook_add preinit_main ramips_set_preinit_iface
