// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "qca953x.dtsi"

/ {
	compatible = "engenius,ews511ap", "qca,qca9531";
	model = "EnGenius EWS511AP";

	keys {
		compatible = "gpio-keys-polled";

		poll-interval = <20>;
		pinctrl-names = "default";
		pinctrl-0 = <&jtag_disable_pins>;

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};
	};

	aliases {
		led-boot = &power_led;
		led-failsafe = &power_led;
		led-running = &power_led;
		led-upgrade = &power_led;
	};

	leds {
		compatible = "gpio-leds";

		power_led: power {
			label = "ews511ap:amber:power";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		lan1 {
			label = "ews511ap:blue:lan1";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		lan2 {
			label = "ews511ap:blue:lan2";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		wlan2g {
			label = "ews511ap:green:wlan2g";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wlan5g {
			label = "ews511ap:green:wlan5g";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	watchdog {
		compatible = "linux,wdt-gpio";

		gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		hw_algo = "toggle";
		/* hw_margin_ms is actually 300s but driver limits it to 60s */
		hw_margin_ms = <60000>;
		always-running;
	};
};

&wdt {
	status = "okay";
};

&rst {
	status = "okay";
};

&pcie0 {
	status = "okay";
};

&uart {
	status = "okay";
};

&spi {
	status = "okay";
	num-cs = <0>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			ubootenv: partition@40000 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
			};

			art: partition@50000 {
				label = "art";
				reg = <0x050000 0x010000>;
				read-only;
			};

			partition@60000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x060000 0xfa0000>;
			};
		};
	};
};

&eth0 {
	status = "okay";
	phy-handle = <&swphy4>;
};

&eth1 {
	status = "okay";
};

&wmac {
	status = "okay";
	mtd-cal-data = <&art 0x1000>;
};
