/dts-v1/;

#include "rt3050.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "belkin,f5d8235-v2", "ralink,rt3052-soc";
	model = "Belkin F5D8235 v2";

	aliases {
		led-boot = &led_router;
		led-failsafe = &led_router;
		led-running = &led_router;
		led-upgrade = &led_router;
	};

	cfi@1f000000 {
		compatible = "cfi-flash";
		reg = <0x1f000000 0x800000>;
		bank-width = <2>;
		device-width = <2>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				label = "uboot";
				reg = <0x0 0x50000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x790000>;
			};

			partition@7e0000 {
				label = "nvram";
				reg = <0x7e0000 0x10000>;
			};

			factory: partition@7f0000 {
				label = "factory";
				reg = <0x7f0000 0x10000>;
			};
		};
	};

	rtl8366rb {
		compatible = "realtek,rtl8366rb";
		gpio-sda = <&gpio0 1 GPIO_ACTIVE_HIGH>;
		gpio-sck = <&gpio0 2 GPIO_ACTIVE_HIGH>;
	};

	leds {
		compatible = "gpio-leds";

		internet {
			label = "f5d8235-v2:blue:internet";
			gpios = <&gpio0 5 GPIO_ACTIVE_LOW>;
		};

		internet2 {
			label = "f5d8235-v2:amber:internet";
			gpios = <&gpio0 6 GPIO_ACTIVE_LOW>;
		};

		modem {
			label = "f5d8235-v2:blue:modem";
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
		};

		modem2 {
			label = "f5d8235-v2:amber:modem";
			gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
		};

		led_router: router {
			label = "f5d8235-v2:blue:router";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
		};

		storage {
			label = "f5d8235-v2:blue:storage";
			gpios = <&gpio0 23 GPIO_ACTIVE_LOW>;
			trigger-sources = <&otg_port1>;
			linux,default-trigger = "usbport";
		};

		storage2 {
			label = "f5d8235-v2:amber:storage";
			gpios = <&gpio0 22 GPIO_ACTIVE_LOW>;
		};

		security {
			label = "f5d8235-v2:blue:security";
			gpios = <&gpio0 13 GPIO_ACTIVE_LOW>;
		};

		security2 {
			label = "f5d8235-v2:amber:security";
			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
		};
	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "spi", "i2c", "jtag", "mdio", "uartf";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	mtd-mac-address = <&uboot 0x40004>;
	pinctrl-names = "default";
	pinctrl-0 = <&rgmii_pins>;
};

&esw {
	ralink,rgmii = <1>;
	mediatek,portmap = <0x3f>;
	ralink,fct2 = <0x0002500c>;
	/*
	 * ext phy base addr 31, rx/tx clock skew 0,
	 * turbo mii off, rgmi 3.3v off, port 5 polling off
	 * port5: enabled, gige, full-duplex, rx/tx-flow-control
	 * port6: enabled, gige, full-duplex, rx/tx-flow-control
	*/
	ralink,fpa2 = <0x1f003fff>;
};

&wmac {
	ralink,mtd-eeprom = <&uboot 0x40000>;
};

&otg {
	status = "okay";
};
