#!/bin/sh
#
# Copyright (C) 2013-2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh

board_config_update

case "$(board_name)" in
a4001n1)
	ucidef_set_led_netdev "lan" "LAN" "A4001N1:green:eth" "eth0"
	ucidef_set_led_usbdev "usb" "USB" "A4001N1:green:3g" "1-1"
	;;
a4001n)
	ucidef_set_led_usbdev "usb" "USB" "A4001N:green:usb" "1-1"
	;;
ad1018-nor)
	ucidef_set_led_netdev "wlan0" "WLAN" "AD1018:green:wifi" "wlan0"
	;;
ar-5315u)
	ucidef_set_led_usbdev "usb" "USB" "AR-5315u:green:usb" "1-1"
	;;
av4202n)
	ucidef_set_led_netdev "wlan0" "WLAN" "AV4202N:blue:wifi" "wlan0"
	;;
cpva502p)
	ucidef_set_led_netdev "lan" "LAN" "CPVA502+:amber:link" "eth0"
	;;
dgnd3700v1_dgnd3800b)
	ucidef_set_led_netdev "lan" "LAN" "DGND3700v1_3800B:green:lan" "eth0.1"
	ucidef_set_led_netdev "wan" "WAN" "DGND3700v1_3800B:green:inet" "eth0.2"
	ucidef_set_led_netdev "wlan0" "WIFI2G" "DGND3700v1_3800B:green:wifi2g" "wlan0"
	ucidef_set_led_netdev "wlan1" "WIFI5G" "DGND3700v1_3800B:blue:wifi5g" "wlan1"
	ucidef_set_led_usbdev "usb1" "USB1" "DGND3700v1_3800B:green:usb-back" "1-1"
	ucidef_set_led_usbdev "usb2" "USB2" "DGND3700v1_3800B:green:usb-front" "1-2"
	;;
evg2000)
	ucidef_set_led_netdev "lan" "LAN" "EVG2000:green:lan" "eth0"
	ucidef_set_led_netdev "wan" "WAN" "EVG2000:green:wan" "eth1"
	ucidef_set_led_netdev "wlan0" "WIFI" "EVG2000:green:wireless" "wlan0"
	ucidef_set_led_usbdev "usb1" "USB1" "EVG2000:green:voip1" "1-1"
	ucidef_set_led_usbdev "usb2" "USB2" "EVG2000:green:voip2" "1-2"
	;;
fast2704n)
	ucidef_set_led_netdev "wan" "WAN" "F@ST2704N:green:inet" "eth0.2"
	;;
fast2704v2)
	ucidef_set_led_usbdev "usb" "USB" "F@ST2704V2:green:usb" "1-1"
	;;
hg553)
	ucidef_set_led_netdev "lan" "LAN" "HW553:blue:lan" "eth0"
	ucidef_set_led_usbdev "usb1" "USB1" "HW553:red:hspa" "1-1"
	ucidef_set_led_usbdev "usb2" "USB2" "HW553:blue:hspa" "1-2"
	;;
hg556a_*)
	ucidef_set_led_netdev "lan" "LAN" "HW556:red:dsl" "eth0"
	ucidef_set_led_usbdev "usb" "USB" "HW556:red:hspa" "1-2"
	;;
hg622)
	ucidef_set_led_usbdev "usb" "USB" "HG622:green:usb" "1-2"
	;;
hg655b)
	ucidef_set_led_usbdev "usb" "USB" "HW65x:green:usb" "1-2"
	;;
homehub2a)
	ucidef_set_led_netdev "lan" "LAN" "HOMEHUB2A:blue:broadband" "eth0.1"
	ucidef_set_led_netdev "wlan0" "WIFI" "HOMEHUB2A:green:wireless" "wlan0"
	ucidef_set_led_usbdev "usb1" "USB1" "HOMEHUB2A:blue:phone" "1-1"
	ucidef_set_led_usbdev "usb2" "USB2" "HOMEHUB2A:green:phone" "2-1"
	;;
livebox1)
	ucidef_set_led_netdev "lan" "LAN" "Livebox1:red:traffic" "eth0"
	ucidef_set_led_netdev "wan" "WAN" "Livebox1:red:adsl" "eth1"
	ucidef_set_led_netdev "wlan0" "WIFI" "Livebox1:red:wifi" "wlan0"
	;;
r1000h)
	ucidef_set_led_usbport "usb" "USB" "R1000H:green:usb" "usb1-port1" "usb2-port1"
	;;
r5010un_v2)
	ucidef_set_led_usbdev "usb" "USB" "R5010UNv2:green:usb" "1-1"
	;;
esac

board_config_flush

exit 0
