#!/bin/sh

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)
boardname="${board##*,}"

case "$board" in
8dev,carambola2)
	ucidef_set_led_netdev "lan" "LAN" "$boardname:orange:eth0" "eth0"
	ucidef_set_led_switch "wan" "WAN" "$boardname:orange:eth1" "switch0" "0x04"
	;;
avm,fritz300e)
	ucidef_set_led_netdev "lan" "LAN" "$boardname:green:lan" "eth0"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "$boardname:green:rssi0" "wlan0" "1" "100"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "$boardname:green:rssi1" "wlan0" "20" "100"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "$boardname:green:rssi2" "wlan0" "40" "100"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "$boardname:green:rssi3" "wlan0" "60" "100"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "$boardname:green:rssi4" "wlan0" "80" "100"
	;;
avm,fritz4020)
	ucidef_set_led_netdev "wan" "WAN" "$boardname:green:wan" "eth1"
	ucidef_set_led_switch "lan" "LAN" "$boardname:green:lan" "switch0" "0x1E"
	;;
buffalo,whr-g301n)
	ucidef_set_led_netdev "wan" "WAN" "$boardname:green:wan" "eth0"
	ucidef_set_led_switch "lan1" "LAN1" "$boardname:green:lan1" "switch0" "0x02"
	ucidef_set_led_switch "lan2" "LAN2" "$boardname:green:lan2" "switch0" "0x04"
	ucidef_set_led_switch "lan3" "LAN3" "$boardname:green:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan4" "LAN4" "$boardname:green:lan4" "switch0" "0x10"
	;;
comfast,cf-e110n-v2)
	ucidef_set_led_netdev "lan" "LAN" "$boardname:green:lan" "eth1"
	ucidef_set_led_switch "wan" "WAN" "$boardname:green:wan" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "$boardname:green:wlan" "phy0tpt"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "$boardname:red:rssilow" "wlan0" "1" "100"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "$boardname:red:rssimediumlow" "wlan0" "26" "100"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "$boardname:green:rssimediumhigh" "wlan0" "51" "100"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "$boardname:green:rssihigh" "wlan0" "76" "100"
	;;
comfast,cf-e120a-v3)
	ucidef_set_led_netdev "lan" "LAN" "$boardname:green:lan" "eth1"
	ucidef_set_led_switch "wan" "WAN" "$boardname:green:wan" "switch0" "0x04"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "$boardname:red:rssilow" "wlan0" "1" "100"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "$boardname:red:rssimediumlow" "wlan0" "26" "100"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "$boardname:green:rssimediumhigh" "wlan0" "51" "100"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "$boardname:green:rssihigh" "wlan0" "76" "100"
	;;
comfast,cf-e5)
	ucidef_set_led_switch "lan" "LAN" "$boardname:blue:lan" "switch0" "0x02"
	ucidef_set_led_netdev "wan" "WAN" "$boardname:blue:wan" "eth1"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "$boardname:blue:rssi0" "wlan0" "1" "100"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "$boardname:blue:rssi1" "wlan0" "33" "100"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "$boardname:blue:rssi2" "wlan0" "66" "100"
	;;
dlink,dir-859-a1)
	ucidef_set_led_switch "internet" "WAN" "$boardname:green:internet" "switch0" "0x20"
	;;
engenius,ecb1750)
	ucidef_set_led_netdev "lan" "LAN" "$boardname:blue:lan" "eth0"
	;;
engenius,ews511ap)
	ucidef_set_led_netdev "lan1" "LAN1" "$boardname:blue:lan1" "eth1"
	ucidef_set_led_netdev "lan2" "LAN2" "$boardname:blue:lan2" "eth0"
	;;
etactica,eg200)
	ucidef_set_led_netdev "lan" "LAN" "$boardname:red:eth0" "eth0"
	ucidef_set_led_oneshot "modbus" "Modbus" "$boardname:red:modbus" "100" "33"
	ucidef_set_led_default "etactica" "etactica" "$boardname:red:etactica" "ignore"
	;;
glinet,gl-ar150)
	ucidef_set_led_netdev "wan" "WAN" "$boardname:green:wan" "eth1"
	ucidef_set_led_switch "lan" "LAN" "$boardname:green:lan" "switch0" "0x02"
	;;
glinet,gl-ar300m-nand|\
glinet,gl-ar300m-nor)
	ucidef_set_led_netdev "lan" "LAN" "gl-ar300m:green:lan" "eth0"
	;;
glinet,gl-ar300m-lite)
	ucidef_set_led_netdev "lan" "LAN" "gl-ar300m-lite:green:lan" "eth0"
	;;
glinet,gl-x750)
	ucidef_set_led_netdev "wan" "WAN" "$boardname:green:wan" "eth1"
	;;
netgear,wnr612-v2|\
on,n150r)
	ucidef_set_led_netdev "wan" "WAN" "netgear:green:wan" "eth0"
	ucidef_set_led_switch "lan1" "LAN1" "netgear:green:lan1" "switch0" "0x02" "0x0f"
	ucidef_set_led_switch "lan2" "LAN2" "netgear:green:lan2" "switch0" "0x04" "0x0f"
	;;
pcs,cap324)
	ucidef_set_led_netdev "lan" "LAN" "pcs:lan:green" "eth0"
	;;
pcs,cr3000)
	ucidef_set_led_netdev "wan" "WAN" "pcs:blue:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "pcs:blue:lan1" "switch0" "0x04"
	ucidef_set_led_switch "lan2" "LAN2" "pcs:blue:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "pcs:blue:lan3" "switch0" "0x10"
	ucidef_set_led_switch "lan4" "LAN4" "pcs:blue:lan4" "switch0" "0x02"
	;;
tplink,archer-a7-v5|\
tplink,archer-c7-v4|\
tplink,archer-c7-v5)
	ucidef_set_led_switch "wan" "WAN" "tp-link:green:wan" "switch0" "0x02"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x04"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x10"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x20"
	;;
tplink,archer-c2-v3|\
tplink,tl-wr1043nd-v4|\
tplink,tl-wr1043n-v5)
	ucidef_set_led_switch "wan" "WAN" "tp-link:green:wan" "switch0" "0x20"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x10"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x04"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x02"
	;;
tplink,archer-c6-v2)
	ucidef_set_led_switch "lan" "LAN" "tp-link:green:lan" "switch0" "0x3C"
	ucidef_set_led_switch "wan" "WAN" "tp-link:green:wan" "switch0" "0x02"
	;;
tplink,archer-c25-v1|\
tplink,tl-wr841-v9|\
tplink,tl-wr841-v10|\
tplink,tl-wr841-v11|\
tplink,tl-wr841-v12|\
tplink,tl-wr842n-v3)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x10"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x04"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x02"
	;;
tplink,archer-c58-v1|\
tplink,archer-c59-v1|\
tplink,archer-c60-v1|\
tplink,archer-c60-v2)
	ucidef_set_led_switch "lan" "LAN" "tp-link:green:lan" "switch0" "0x1E"
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth1"
	;;
tplink,archer-d50-v1)
	ucidef_set_led_switch "lan" "LAN" "tp-link:white:lan" "switch0" "0x1c"
	ucidef_set_led_switch "wan_data" "WAN Data" "tp-link:white:internet" "switch0" "0x02" "" "tx rx"
	ucidef_set_led_switch "wan_link" "WAN Link" "tp-link:white:wan" "switch0" "0x02" "" "link"
	;;
tplink,cpe220-v3)
	ucidef_set_led_netdev "lan0" "LAN0" "tp-link:green:lan0" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x10"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "tp-link:green:link1" "wlan0" "1" "100"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "tp-link:green:link2" "wlan0" "30" "100"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "tp-link:green:link3" "wlan0" "60" "100"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "tp-link:green:link4" "wlan0" "80" "100"
	;;
tplink,cpe210-v2|\
tplink,cpe210-v3)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:green:lan" "eth0"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "tp-link:green:link1" "wlan0" "1" "100"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "tp-link:green:link2" "wlan0" "30" "100"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "tp-link:green:link3" "wlan0" "60" "100"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "tp-link:green:link4" "wlan0" "80" "100"
	;;
tplink,re450-v2)
	ucidef_set_led_netdev "lan_data" "LAN Data" "tp-link:green:lan_data" "eth0" "tx rx"
	ucidef_set_led_netdev "lan_link" "LAN Link" "tp-link:green:lan_link" "eth0" "link"
	;;
tplink,tl-mr3020-v1|\
tplink,tl-mr3040-v2)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:green:lan" "eth0"
	;;
tplink,tl-wr740n-v1|\
tplink,tl-wr740n-v3|\
tplink,tl-wr741-v1|\
tplink,tl-wr743nd-v1|\
tplink,tl-wr841-v5|\
tplink,tl-wr941-v4)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth0"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x02"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x04"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x10"
	;;
tplink,tl-wr740n-v4|\
tplink,tl-wr741nd-v4|\
tplink,tl-wr841-v8|\
tplink,tl-wr842n-v2)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x04"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x10"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x02"
	;;
ubnt,bullet-m|\
ubnt,bullet-m-xw|\
ubnt,nanostation-m|\
ubnt,nanostation-m-xw|\
ubnt,rocket-m)
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "ubnt:red:link1" "wlan0" "1" "100"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "ubnt:orange:link2" "wlan0" "26" "100"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "ubnt:green:link3" "wlan0" "51" "100"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "ubnt:green:link4" "wlan0" "76" "100"
	;;
ubnt,nanobeam-ac|\
ubnt,nanostation-ac)
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "ubnt:blue:rssi0" "wlan0" "1" "100"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "ubnt:blue:rssi1" "wlan0" "26" "100"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "ubnt:blue:rssi2" "wlan0" "51" "100"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "ubnt:blue:rssi3" "wlan0" "76" "100"
	;;
wd,mynet-wifi-rangeextender)
	ucidef_set_led_netdev "lan" "LAN" "$boardname:green:lan" "eth0"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "$boardname:rssi-low" "wlan0" "1" "100"
	ucidef_set_led_rssi "rssimedium" "RSSIMED" "$boardname:blue:rssi-med" "wlan0" "33" "100"
	ucidef_set_led_rssi "rssihigh" "RSSIMAX" "$boardname:blue:rssi-max" "wlan0" "66" "100"
	;;
yuncore,a770)
	ucidef_set_led_netdev "wan" "WAN" "$boardname:green:wan" "eth1"
	ucidef_set_led_switch "lan" "LAN" "$boardname:green:lan" "switch0" "0x10"
	;;
zbtlink,zbt-wd323)
	ucidef_set_led_switch "lan1" "LAN1" "zbt-wd323:orange:lan1" "switch0" "0x10"
	ucidef_set_led_switch "lan2" "LAN2" "zbt-wd323:orange:lan2" "switch0" "0x08"
	;;
esac

board_config_flush

exit 0
