//SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include "mt7628an.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "wiznet,wizfi630s", "mediatek,mt7628an-soc";
	model = "WIZnet WizFi630S";

	chosen {
		bootargs = "console=ttyS1,115200";
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x8000000>;
	};

	aliases {
		led-boot = &led_run;
		led-failsafe = &led_run;
		led-running = &led_run;
		led-upgrade = &led_run;
		serial0 = &uart1;
		serial1 = &uartlite;
	};

	leds {
		compatible = "gpio-leds";

		led_run: run {
			label = "wizfi630s:green:run";
			gpios = <&gpio0 4 GPIO_ACTIVE_LOW>;
		};

		ledwps {
			label = "wizfi630s:green:wps";
			gpios = <&gpio1 10 GPIO_ACTIVE_LOW>;
		};

		leduart1 {
			label = "wizfi630s:green:uart1";
			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
		};

		leduart2 {
			label = "wizfi630s:green:uart2";
			gpios = <&gpio0 3 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio1 0 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		scm1 {
			label = "SCM1";
			gpios = <&gpio0 5 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_1>;
		};

		scm2 {
			label = "SCM2";
			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_2>;
		};

	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "gpio";
			ralink,function = "gpio";
		};

		i2s {
			ralink,group = "i2s";
			ralink,function = "gpio";
		};

		wdt {
			ralink,group = "wdt";
			ralink,function = "gpio";
		};


		i2c {
			ralink,group = "i2c";
			ralink,function = "gpio";
		};

		refclk {
			ralink,group = "refclk";
			ralink,function = "gpio";
		};
	};
};

&wmac {
	status = "okay";
};

&spi0 {
	status = "okay";

	pinctrl-names = "default";
	pinctrl-0 = <&spi_pins>, <&spi_cs1_pins>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <40000000>;
		m25p,chunked-io = <31>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x1fb0000>;
			};
		};
	};
};

&i2c {
	status = "okay";
};

&uart1 {
	status = "okay";
};

&pwm {
	status = "okay";
};

&ethernet {
	mtd-mac-address = <&factory 0x28>;
};

&esw {
	mediatek,portmap = <0x3e>;
};

&sdhci {
	status = "okay";
	mediatek,cd-high;
};

&wmac {
	status = "okay";
};
