// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "qca953x.dtsi"

/ {
	compatible = "tplink,archer-d50-v1", "qca,qca9531";
	model = "TP-Link Archer D50 v1";

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	gpio_leds: leds {
		compatible = "gpio-leds";

		led_wlan2g: wlan2g {
			label = "tp-link:white:wlan2g";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		led_wlan5g: wlan5g {
			label = "tp-link:white:wlan5g";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
                };

		qss_led: qss {
			label = "tp-link:white:qss";
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};

		wan {
			label = "tp-link:white:wan";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		lan {
			label = "tp-link:white:lan";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

		usb {
			label = "tp-link:white:usb";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
			trigger-sources = <&hub_port0>;
			linux,default-trigger = "usbport";
		};

		internet {
			label = "tp-link:white:internet";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		system: system{
			label = "tp-link:white:system";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
		};

		rfkill {
			label = "RFKILL button";
			linux,code = <KEY_RFKILL>;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "WPS button";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};
	};
};

&uart {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot:	partition@0 {
				label = "u-boot";
				reg = <0x000000 0x020000>;
				read-only;
			};

			partition@20000 {
				compatible = "tplink,firmware";
				label = "firmware";
				reg = <0x020000 0x7a0000>;
			};

			partition@7c0000 {
				label = "config";
				reg = <0x7c0000 0x010000>;
				read-only;
			};

			romfile: partition@7d0000 {
				label = "romfile";
				reg = <0x7d0000 0x010000>;
				read-only;
			};

			partition@7e0000 {
				label = "rom";
				reg = <0x7e0000 0x010000>;
				read-only;
			};

			art: partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x010000>;
				read-only;
			};
		};
	};
};

&eth1 {
	mtd-mac-address = <&romfile 0xf100>;
};

&eth0 {
	status = "okay";
	phy-handle = <&swphy4>;

	mtd-mac-address = <&romfile 0xf100>;
	mtd-mac-address-increment = <1>;
};

&wmac {
	status = "okay";
	mtd-cal-data = <&art 0x1000>;
	mtd-mac-address = <&romfile 0xf100>;
};

&pcie0 {
	status = "okay";

	wifi@0,0 {
		compatible = "pci168c,003c";
		reg = <0x0000 0 0 0 0>;
	};
};

&usb_phy {
	status = "okay";
};

&usb0 {
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	hub_port0: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};
