#!/bin/sh
#
# Copyright (C) 2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)
boardname="${board##*,}"

case "$board" in
alfa-network,ap120c-ac)
	ucidef_set_led_netdev "wan" "WAN" "${boardname}:amber:wan" "eth1"
	;;
asus,rt-ac58u)
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "${boardname}:blue:wlan2G" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "${boardname}:blue:wlan5G" "phy1tpt"
	ucidef_set_led_netdev "wan" "WAN" "${boardname}:blue:wan" "eth1"
	ucidef_set_led_switch "lan" "LAN" "${boardname}:blue:lan" "switch0" "0x1e"
	;;
avm,fritzbox-4040)
	ucidef_set_led_wlan "wlan" "WLAN" "fritz4040:green:wlan" "phy0tpt" "phy1tpt"
	ucidef_set_led_netdev "wan" "WAN" "fritz4040:green:wan" "eth1"
	ucidef_set_led_switch "lan" "LAN" "fritz4040:green:lan" "switch0" "0x1e"
	;;
avm,fritzbox-7530 |\
glinet,gl-b1300)
	ucidef_set_led_wlan "wlan" "WLAN" "${boardname}:green:wlan" "phy0tpt"
	;;
engenius,eap1300)
	ucidef_set_led_netdev "lan" "LAN" "${boardname}:blue:lan" "eth0"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "${boardname}:blue:wlan2g" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "${boardname}:yellow:wlan5g" "phy1tpt"
	ucidef_set_led_default "mesh" "MESH" "${boardname}:blue:mesh" "0"
	;;
engenius,ens620ext)
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "${boardname}:green:wlan2G" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "${boardname}:green:wlan5G" "phy1tpt"
	ucidef_set_led_netdev "lan1" "LAN1" "${boardname}:green:lan1" "eth0"
	ucidef_set_led_netdev "lan2" "LAN2" "${boardname}:green:lan2" "eth1"
	;;
netgear,ex6100v2 |\
netgear,ex6150v2)
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "ex61x0v2:green:router" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "ex61x0v2:green:client" "phy1tpt"
	;;
qxwlan,e2600ac-c1 |\
qxwlan,e2600ac-c2)
	ucidef_set_led_wlan "wlan2g" "WLAN0" "e2600ac:green:wlan0" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN1" "e2600ac:green:wlan1" "phy1tpt"
	;;
zyxel,nbg6617)
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "${boardname}:green:wlan2G" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "${boardname}:green:wlan5G" "phy1tpt"
	;;
zyxel,wre6606)
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "${boardname}:green:wlan2g" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "${boardname}:green:wlan5g" "phy1tpt"
	;;
*)
	;;
esac

board_config_flush

exit 0
