/dts-v1/;

#include "rt3883.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "samsung,cy-swr1100", "ralink,rt3883-soc";
	model = "Samsung CY-SWR1100";

	aliases {
		led-boot = &led_wps;
		led-failsafe = &led_wps;
	};

	nor-flash@1c000000 {
		compatible = "cfi-flash";
		reg = <0x1c000000 0x800000>;
		bank-width = <2>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "uboot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "uboot-env";
				reg = <0x30000 0x4000>;
				read-only;
			};

			factory: partition@34000 {
				label = "factory";
				reg = <0x34000 0x4000>;
				read-only;
			};

			partition@38000 {
				label = "nvram";
				reg = <0x38000 0x8000>;
				read-only;
			};

			partition@40000 {
				label = "devdata";
				reg = <0x40000 0x10000>;
			};

			partition@50000 {
				compatible = "seama";
				label = "firmware";
				reg = <0x50000 0x7b0000>;
			};
		};
	};

	rtl8367 {
		compatible = "realtek,rtl8367";
		gpio-sda = <&gpio0 1 GPIO_ACTIVE_HIGH>;
		gpio-sck = <&gpio0 2 GPIO_ACTIVE_HIGH>;
		realtek,extif0 = <1 0 1 1 1 1 1 1 2>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio0 6 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio0 3 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_wps: wps {
			label = "cy-swr1100:blue:wps";
			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
		};

		usb {
			label = "cy-swr1100:blue:usb";
			gpios = <&gpio1 1 GPIO_ACTIVE_LOW>;
			trigger-sources = <&ohci_port1>, <&ehci_port1>;
			linux,default-trigger = "usbport";
		};
	};
};

&gpio1 {
	status = "okay";
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "i2c", "spi";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	port@0 {
		mediatek,fixed-link = <1000 1 1 1>;
		phy-mode = "rgmii";
	};
};

&pci {
	status = "okay";
};

&pci1 {
	status = "okay";

	wifi@0,0 {
		compatible = "pci0,0";
		reg = <0x10000 0 0 0 0>;
		ralink,5ghz = <0>;
		ralink,mtd-eeprom = <&factory 0x2000>;
	};
};

&wmac {
	status = "okay";
	ralink,2ghz = <0>;
	ralink,mtd-eeprom = <&factory 0>;
};

&ehci {
	status = "okay";
};

&ohci {
	status = "okay";
};
