/dts-v1/;

#include "bcm6368.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "ADB P.DG AV4202N";
	compatible = "adb,av4202n", "brcm,bcm6368";

	chosen {
		bootargs = "rootfstype=squashfs,jffs2 noinitrd console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	keys {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&pinctrl 34 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};

		wlan {
			label = "wlan";
			gpios = <&pinctrl 37 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WLAN>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		power_white {
			label = "AV4202N:white:power";
			gpios = <&pinctrl 10 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};
		power_red {
			label = "AV4202N:red:power";
			gpios = <&pinctrl 11 GPIO_ACTIVE_LOW>;
		};
		wan_white {
			label = "AV4202N:white:wan";
			gpios = <&pinctrl 26 GPIO_ACTIVE_LOW>;
		};
		wan_red {
			label = "AV4202N:red:wan";
			gpios = <&pinctrl 27 GPIO_ACTIVE_LOW>;
		};
		phone_white {
			label = "AV4202N:white:phone";
			gpios = <&pinctrl 24 GPIO_ACTIVE_LOW>;
		};
		phone_red {
			label = "AV4202N:red:phone";
			gpios = <&pinctrl 25 GPIO_ACTIVE_LOW>;
		};
		wifi {
			label = "AV4202N:blue:wifi";
			gpios = <&pinctrl 22 GPIO_ACTIVE_LOW>;
		};
	};
};

&pflash {
	status = "ok";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		cfe@0 {
			label = "CFE";
			reg = <0x000000 0x020000>;
			read-only;
		};

		linux@20000 {
			label = "linux";
			reg = <0x020000 0xfc0000>;
			compatible = "brcm,bcm963xx-imagetag";
		};

		nvram@fe0000 {
			label = "nvram";
			reg = <0xfe0000 0x020000>;
		};
	};
};

&uart0 {
	status = "ok";
};
