/*
 *  BSD LICENSE
 *
 *  Copyright(c) 2017 Kristian Evensen <kristian.evensen@gmail.com>.
 *  All rights reserved.
 *
 *  Redistribution and use in source and binary forms, with or without
 *  modification, are permitted provided that the following conditions
 *  are met:
 *
 *    * Redistributions of source code must retain the above copyright
 *      notice, this list of conditions and the following disclaimer.
 *    * Redistributions in binary form must reproduce the above copyright
 *      notice, this list of conditions and the following disclaimer in
 *      the documentation and/or other materials provided with the
 *      distribution.
 *    * Neither the name of Broadcom Corporation nor the names of its
 *      contributors may be used to endorse or promote products derived
 *      from this software without specific prior written permission.
 *
 *  THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
 *  "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
 *  LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
 *  A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
 *  OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
 *  SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
 *  LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
 *  DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
 *  THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
 *  (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
 *  OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
 */

/dts-v1/;

#include "mt7620a.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "sanlinking,d240", "ralink,mt7620a-soc";
	model = "Sanlinking Technologies D240";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	gpio-export {
		compatible = "gpio-export";
		#size-cells = <0>;

		power_mpcie2 {
			gpio-export,name = "power_mpcie2";
			gpio-export,output = <1>;
			gpios = <&gpio2 5 GPIO_ACTIVE_HIGH>;
		};

		power_mpcie1 {
			gpio-export,name = "power_mpcie1";
			gpio-export,output = <1>;
			gpios = <&gpio2 6 GPIO_ACTIVE_HIGH>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "d240:blue:power";
			gpios = <&gpio1 14 GPIO_ACTIVE_HIGH>;
		};

		usb {
			label = "d240:blue:usb";
			gpios = <&gpio1 15 GPIO_ACTIVE_HIGH>;
			trigger-sources = <&ohci_port1>, <&ehci_port1>;
			linux,default-trigger = "usbport";
		};

		air {
			label = "d240:blue:wifi";
			gpios = <&gpio3 0 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio0 1 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&gpio1 {
	status = "okay";
};

&gpio2 {
	status = "okay";
};

&gpio3 {
	status = "okay";
};

&spi0 {
	status = "okay";

	en25q128@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0xfb0000>;
			};
		};
	};
};

&sdhci {
	status = "okay";
	/* the pins function is already set during pinmux driver load */
	/delete-property/ pinctrl-0;
};

&ehci {
	status = "okay";
};

&ohci {
	status = "okay";
};

&ethernet {
	mtd-mac-address = <&factory 0x4>;
	mediatek,portmap = "wllll";
};

&wmac {
	ralink,mtd-eeprom = <&factory 0>;
};

&pinctrl {
	state_default: pinctrl0 {
		default {
			ralink,group = "i2c", "uartf", "wled", "spi refclk", "pa";
			ralink,function = "gpio";
		};

		/*
		 * The sd function of the nd_sd group configures two of the
		 * groups pins as gpios. The pins are used as PCIe reset/power.
		 * Due to the driver load order, the pins are configured way to
		 * late if triggered by the sd-card driver.
		 * To not introduce another kind of driver load order
		 * dependency and configure the pins as early as possible,
		 * means during pinmux driver load.
		 */
		gpio_sd {
			ralink,group = "nd_sd";
			ralink,function = "sd";
		};
	};
};

&pcie {
	status = "okay";
};
