#include "rt5350.dtsi"

#include <dt-bindings/gpio/gpio.h>

/ {
	compatible = "vocore,vocore", "ralink,rt5350-soc";

	aliases {
		led-boot = &led_status;
		led-failsafe = &led_status;
		led-running = &led_status;
		led-upgrade = &led_status;
	};

	gpio-export {
		compatible = "gpio-export";
		#size-cells = <0>;

		gpio0 {
			gpio-export,name = "gpio0";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio0 0 GPIO_ACTIVE_HIGH>;
		};

		/* UARTF */
		gpio7 {
			/* UARTF_RTS_N */
			gpio-export,name = "gpio7";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio0 7 GPIO_ACTIVE_HIGH>;
		};

		gpio8 {
			/* UARTF_TXD */
			gpio-export,name = "gpio8";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio0 8 GPIO_ACTIVE_HIGH>;
		};

		gpio9 {
			/* UARTF_CTS_N */
			gpio-export,name = "gpio9";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio0 9 GPIO_ACTIVE_HIGH>;
		};

		gpio12 {
			/* UARTF_DCD_N */
			gpio-export,name = "gpio12";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio0 12 GPIO_ACTIVE_HIGH>;
		};

		gpio13 {
			/* UARTF_DSR_N */
			gpio-export,name = "gpio13";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio0 13 GPIO_ACTIVE_HIGH>;
		};

		gpio14 {
			/* UARTF_RIN */
			gpio-export,name = "gpio14";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio0 14 GPIO_ACTIVE_HIGH>;
		};

		/* JTAG */
		gpio17 {
			/* JTAG_TDO */
			gpio-export,name = "gpio17";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio0 17 GPIO_ACTIVE_HIGH>;
		};

		gpio18 {
			/* JTAG_TDI */
			gpio-export,name = "gpio18";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio0 18 GPIO_ACTIVE_HIGH>;
		};

		gpio19 {
			/* JTAG_TMS */
			gpio-export,name = "gpio19";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio0 19 GPIO_ACTIVE_HIGH>;
		};

		gpio20 {
			/* JTAG_TCLK */
			gpio-export,name = "gpio20";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio0 20 GPIO_ACTIVE_HIGH>;
		};

		gpio21 {
			/* JTAG_TRST_N */
			gpio-export,name = "gpio21";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio0 21 GPIO_ACTIVE_HIGH>;
		};

		/* ETH LEDs */
		gpio22 {
			/* ETH0_LED */
			gpio-export,name = "gpio22";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio1 0 GPIO_ACTIVE_HIGH>;
		};

		gpio23 {
			/* ETH1_LED */
			gpio-export,name = "gpio23";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio1 1 GPIO_ACTIVE_HIGH>;
		};

		gpio24 {
			/* ETH2_LED */
			gpio-export,name = "gpio24";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio1 2 GPIO_ACTIVE_HIGH>;
		};

		gpio25 {
			/* ETH3_LED */
			gpio-export,name = "gpio25";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio1 3 GPIO_ACTIVE_HIGH>;
		};

		gpio26 {
			/* ETH4_LED */
			gpio-export,name = "gpio26";
			gpio-export,direction_may_change = <1>;
			gpios = <&gpio1 4 GPIO_ACTIVE_HIGH>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_status: status {
			/* UARTF_RXD */
			label = "vocore:green:status";
			gpios = <&gpio0 10 GPIO_ACTIVE_HIGH>;
		};

		eth {
			/* UARTF_DTR_N */
			label = "vocore:orange:eth";
			gpios = <&gpio0 11 GPIO_ACTIVE_HIGH>;
		};
	};
};

&gpio1 {
	status = "okay";
};

&i2c {
	status = "okay";
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "jtag", "uartf", "led";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x4>;
};

&esw {
	mediatek,portmap = <0x11>;
	mediatek,portdisable = <0x2e>;
};

&wmac {
	ralink,mtd-eeprom = <&factory 0>;
};

&ehci {
	status = "okay";
};

&ohci {
	status = "okay";
};

&spi1 {
	status = "okay";

	spidev@0 {
		compatible = "linux,spidev";
		spi-max-frequency = <10000000>;
		reg = <0>;
	};
};
