// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "ar9344.dtsi"

/ {
	model = "Western Digital My Net N750";
	compatible = "wd,mynet-n750", "qca,ar9344";

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	aliases {
		led-boot = &power;
		led-failsafe = &power;
		led-running = &power;
		led-upgrade = &power;
	};

	leds {
		compatible = "gpio-leds";

		wifi {
			label = "mynet-n750:blue:wireless";
			gpios = <&gpio 11 GPIO_ACTIVE_HIGH>;
		};

		internet {
			label = "mynet-n750:blue:internet";
			gpios = <&gpio 12 GPIO_ACTIVE_HIGH>;
		};

		wps {
			label = "mynet-n750:blue:wps";
			gpios = <&gpio 13 GPIO_ACTIVE_HIGH>;
		};

		power: power {
			label = "mynet-n750:blue:power";
			gpios = <&gpio 14 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};

		wps {
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
		};
	};
};

&ref {
	clock-frequency = <40000000>;
};

&uart {
	status = "okay";
};

&gpio {
	status = "okay";

	gpio_ext_lna0 {
		gpio-hog;
		gpios = <15 0>;
		output-high;
		line-name = "mynet-n750:ext:lna0";
	};

	gpio_ext_lna1 {
		gpio-hog;
		gpios = <18 0>;
		output-high;
		line-name = "mynet-n750:ext:lna1";
	};
};

&spi {
	num-cs = <1>;

	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "bootloader";
				reg = <0x000000 0x40000>;
				read-only;
			};

			partition@40000 {
				label = "bdcfg";
				reg = <0x040000 0x10000>;
				read-only;
			};

			partition@50000 {
				label = "devdata";
				reg = <0x050000 0x10000>;
				read-only;
			};

			partition@60000 {
				label = "devconf";
				reg = <0x060000 0x10000>;
				read-only;
			};

			partition@70000 {
				compatible = "seama";
				label = "firmware";
				reg = <0x070000 0xf80000>;
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&usb {
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	port@1 {
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <1>;
		#trigger-source-cells = <0>;

		hub_port1: port@1 {
			reg = <1>;
			#trigger-source-cells = <0>;
		};

		hub_port2: port@2 {
			reg = <2>;
			#trigger-source-cells = <0>;
		};
	};
};

&usb_phy {
	status = "okay";
};

&pcie {
	status = "okay";

	wifi@0,0 {
		compatible = "pci168c,0033";
		reg = <0x0000 0 0 0 0>;
		qca,no-eeprom;
	};
};

&wmac {
	status = "okay";
	qca,no-eeprom;
};

&mdio0 {
	status = "okay";
	phy-mask = <0>;

	switch0@1f {
		compatible = "qca,ar8327";
		reg = <0x1f>;

		qca,ar8327-initvals = <
			0x04 0x07600000 /* PORT0 PAD MODE CTRL */
			0x10 0x80000080 /* POWER_ON_STRIP */
			0x50 0xc737c737 /* LED_CTRL0 */
			0x54 0x00000000 /* LED_CTRL1 */
			0x58 0x00000000 /* LED_CTRL2 */
			0x5c 0x0030c300 /* LED_CTRL3 */
			0x7c 0x0000007e /* PORT0_STATUS */
			>;
	};
};

&eth0 {
	status = "okay";

	/* default for ar934x, except for 1000M */
	pll-data = <0x06000000 0x00000101 0x00001616>;

	phy-mode = "rgmii";
	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};
