// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "qca956x.dtsi"

/ {
	compatible = "tplink,archer-c25-v1", "qca,qca9561";
	model = "TP-Link Archer C25 v1";

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	led_spi {
		compatible = "spi-gpio";
		#address-cells = <1>;
		#size-cells = <0>;

		sck-gpios = <&gpio 15 GPIO_ACTIVE_HIGH>;
		mosi-gpios = <&gpio 14 GPIO_ACTIVE_HIGH>;
		cs-gpios = <&gpio 16 GPIO_ACTIVE_HIGH>;
		num-chipselects = <1>;

		/* can be removed on 4.19 */
		gpio-sck = <&gpio 15 GPIO_ACTIVE_HIGH>;
		gpio-mosi = <&gpio 14 GPIO_ACTIVE_HIGH>;

		led_gpio: led_gpio@0 {
			compatible = "fairchild,74hc595";
			reg = <0>;
			gpio-controller;
			#gpio-cells = <2>;
			registers-number = <1>;
			spi-max-frequency = <10000000>;
		};
	};

	keys {
		compatible = "gpio-keys";

		wifi_button {
			label = "WiFi button";
			linux,code = <KEY_RFKILL>;
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};

		reset_button {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};
	};

	aliases {
		led-boot = &power;
		led-failsafe = &power;
		led-running = &power;
		led-upgrade = &power;
	};

	leds {
		compatible = "gpio-leds";

		power: power {
			label = "tp-link:green:power";
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wps {
			label = "tp-link:green:wps";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};

		wlan2g {
			label = "tp-link:green:wlan2g";
			gpios = <&led_gpio 6 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		wlan5g {
			label = "tp-link:green:wlan5g";
			gpios = <&led_gpio 7 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wan_green {
			label = "tp-link:green:wan";
			gpios = <&led_gpio 5 GPIO_ACTIVE_LOW>;
		};

		wan_amber {
			label = "tp-link:amber:wan";
			gpios = <&led_gpio 4 GPIO_ACTIVE_LOW>;
		};

		lan1 {
			label = "tp-link:green:lan1";
			gpios = <&led_gpio 0 GPIO_ACTIVE_LOW>;
		};

		lan2 {
			label = "tp-link:green:lan2";
			gpios = <&led_gpio 1 GPIO_ACTIVE_LOW>;
		};

		lan3 {
			label = "tp-link:green:lan3";
			gpios = <&led_gpio 2 GPIO_ACTIVE_LOW>;
		};

		lan4 {
			label = "tp-link:green:lan4";
			gpios = <&led_gpio 3 GPIO_ACTIVE_LOW>;
		};
	};
};

&spi {
	status = "okay";
	num-cs = <1>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "factory-boot";
				reg = <0x000000 0x020000>;
				read-only;
			};

			partition@20000 {
				label = "u-boot";
				reg = <0x020000 0x010000>;
				read-only;
			};

			partition@30000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x030000 0x7a0000>;
			};

			config: partition@7d0000 {
				label = "config";
				reg = <0x7d0000 0x010000>;
				read-only;
			};

			info: partition@7e0000 {
				label = "info";
				reg = <0x7e0000 0x010000>;
				read-only;
			};

			art: partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x010000>;
				read-only;
			};
		};
	};
};

&uart {
	status = "okay";
};

&pcie {
	status = "okay";
};

&eth0 {
	phy-mode = "mii";
	phy-handle = <&swphy4>;

	status = "okay";
	mtd-mac-address = <&info 0x8>;
};

&eth1 {
	status = "okay";
	mtd-mac-address = <&info 0x8>;
	mtd-mac-address-increment = <1>;
};

&wmac {
	status = "okay";
	mtd-cal-data = <&art 0x1000>;
	mtd-mac-address = <&info 0x8>;
};
