// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "qca9557.dtsi"

/ {
	model = "EnGenius EPG5000";
	compatible = "engenius,epg5000", "qca,qca9557";

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	aliases {
		led-boot = &power;
		led-failsafe = &power;
		led-running = &power;
		led-upgrade = &power;
	};

	leds {
		compatible = "gpio-leds";

		power: power {
			label = "epg5000:amber:power";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wlan2g {
			label = "epg5000:blue:wlan2g";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		wlan5g {
			label = "epg5000:blue:wlan5g";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wps_amber {
			label = "epg5000:amber:wps";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};

		wps_blue {
			label = "epg5000:blue:wps";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};
};

&eth0 {
	status = "okay";

	phy-handle = <&phy0>;
	pll-data = <0xa6000000 0x00000101 0x00001616>;
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;

		qca,ar8327-initvals = <
			0x04 0x87600000 /* PORT0 PAD MODE CTRL */
			0x7c 0x0000007e /* PORT0_STATUS */
			>;
	};
};

&pcie0 {
	status = "okay";

	wifi@0,0 {
		compatible = "pci168c,003c";
		reg = <0x0000 0 0 0 0>;
	};
};

&spi {
	status = "okay";

	num-cs = <1>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x030000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x030000 0x010000>;
			};

			partition@40000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x040000 0xe50000>;
			};

			partition@790000 {
				label = "manufacture";
				reg = <0xe90000 0x100000>;
				read-only;
			};

			partition@ed0000 {
				label = "backup";
				reg = <0xf90000 0x010000>;
				read-only;
			};

			partition@fe0000 {
				label = "storage";
				reg = <0xfa0000 0x050000>;
				read-only;
			};

			partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&uart {
	status = "okay";
};

&usb_phy1 {
	status = "okay";
};

&usb1 {
	status = "okay";
};

&wmac {
	status = "okay";

	qca,no-eeprom;
};
