/dts-v1/;

#include "HC5X61.dtsi"

/ {
	compatible = "hiwifi,hc5661", "hiwifi,hc5x61", "ralink,mt7620a-soc";
	model = "HiWiFi HC5661";

	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
	};

	leds {
		compatible = "gpio-leds";

		led_system: system {
			label = "hc5661:blue:system";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
		};

		internet {
			label = "hc5661:blue:internet";
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
		};

		wlan2g {
			label = "hc5661:blue:wlan2g";
			gpios = <&gpio3 0 GPIO_ACTIVE_LOW>;
		};

		wlan5g {
			label = "hc5661:blue:wlan5g";
			gpios = <&gpio0 7 GPIO_ACTIVE_LOW>;
		};
	};
};
