#!/bin/sh

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
dlink,dir-510l)
	ucidef_add_gpio_switch "usb_enable1" "USB 1A enable" "12" "0"
	ucidef_add_gpio_switch "usb_enable05" "USB 0.5A enable" "13" "1"
	;;
head-weblink,hdrm200)
	ucidef_add_gpio_switch "sim_switch" "SIM slot switch" "0"
	ucidef_add_gpio_switch "io1" "I/O 1" "1"
	ucidef_add_gpio_switch "io2" "I/O 2" "2"
	ucidef_add_gpio_switch "io3" "I/O 3" "11"
	ucidef_add_gpio_switch "io4" "I/O 4" "14"
	ucidef_add_gpio_switch "power_mpcie" "mPCIe power" "21" "1"
	;;
mikrotik,rb750gr3)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "17"
	;;
telco-electronics,x1)
	ucidef_add_gpio_switch "modem_reset" "Modem Reset" "16"
	;;
ubnt-erx)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "0"
	;;
ubnt-erx-sfp)
	ucidef_add_gpio_switch "poe_power_port0" "PoE Power Port0" "496"
	ucidef_add_gpio_switch "poe_power_port1" "PoE Power Port1" "497"
	ucidef_add_gpio_switch "poe_power_port2" "PoE Power Port2" "498"
	ucidef_add_gpio_switch "poe_power_port3" "PoE Power Port3" "499"
	ucidef_add_gpio_switch "poe_power_port4" "PoE Power Port4" "500"
	;;
zbtlink,zbt-we826-e)
	ucidef_add_gpio_switch "sim_switch" "SIM slot switch" "13"
	ucidef_add_gpio_switch "power_mpcie" "mPCIe power" "14" "1"
	;;
esac

board_config_flush

exit 0
