/dts-v1/;

#include "rt5350.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "tenda,3g150b", "ralink,rt5350-soc";
	model = "Tenda 3G150B";

	aliases {
		led-boot = &led_ap;
		led-failsafe = &led_ap;
		led-running = &led_ap;
		led-upgrade = &led_ap;
	};

	leds {
		compatible = "gpio-leds";

		led_ap: ap {
			label = "3g150b:blue:ap";
			gpios = <&gpio0 7 GPIO_ACTIVE_LOW>;
		};

		3g {
			label = "3g150b:blue:3g";
			gpios = <&gpio0 14 GPIO_ACTIVE_LOW>;
			trigger-sources = <&ohci_port1>, <&ehci_port1>;
			linux,default-trigger = "usbport";
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	gpio_export {
		compatible = "gpio-export";
		#size-cells = <0>;

		usb {
			gpio-export,name = "usb";
			gpio-export,output = <1>;
			gpios = <&gpio0 13 GPIO_ACTIVE_HIGH>;
		};
	};
};

&spi0 {
	status = "okay";

	m25p80@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x3b0000>;
			};
		};
	};
};

&gpio1 {
	status = "okay";
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "i2c", "jtag", "uartf", "led";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x4>;
};

&esw {
	mediatek,portmap = <0x2f>;
};

&wmac {
	ralink,mtd-eeprom = <&factory 0>;
	ralink,led-polarity = <1>;
};

&ehci {
	status = "okay";
};

&ohci {
	status = "okay";
};
