#!/bin/sh

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
meraki,mr24)
	ucidef_set_led_netdev "wan" "WAN" "mr24:green:wan" "eth0"
	ucidef_set_led_wlan "wlan1" "WLAN1" "mr24:green:wifi1" "phy0assoc"
	ucidef_set_led_wlan "wlan2" "WLAN2" "mr24:green:wifi2" "phy0assoc"
	ucidef_set_led_wlan "wlan3" "WLAN3" "mr24:green:wifi3" "phy0assoc"
	ucidef_set_led_wlan "wlan4" "WLAN4" "mr24:green:wifi4" "phy0tpt"
	;;

meraki,mx60)
	ucidef_set_led_switch "wan" "WAN" "mx60:green:wan" "switch0" "0x20"
	ucidef_set_led_switch "lan1" "LAN1" "mx60:green:lan1" "switch0" "0x10"
	ucidef_set_led_switch "lan2" "LAN2" "mx60:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "mx60:green:lan3" "switch0" "0x04"
	ucidef_set_led_switch "lan4" "LAN4" "mx60:green:lan4" "switch0" "0x02"
	;;

netgear,wndap620)
	ucidef_set_led_switch "lan_act" "LAN (Activity)" "wndap6x0:green:activity" "switch0" "0x04" "0x0f" "rx tx"
	ucidef_set_led_switch "lan_100" "LAN 100Mbps" "wndap620:amber:link100" "switch0" "0x04" "0x04" "link"
	ucidef_set_led_switch "lan_1000" "LAN 1000Mbps" "wndap620:green:link1000" "switch0" "0x04" "0x08" "link"
	;;

netgear,wndap660)
	ucidef_set_led_netdev "lan_act" "LAN (Activity)" "wndap6x0:green:activity" "eth0"
	ucidef_set_led_switch "lan1_100" "LAN 100Mbps" "wndap660:amber:lan1-link100" "switch0" "0x04" "0x04" "link"
	ucidef_set_led_switch "lan1_1000" "LAN 1000Mbps" "wndap660:green:lan1-link1000" "switch0" "0x04" "0x08" "link"
	ucidef_set_led_switch "lan2_100" "LAN 100Mbps" "wndap660:amber:lan2-link100" "switch0" "0x02" "0x04" "link"
	ucidef_set_led_switch "lan2_1000" "LAN 1000Mbps" "wndap660:green:lan2-link1000" "switch0" "0x02" "0x08" "link"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "wndap6x0:green:wlan2g" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "wndap6x0:green:wlan5g" "phy1tpt"
	;;

netgear,wndr4700)
	ucidef_set_led_switch "wan_green" "WAN (green)" "wndr4700:green:wan" "switch0" "0x20"
	ucidef_set_led_netdev "wan_yellow" "WAN (yellow)" "wndr4700:yellow:wan" "eth0.2" "tx rx"
	ucidef_set_led_usbport "usb3" "USB3" "wndr4700:blue:usb" "usb2-port1" "usb2-port2" "usb3-port1" "usb3-port2"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "wndr4700:blue:wlan" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "wndr4700:blue:wlan" "phy1tpt"
	;;

*)
	;;
esac

board_config_flush

exit 0
