#include "mt7628an.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "widora,neo", "mediatek,mt7628an-soc";

	aliases {
		led-boot = &led_wifi;
		led-failsafe = &led_wifi;
		led-running = &led_wifi;
		led-upgrade = &led_wifi;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x8000000>;
	};

	leds {
		compatible = "gpio-leds";

		led_wifi: wifi {
			label = "widora:orange:wifi";
			gpios = <&wgpio 0 GPIO_ACTIVE_HIGH>;
			default-state = "on";
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		wps {
			label = "reset";
			gpios = <&gpio1 6 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	wgpio: gpio-wifi {
		compatible = "mediatek,gpio-wifi";
		#address-cells = <1>;
		#size-cells = <0>;
		gpio-controller;
		#gpio-cells = <2>;
	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "gpio";
			ralink,function = "gpio";
		};

		perst {
			ralink,group = "perst";
			ralink,function = "gpio";
		};

		refclk {
			ralink,group = "refclk";
			ralink,function = "gpio";
		};

		i2s {
			ralink,group = "i2s";
			ralink,function = "gpio";
		};

		spis {
			ralink,group = "spis";
			ralink,function = "gpio";
		};

		wled_kn {
			ralink,group = "wled_kn";
			ralink,function = "gpio";
		};

		wled_an {
			ralink,group = "wled_an";
			ralink,function = "wled_an";
		};

		wdt {
			ralink,group = "wdt";
			ralink,function = "gpio";
		};
	};
};

&i2c {
	status = "okay";
};

&uart1 {
	status = "okay";
};

&uart2 {
	status = "okay";
};

&pwm {
	status = "okay";
};

&ethernet {
	mtd-mac-address = <&factory 0x28>;
};

&sdhci {
	status = "okay";
	mediatek,cd-low;
};

&wmac {
	status = "okay";
};
