/*
 * Device tree source for D-Link DSR-500N.
 *
 * Written by: Aaro Koskinen <aaro.koskinen@iki.fi>
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */

/include/ "dlink_dsr-500n-1000n.dtsi"
#include <dt-bindings/gpio/gpio.h>

/ {
	model = "dlink,dsr-500n";
	compatible = "dlink,dsr-500n", "cavium,octeon-3860";

	soc@0 {
		uart0: serial@1180000000800 {
			clock-frequency = <300000000>;
		};
	};

	leds {
		compatible = "gpio-leds";

		usb {
			gpios = <&gpio 9 GPIO_ACTIVE_LOW>;
		};

		wps {
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};

		wireless {
			label = "2.4g";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
		};
	};
};
